

**ECSS Secretariat**

**ESA-ESTEC**

**Standards Section**

**Noordwijk, The Netherlands**

**Foreword**

ECSS is a cooperative effort of the European Space Agency, national space agencies and European industry associations for the purpose of developing and maintaining common standards. Requirements in this Standard are defined in terms of what shall be accomplished, rather than in terms of how to organize and perform the necessary work. This allows existing organizational structures and methods to be applied where they are effective, and for the structures and methods to evolve as necessary without rewriting the standards.

This Standard has been prepared by the Working Group, reviewed by the ECSS Executive Secretariat and approved by the ECSS Technical Authority.

**Disclaimer**

ECSS does not provide any warranty whatsoever, whether expressed, implied, or statutory, including, but not limited to, any warranty of merchantability or fitness for a particular purpose or any warranty that the contents of the item are error-free. In no respect shall ECSS incur any liability for any damages, including, but not limited to, direct, indirect, special, or consequential damages arising out of, resulting from, or in any way connected to the use of this Standard, whether or not based upon warranty, business agreement, tort, or otherwise; whether or not injury was sustained by persons or property or otherwise; and whether or not loss was sustained from, or arose out of, the results of, the item, or any services that may be provided by ECSS.

Published by: ESA Standards Section

ESTEC, P.O. Box 299,

2200 AG Noordwijk

The Netherlands

Copyright: 2025© by the European Space Agency for the members of ECSS

Change log

|  |  |
| --- | --- |
| ECSS-E-ST-40-07C  2 March 2020 | First issue |
|  | First issue, Revision 1  Main changes related to the implementation of change requests:   * Massive clarifications, improvements, rework and completion for the behaviour description of the software interfaces. * Massive editorial corrections. * Few new software interfaces added: IPublishField, IStringType. * Section to explain types and eager resolution added. * SMP version check added. * C++ and XML artefacts (a.k.a. SMP\_FILES) updated accordingly. * Title updated to include “Level 1”   *NOTE: Due to the amount of changes it was decided to create a new DOORS module that is not linked to the previous version.* |

Table of contents

[Change log 3](#_Toc205281416)

[Introduction 9](#_Toc205281417)

[1 Scope 10](#_Toc205281418)

[2 Normative references 11](#_Toc205281419)

[3 Terms, definitions and abbreviated terms 12](#_Toc205281420)

[3.1 Terms from other standards 12](#_Toc205281421)

[3.2 Terms specific to the present standard 12](#_Toc205281422)

[3.3 Abbreviated terms 17](#_Toc205281423)

[3.4 Nomenclature 17](#_Toc205281424)

[4 Principles 18](#_Toc205281425)

[4.1 Objectives 18](#_Toc205281426)

[4.2 Common Concepts and common types 18](#_Toc205281427)

[4.3 Architecture 19](#_Toc205281428)

[4.4 Time handling principle 20](#_Toc205281429)

[4.5 Simulation lifecycle 21](#_Toc205281430)

[4.6 Simulation method 22](#_Toc205281431)

[4.6.1 Discrete-event simulation (DES) 22](#_Toc205281432)

[4.6.2 Parallelization and distribution 23](#_Toc205281433)

[4.6.3 Inter component communication 23](#_Toc205281434)

[4.7 Models, Services and Components 24](#_Toc205281435)

[4.7.1 Objects 24](#_Toc205281436)

[4.7.2 Components 26](#_Toc205281437)

[4.7.3 Factories 28](#_Toc205281438)

[4.7.4 Models and Services 28](#_Toc205281439)

[4.8 Publication, Types and Persistence 29](#_Toc205281440)

[4.9 Dynamic invocation 31](#_Toc205281441)

[4.10 Components meta data 35](#_Toc205281442)

[4.10.1 Catalogue 35](#_Toc205281443)

[4.10.2 Package 35](#_Toc205281444)

[4.10.3 Configuration 35](#_Toc205281445)

[4.11 Model exchanges considerations 36](#_Toc205281446)

[4.11.1 Overview 36](#_Toc205281447)

[4.11.2 SMP Bundle 36](#_Toc205281448)

[5 Interface requirements 37](#_Toc205281449)

[5.1 Common 37](#_Toc205281450)

[5.1.1 Primitive Types specification 37](#_Toc205281451)

[5.1.2 Time Kinds 39](#_Toc205281452)

[5.1.3 Path string 40](#_Toc205281453)

[5.1.4 Universally Unique Identifiers (UUID) 41](#_Toc205281454)

[5.1.5 Exception specification 42](#_Toc205281455)

[5.2 Components and Objects interfaces 42](#_Toc205281456)

[5.2.1 Object Specification (IObject) 42](#_Toc205281457)

[5.2.2 Collection Specification (ICollection) 43](#_Toc205281458)

[5.2.3 Component Specification 44](#_Toc205281459)

[5.2.4 Aggregation 51](#_Toc205281460)

[5.2.5 Composition 54](#_Toc205281461)

[5.2.6 Events 57](#_Toc205281462)

[5.2.7 Entry points 60](#_Toc205281463)

[5.2.8 Dynamic Invocation 61](#_Toc205281464)

[5.2.9 Persistence (IPersist) 66](#_Toc205281465)

[5.2.10 Failures 67](#_Toc205281466)

[5.2.11 Fields 69](#_Toc205281467)

[5.2.12 Requirements on utilization of Simulation Environments interfaces by components 77](#_Toc205281468)

[5.2.13 Properties 78](#_Toc205281469)

[5.2.14 Operations 80](#_Toc205281470)

[5.3 Simulation Environment interfaces 82](#_Toc205281471)

[5.3.1 Logger (ILogger interface) 82](#_Toc205281472)

[5.3.2 Time Keeper (ITimeKeeper) 84](#_Toc205281473)

[5.3.3 Scheduler (IScheduler) 86](#_Toc205281474)

[5.3.4 Event Manager (IEventManager) 98](#_Toc205281475)

[5.3.5 Resolver (IResolver) 102](#_Toc205281476)

[5.3.6 Link Registry (ILinkRegistry) 103](#_Toc205281477)

[5.3.7 Simulator (ISimulator) 105](#_Toc205281478)

[5.3.8 Persistence 120](#_Toc205281479)

[5.3.9 Publication 121](#_Toc205281480)

[5.3.10 Type Registry 130](#_Toc205281481)

[5.3.11 Component Factory (IFactory) 139](#_Toc205281482)

[5.3.12 Event loop requirements 140](#_Toc205281483)

[5.3.13 Threading requirements 141](#_Toc205281484)

[5.4 Meta data 142](#_Toc205281485)

[5.4.1 Catalogue 142](#_Toc205281486)

[5.4.2 Package 148](#_Toc205281487)

[5.4.3 Configuration data 148](#_Toc205281488)

[6 Implementation mapping 149](#_Toc205281489)

[6.1 C/C++ Standard 149](#_Toc205281490)

[6.1.1 General 149](#_Toc205281491)

[6.1.2 Requirements 149](#_Toc205281492)

[6.2 Catalogue to C++ 150](#_Toc205281493)

[6.2.1 Mapping templates 150](#_Toc205281494)

[6.2.2 Namespaces and files 153](#_Toc205281495)

[6.2.3 Element and Type Visibility Kind 153](#_Toc205281496)

[6.2.4 Mapping of elements 154](#_Toc205281497)

[6.2.5 Basic Value Types 165](#_Toc205281498)

[6.2.6 Compound Value Types 167](#_Toc205281499)

[6.2.7 Reference Types 170](#_Toc205281500)

[6.3 Package to library 173](#_Toc205281501)

[6.3.1 Mapping templates 173](#_Toc205281502)

[6.3.2 Common to Unix and Windows 174](#_Toc205281503)

[6.3.3 Unix (Shared object) 175](#_Toc205281504)

[6.3.4 Addendum for Windows Dynamic Link Library (DLL) 177](#_Toc205281505)

[6.3.5 SMP Bundle 177](#_Toc205281506)

[Annex A (normative) Catalogue file - DRD 178](#_Toc205281507)

[A.1 Catalogue DRD 178](#_Toc205281508)

[A.1.1 Requirement identification and source document 178](#_Toc205281509)

[A.1.2 Purpose and objective 178](#_Toc205281510)

[A.2 Expected response 178](#_Toc205281511)

[A.2.1 Scope and content 178](#_Toc205281512)

[A.2.2 Special remarks 178](#_Toc205281513)

[Annex B (normative) Package file - DRD 179](#_Toc205281514)

[B.1 Package DRD 179](#_Toc205281515)

[B.1.1 Requirement identification and source document 179](#_Toc205281516)

[B.1.2 Purpose and objective 179](#_Toc205281517)

[B.2 Expected response 179](#_Toc205281518)

[B.2.1 Scope and content 179](#_Toc205281519)

[B.2.2 Special remarks 179](#_Toc205281520)

[Annex C (normative) Configuration file - DRD 180](#_Toc205281521)

[C.1 Configuration DRD 180](#_Toc205281522)

[C.1.1 Requirement identification and source document 180](#_Toc205281523)

[C.1.2 Purpose and objective 180](#_Toc205281524)

[C.2 Expected response 180](#_Toc205281525)

[C.2.1 Scope and content 180](#_Toc205281526)

[C.2.2 Special remarks 180](#_Toc205281527)

[Annex D (normative) Manifest file - DRD 181](#_Toc205281528)

[D.1 Manifest DRD 181](#_Toc205281529)

[D.1.1 Requirement identification and source document 181](#_Toc205281530)

[D.1.2 Purpose and objective 181](#_Toc205281531)

[D.2 Expected response 181](#_Toc205281532)

[D.2.1 Scope and content 181](#_Toc205281533)

[D.2.2 Special remarks 183](#_Toc205281534)

[Bibliography 184](#_Toc205281535)

**Figures**

[Figure 4‑1: Common Concepts and Type System 19](#_Toc205281536)

[Figure 4‑2: SMP Architecture 19](#_Toc205281537)

[Figure 4‑3: SMP State machine 21](#_Toc205281538)

[Figure 4‑4: Object mechanisms 25](#_Toc205281539)

[Figure 4‑5: Overview of components hierarchy 26](#_Toc205281540)

[Figure 4‑6: Component Mechanisms 27](#_Toc205281541)

[Figure 4‑7: Component State machine 27](#_Toc205281542)

[Figure 4‑8: Sequence of calls for dynamic invocation of an Operation 32](#_Toc205281543)

[Figure 4‑9: Sequence of calls for dynamic invocation of a Property Setter 34](#_Toc205281544)

**Tables**

[Table 4‑1: Overview of simulation states 22](#_Toc205281545)

[Table 4‑2: ViewKind values 30](#_Toc205281546)

[Table 5‑1: Primitive Types 37](#_Toc205281547)

[Table 5‑2: Component states 44](#_Toc205281548)

[Table 5‑3: Request Type 66](#_Toc205281549)

[Table 5‑4: Semantically equivalent types for connections 75](#_Toc205281550)

[Table 5‑5: Property Access Kind values 78](#_Toc205281551)

[Table 5‑6: Parameter Direction Kind values 81](#_Toc205281552)

[Table 5‑7: Default Log Message Kinds 82](#_Toc205281553)

[Table 5‑8: Condition for emitting predefined global events 101](#_Toc205281554)

[Table 5‑9: Library loading flags 119](#_Toc205281555)

[Table 6‑1: C++ declaration templates 150](#_Toc205281556)

[Table 6‑2: C++ definition templates 152](#_Toc205281557)

[Table 6‑3: C++ mapping for the Visibility kind attribute 153](#_Toc205281558)

[Table 6‑4: C++ mapping of Association depending on ByPointer attribute 156](#_Toc205281559)

[Table 6‑5: C++ mapping for the Direction kind attribute 157](#_Toc205281560)

[Table 6‑6: C++ mapping for Property depending on ByPointer attribute 159](#_Toc205281561)

[Table 6‑7: C++ mapping for the Operator attribute kinds 162](#_Toc205281562)

[Table 6‑8: C++ declaration templates for packages 173](#_Toc205281563)

Introduction

Space programmes have developed simulation software for a number of years, which are used for a variety of applications including analysis, engineering operations preparation and training. Typically, different departments perform developments of these simulators, running on several different platforms and using different computer languages. A variety of subcontractors are involved in these projects and as a result a wide range of simulation software are often developed. This standard addresses the issues related to portability and reuse of simulation models. It is based on the work performed by ESA in the development of the Simulator Model Portability Standards SMP1 and SMP2 starting from the mid-end of the nineties.

This standard integrates the ECSS-E-ST-40 with additional requirements which are specific to the development of simulation software. The formulation of this standard takes into account:

* The existing ISO 9000 family of documents, and
* The Simulation Model Portability specification version 1.2.

The intended readership of this standard is the simulator software customer and supplier.

# Scope

ECSS-E-ST-40-07 is a standard based on ECSS-E-ST-40 for the engineering of simulation software.

ECSS-E-ST-40-07 complements ECSS-E-ST-40 in being more specific to simulation software. Simulation software include both Simulation environments and simulation models. The standard enables the effective reuse of simulation models within and between space projects and their stakeholders. In particular, the standard supports model reuse across different simulation environments and exchange between different organizations and missions.

This standard can be used as an additional standard to ECSS-E-ST-40 providing the additional requirements which are specific to simulation software.

This standard may be tailored for the specific characteristic and constrains of a space project in conformance with ECSS-S-ST-00.

**Applicability**

This standard lays down requirements for simulation software including both Simulation environments and simulation models. The requirements cover simulation models’ interfaces and simulation environment interfaces for the purpose of model re-use and exchange to allow simulation models to be run in any conformant simulation environment.

A consequence of being compliant to this standard for a model is the *possibility* of being reused in several simulation facilities or even in several projects. However, adherence to this standard does not imply or guarantees model reusability, it is only a precondition. Other characteristics of the model, to be defined outside this standard, such as its functional interfaces and behaviour, its configuration data as well as quality, suitability and performance, etc. are also heavily affecting the potential for a model to be reused. In addition, agreements need to be reached on simulation environments compatibility, model validation status as well as legal issues and export control restrictions.

Therefore, this standard *enables* but does not mandate, impose nor guarantee successful model re-use and exchange.

Model reuse in this standard is meant both at source-code and binary level, with the latter restricted to a fixed platform.

# Normative references

The following normative documents contain provisions which, through reference in this text, constitute provisions of this ECSS Standard. For dated references, subsequent amendments to, or revision of any of these publications do not apply. However, parties to agreements based on this ECSS Standard are encouraged to investigate the possibility of applying the more recent editions of the normative documents indicated below. For undated references, the latest edition of the publication referred to applies.

|  |  |
| --- | --- |
| ECSS-S-ST-00-01 | ECSS system - Glossary of terms |
| ECSS-E-ST-40 | Space engineering - Software general requirements |
| [SMP\_FILES] | ECSS\_SMP\_L1\_(31March2025).zip – SMP Level 1 C++ Header files, XML schemas and Catalogue (Available from ECSS website). |
| <https://www.w3.org/TR/xmlschema11-2/> | XML schema specification |
| <http://www.opengroup.org> | The UUID specification from Open Group. |
| <https://www.osgi.org/developer/specifications/> | OSGi Specifications |

# Terms, definitions and abbreviated terms

## Terms from other standards

1. For the purpose of this Standard, the terms and definitions from ECSS-S-ST-00-01 and ECSS-E-ST-40 apply.
2. For the purpose of this Standard, the terms and definitions from ECSS‐E‐ST‐70 apply, in particular the following term:
   1. mission

## Terms specific to the present standard

In the following list of terms, underlined words are further defined in the same list.

1. aggregate

relationship between two components implemented by storing their references

1. Each component in such a relationship keeps its own lifecycle and it does not depend on that of other components.
2. association

relationship between two instances of any data-type, where each instance has its own lifecycle and there is no owner

1. component

building block of a simulation that can be instantiated and that has a well-defined contract to its environment

1. composite

component implementing composition

1. composition

hierarchical relationship where the child component is destroyed if the parent component is destroyed

1. configuration

specification of values for fields of components

1. constructor

specific operation of a component, bearing the same name of the component, whose purpose is to allocate and build an instance of said component

1. consumer

component that can receive data in one of its input fields from an output field of another component

1. container

typed collection of child components

1. contract

set of interfaces, operations, fields, properties, entry points, event sinks, event sources and all the associated constraints, used to interact with a component

1. data transfer

copy of value from an output field to an input field

1. entry point

operation without parameters that does not return a value, which can be added to the scheduler or event manager service

1. epoch time

absolute time of the simulation

1. event

see “simulation event”

1. event manager

component that implements the IEventManager interface

1. The IEventManager interface is specified in clause 5.3.4.
2. event sink

receiver of specific notifications, owned by a component and subscribed via a subscription mechanism

1. event source

emitter of specific notifications, owned by a component and offering a subscription mechanism

1. exception

non-recoverable error that can occur when calling into an operation or property

1. field

feature characterised by a value type and holding a value

1. input field

field explicitly marked for receiving values as a result of a data transfer

1. interface

named set of properties and operations

1. logger

component that implements the ILogger interface

1. The ILogger interface is specified in clause 5.3.1.
2. mission time

relative time measuring elapsed time from a mission specific point in time

1. model

component that implements the IModel interface

1. The IModel interface is specified in clause 5.2.3.2.
2. model implementation

executable code implementing a model

1. model instance

occurrence of a model implementation

1. output field

field explicitly marked for being the source of a value in a data transfer

1. operation

declaration of a behavioural feature of a component or an interface with the option to define parameters, return value and raised exceptions

1. package

collection of types, where each one is either a value type or a component

1. platform

set of subsystems/technologies that provide a coherent set of functionality through APIs and specified usage patterns

1. primitive type

type that can no longer be de-composed and that is pre-defined by the standard

1. The available primitive types are listed in Table 5‑1: Primitive Types.
2. property

typed feature of a class, an interface or a component that can be accessed by two operations, the setter and the getter, not necessarily both present

1. provider

component that can send data of one of its output fields to an input field of another component

1. reference

pointer to a component

1. When dealing with the C++ mapping, the term reference has a meaning specific to that language, whereas in the rest of this standard it means pointer to a component (but it cannot for instance be a pointer to a class).
2. resolver

component that implements the IResolver interface

1. The IResolver interface is specified in clause 5.3.5.
2. schedule

planned time ordered execution of entry points

1. scheduler

component that implements the IScheduler interface

1. The IScheduler interface is specified in clause 5.3.3.
2. service

component that implements the IService interface

1. The IService interface is specified in clause 5.2.3.3.
2. simple type

type that can be assimilated to a primitive type

1. simple field

field of simple type

1. simulation environment

platform implementing the standard E-ST-40-07 services (event manager, link registry, logger, resolver, scheduler and time keeper) and the ISimulator interface

1. simulation event

call to an entry point by either scheduler or event manager

1. The term “event” is synonymous.
2. simulation time

relative time since start of simulation

1. simulator

collection of services and hierarchy of model instances together with a simulation environment

1. simulation

single execution of a simulator

1. simulation service

service instance resolvable by name in the global scope of the simulation environment

1. source

component that owns one or more references, one or more event links, or one or more output fields

1. The term “source component” is synonymous.
2. source component

See source

1. target

component that implements one or more interfaces, provides one or more event sinks, or one or more input fields

1. The term “target component” is synonymous.
2. target component

see “target”

1. simulation timeline

sequence of executions of discrete events performed by the Scheduler service.

1. The Scheduler service is specified in clause 5.3.3.
2. time keeper

component that implements the ITimeKeeper interface

1. The ITimeKeeper interface is specified in clause 5.3.2.
2. value

state of a value type

1. value type

set of values which a variable can possess

1. Zulu time

the computer clock time, also called wall clock time

## Abbreviated terms

For the purpose of this Standard, the abbreviated terms and symbols from ECSS-S-ST-00-01 and the following apply:

| Abbreviation | Meaning |
| --- | --- |
| DES | Discrete-Event Simulation |
| SMDL | Simulation Model Definition Language |
| SMP | Simulation Modelling Platform |
| URI | Uniform Resource Identifier |
| URL | Uniform Resource Locator |
| UUID | Universally Unique IDentifier |

## Nomenclature

The following nomenclature applies throughout this document:

1. The word “shall” is used in this Standard to express requirements. All the requirements are expressed with the word “shall”.
2. The word “should” is used in this Standard to express recommendations. All the recommendations are expressed with the word “should”.
3. It is expected that, during tailoring, recommendations in this document are either converted into requirements or tailored out.
4. The words “may” and “need not” are used in this Standard to express positive and negative permissions, respectively. All the positive permissions are expressed with the word “may”. All the negative permissions are expressed with the words “need not”.
5. The word “can” is used in this Standard to express capabilities or possibilities, and therefore, if not accompanied by one of the previous words, it implies descriptive text.
6. In ECSS “may” and “can” have completely different meanings: “may” is normative (permission), and “can” is descriptive.
7. The present and past tenses are used in this Standard to express statements of fact, and therefore they imply descriptive text.

# Principles

## Objectives

The main objective of this standard is to enable the effective reuse of simulation models and applications within and between space projects and their stakeholders. In particular, the standard supports model reuse across different simulation environments and exchange between different organizations and missions.

The portability of models between different simulation environments is supported by defining a standard interface between the simulation environment and the models. Models can therefore be plugged into a different simulation environment without requiring any modification to the model source code.

The portability of models between different operating systems and hardware takes into consideration dependencies such as avoiding calls to operating specific APIs or use of hardware specific features. The guidelines to the model developer, on how to avoid developing models with such dependencies, is outside the scope of this standard.

## Common Concepts and common types

The main purpose of SMP is to promote platform independence, interoperability and reuse of simulation models. This is done by defining;

* Common Concepts: All SMP models fulfil common high-level concepts addressing fundamental modelling issues. This enables the development of models on an abstract level, which is essential for independence from simulation environments and reuse of models;
* Common Type System: All SMP models are built upon a common type system. This enables different models to have a common understanding of the syntax and semantics of basic types, which is essential for interoperability between different models.

In other words, models are using common concepts and a common type system to become interoperable. Thus, models ‘live’ in between these two common layers as shown in Figure 4‑1.



Figure 4‑1: Common Concepts and Type System

## Architecture

The SMP architecture covers two types of components;

* Simulation Models provide application specific behaviour;
* Simulation Environments provide Simulation Services.

This architecture is depicted in Figure 4‑2.



Figure 4‑2: SMP Architecture

An SMP compliant simulation environment provides the following six simulation services:

* Logger: Allows logging messages (see clause 5.3.1);
* Time Keeper: Provides the four different SMP time kinds (see clause 4.4 and 5.3.2);
* Scheduler: Allows calls of entry points based on timed or cyclic events (see clause 5.3.3);
* Event Manager: Provides mechanisms for global asynchronous events (see clause 5.3.4);
* Resolver: Provides the ability to get a reference to any model within a simulation (see clause 5.3.5);
* Link Registry: Maintains a list of the links between model instances (see clause 5.3.6).

In addition, it supports other concepts laid out in this standard via some dedicated interfaces:

* Simulation state machine controlling interface (see clause 4.5 and 5.3.7);
* Interfaces allowing self-persistence as described in clause 4.8 (see also IStorageReader in clause 5.3.8.1 and IStorageWriter in clause 5.3.8.2);
* Publication: A set of interfaces allowing models to publish their state to the simulation environment (see clause 5.3.9);
* Type registry: A registry allowing components to register types that later can be used for publication (see clause 5.3.10);
* Component Factory: Ability to create components via a factory (see clause 5.3.11).

The arrows in Figure 4‑2 indicate interaction between components. In SMP, communication is performed via interfaces. Two different types of interfaces can be identified in this architecture:

* Interfaces between components and the Simulation Environment, and
* Inter-component communication interfaces.

## Time handling principle

SMP defines four different time scales, referred to as time kinds (see clause 5.1.2 for exact specification):

* Simulation Time: Relative time since start of simulation, starting at 0 when the simulation is setup.
* Zulu Time: Zulu Time is the computer clock time, also called wall clock time.
* Epoch Time: The absolute time of the simulation.
* Mission Time: Mission time is a relative time, i.e. it measures elapsed time from a mission specific point in time.

SMP defines both Epoch and Mission Time as a fixed offset from Simulation Time. The Offset is set via calls to the SMP time keeper service and the two time kinds progress linearly with Simulation time. SMP does not define how Simulation time progress with respect to Zulu time. Typical examples of such a correlation is:

* **Real‐Time:** The simulation time progresses with real-time, where real‐time is typically defined by the computer clock.
* **Accelerated**: The simulation time progresses relative to real‐time using a constant acceleration factor. This factor can be larger than 1.0, which relates to ʺfaster than real‐timeʺ, or smaller than 1.0, which means ʺslower than real‐timeʺ, or 1.0, which coincides with real‐time.
* **Free Running**: The simulation time progresses as fast as possible, and is not related to real‐time. Typically, the speed is coordinated with the timed events of the scheduler, which underlines the close relationship between these two services (Time Keeper and Scheduler).

SMP does not mandate which of these modes a simulation environment supports.

## Simulation lifecycle

Any SMP simulation goes via a lifecycle as defined in Figure 4‑3. The simulation environment is responsible to ensure that this state diagram is followed. It is controlled via the ISimulator interface (see clause 5.3.7).




Figure 4‑3: SMP State machine

Each state in Figure 4‑3 has its own purpose and behaviour as explained in Table 4‑1. Notice that some state transitions are automatically performed by the Simulation Environment as indicated in Figure 4‑3, while others need explicit calls to the ISimulator interface.

ECSS-E-ST-40-07\_1630001

Table 4‑1: Overview of simulation states

| Name | Description |
| --- | --- |
| Building | In Building state, the model hierarchy is created. In this state, Publish() and Configure() can be called any time to call the corresponding Publish() and Configure() operations of each component. |
| Connecting | In Connecting state, the simulation environment traverses the model hierarchy and calls the Connect() method of each component. |
| Initialising | In Initialising state, the simulation environment executes all initialization entry points in the order they have been added to the simulator using the ISimulator AddInitEntryPoint() method (see 5.3.7). |
| Standby | The simulation environment does not progress simulation time. Only entry points registered relative to Zulu time are executed. |
| Executing | The simulation environment does progress simulation time. Entry points registered with any of the available time kinds are executed. |
| Storing | In Storing state, the simulation environment first stores the values of all fields published with the State attribute to storage (typically a file). Afterwards, the Store() method of all components (Models and Services) implementing the optional IPersist interface is called, to allow custom storing of additional information. |
| Restoring | In Restoring state, the simulation environment first restores the values of all fields published with the State attribute from storage. Afterwards, the Restore() method of all components implementing the optional IPersist interface is called, to allow custom restoring of additional information. |
| Reconnecting | In Reconnecting state, the simulation environment makes sure that models that have been added to the simulator after leaving the Building state are properly published, configured and connected. |
| Exiting | In Exiting state, the simulation environment is properly terminating a running simulation. |
| Aborting | In this state, the simulation environment attempts a simulation shut-down, whereby the simulation can stop executing as the users expect, without guaranties for actual release of resources. |

## Simulation method

### Discrete-event simulation (DES)

SMP is built on discrete-event simulation (DES) theory where the behaviour of a system is modelled as a discrete sequence of events in time. Each event that marks a change in the state of the systems occurs at a particular instant in time. The simulation can jump in time from one event to the next since no change in the system occurs between consecutive events.

The main elements in SMP that support this approach are:

* The simulation components schedule EntryPoints (see clause 5.2.7.1) on the SMP scheduler (see clause 5.3.3) for execution of events.
* The Simulation state is captured in the persisted data.

### Parallelization and distribution

SMP assumes a single scheduler executing its events in sequence. All components are loaded inside the same address space allowing direct communication between them. The standard however does not prevent parallelization or distribution to be built into layers on top of the standard.

### Inter component communication

#### Overview

SMP supports the following main methods of communication between components:

* Direct interface based communication
* Data flow based communication
* Event based communication

#### Interface based communication

An interface‐based design adds interfaces as the standard mechanisms for inter-model communication. This isolates the definition of an interface (the “contract”) from its implementation. In an interface‐based design, a model provides any number of interfaces. An Interface defines a contract between models. Every model implementing the interface provides all the functionality of the interface, so that every model which consumes this interface can rely on the interface implementation. As interfaces are a mechanism to de‐couple models, they do not give access to fields, but only to operations. With special operations (i.e. use of Properties. See definition 3.2.32 "property") that read or write a single value, access to fields can be added.

#### Data flow based communication

##### Overview

In a data flow based communication, two components exchange the value of a field. The Provider component transfers an Output field value into an Input field of the Consumer component. The Output field is said to be connected to the Input field through a Dataflow connection.

The dataflow communication can be automatic, i.e. whenever the Output field is updated by its owning component, the value is immediately propagated to the connected Input field. The output fields that take part in an automatic data flow based communication implement IOutputField where the IsAutomatic() method returns true when called (see 5.2.11.7).

The dataflow communication can be scheduled, i.e. when the Output field is updated by its owning component, the value is not automatically propagated to the connected Input field. The transfer is only performed on request, e.g. cyclically by the Simulation Environment, in scheduled simulation events. Hence, the “scheduled” terminology for this kind of dataflow transfer. The output fields that cannot perform automatic dataflow transfer implement IOutputField where the IsAutomatic() method returns false when called (see 5.2.11.7).

Both scheduled and automatic dataflow transfers are possible because SMP does not mandate the use of the one or of the other form. Furthermore, it does not mandate whether an Input field performs any specific action after it has been updated. An Input field can be implemented in a way that it notifies its containing model about a change, which can be used to trigger certain behaviour in the Consumer component.

##### Data types consideration

When two fields are involved in a dataflow connection, compatibility of the field types ensures correct transfer of data between the provider model and the consumer model.

Two levels of type compatibility are specified for the fields:

1. Strict compatibility: both fields are typed by the same type as identified by their type UUID published in the Type Registry. In this case, it is obvious that the fields can be connected via a dataflow connection.
2. Equivalence: the types are equivalent as per their semantics or physical representation. For example, when type 1 is a user-defined type Voltage mapped on a Smp::Float64 and type 2 is an user-defined type Tension mapped on Smp::Float64. As both type 1 and type 2 are Smp::Float64, they are said “equivalent”. Dataflow connection is allowed as there is no issue to transfer information between type 1 and type 2.

#### Event Based communication

For an event‐based design the components are modelled using Event Sinks (see 5.2.6.1) and Event Sources (see 5.2.6.2). Events issued by the source are received by all sinks subscribed to receive the corresponding events.

## Models, Services and Components

### Objects

An object is the base class for all SMP elements. It provides the basic features of a name, description and parent to all SMP elements. This implies that all SMP elements are organized in a hierarchical structure and always able to traverse upwards towards its root. The elements inheriting directly from Object are:

* Entry Points (IEntryPoint) as void operations that can be called by the scheduler and event manager services;
* Entry Point Publisher (IEntryPointPublisher) for publishing of entry points;
* Event Sinks (IEventSink) and Event Sources (IEventSource) for event based communication between objects;
* Composites (IComposite) and Containers (IContainer) to build the object hierarchy;
* References (IReference) allowing objects reference other components;
* Operations (IOperation) for callable functions.
* Properties (IProperty) for data objects accessed through a getter and/or a setter operation;
* Components (IComponent) implementing the simulation behaviour;
* Types (IType) to be used for the definition of fields, properties, operation parameters and operation return values;
* Factory (IFactory) that creates components;
* Persistent Objects (IPersist) that can store and restore their state. IPersist is the basis for the following important elements:
  + Fields (IField) to hold the simulation state and data;
  + Failures (IFailure) to allow objects to represent a failure in a system.




Figure 4‑4: Object mechanisms

### Components




Figure 4‑5: Overview of components hierarchy

The functionality of an SMP based simulator is implemented in elements that implement the IComponent (see 5.2.3.1) interface. A component represents an implementation of a self-contained feature with well-defined interfaces to other components. At initialization time, a simulation is built by assembling a set of instances of components. In addition, to implementing the IComponent interface, a number of additional optional component mechanisms are specified (see Figure 4‑6):

* Component aggregation (IAggregate),
* Inter-component events (IEventProvider and IEventConsumer),
* Dynamic invocation (IDynamicInvocation),
* Link management features (ILinkingComponent),

See clause 5.2 for details on Component Mechanisms.

The Simulator itself is an object, in particular a composite. All its direct children are components, namely models and services.




Figure 4‑6: Component Mechanisms

All SMP components goes via a lifecycle as defined in Figure 4‑7. Each component is responsible to ensure that this state diagram is followed. It is controlled via the IComponent interface (see clause 5.2.3.1).




Figure 4‑7: Component State machine

Each state in Figure 4‑7 has its own purpose and behaviour as explained in Table 5‑2.

### Factories

A Factory is an Object that creates Components. The type of the Component instantiated by the Factory is identified by a Universally Unique Identifier (UUID). The UUID is a 128-bit number which for practical purposes is unique, without depending for uniqueness on a central registration authority or coordination between the parties generating them. The purpose of the Factory is to hide the implementation details of how a Component is instantiated. For example, the base class of the Component implementation is hidden by the Factory.

A Factory is an Object that implements the IFactory interface. The Factory is registered with the simulator by calling the ISimulator::RegisterFactory method. Instances of the Component identified by the Component’s UUID can then be created by calling the ISimulator::CreateInstance method which uses the registered Factory to instantiate the Component.

### Models and Services

Two main flavours of components are specified by SMP: Models and Services. The main differences are:

* Models implement the IModel interface while Services implement the IServices interface. Both interfaces are empty and do not add any additional capabilities, but the difference allows to efficiently differentiate models and services.
* Models are added to the simulation in a hierarchical tree, while services live in the global scope of the simulation.
* The Models can be fallible by implementing the IFallibleModel interface but Services are not.
* Models are added to the Simulations via the ISimulator AddModel method, while Services are added via the AddService method.
* It is possible to get a reference to a service from the ISimulator interface via the GetService method by its name. This implies that all components in a simulation can easily obtain a reference to a service.
* Services can only be added to the simulation during the first startup in building phase, while models can be dynamically added also later in stand-by state.

The mandatory features of an SMP runtime environment are specified as services. See clause 5.3 and Figure 4‑5.

## Publication, Types and Persistence

SMP components publish their state information to the simulation environment to:

* Allow visualization of the simulation state.
* Allow the simulation environment to interact with the state of the component.
* Allow the simulation environment to store and restore the state of the component via the SMP persistence mechanism.

Objects that can be published include Fields (data objects), Properties (data objects updated through dynamic invocation) and Operations (called through dynamic invocation).

Fields, Properties, Operation parameters (in and return parameters) are published against Types (IType) registered with the Type Registry (ITypeRegistry). Each Type is identified uniquely by an UUID. An SMP value Type can be:

* A Primitive type: all types listed in the PrimitiveTimeKind enumeration (see Table 5‑1). Primitive type UUIDs are constants defined in PrimitiveTypes.h [SMP\_FILES].
* Simple type: type that can be assimilated to a Primitive type, i.e. the corresponding IType GetPrimitiveTypeKind method returns a type kind other than PTK\_None. This groups all the user-defined Integer, Enumeration (IEnumerationType), Float and String types. Note that a String type is a type that represents a Smp::Char8 string which has a maximum length and which is encoded in UTF-8. Calling the IType GetPrimitiveTypeKind method on a String type returns PTK\_String8.
* Array type (IArrayType): type that represents a fixed-length sequence of items typed by the same type. The item type can be any possible type. A particular array is a simple type array that contains simple type or primitive type items.
* Structure type (IStructureType): type that represents a Structure composed of a number of Fields.
* Class (IClassType) type: is a specialized Structure type.

A complex type designates a type that is not a simple type. This includes arrays (of simple type items or not), structures and classes, which are actually derived structures.

The simulation environment has to resolve the type associated with a published object by searching for its UUID in the Type Registry at publication time.

All published fields are annotated with a set of attributes provided by the SMP component to the Simulation Environment:

* A View Kind attribute indicating which kind of user this information is intended for. The values and intended interpretation of these values by the Simulation Environment is given in Table 4‑2.
* If the field is part of the simulation state or not (State attribute of field).
* If it is an Input, or an Output, or an Input/Output field (Input and Output attributes of field).

Additional meta information can also be provided via the SMP Catalogue (see 5.4.1).

Table 4‑2: ViewKind values

| Name | Intended interpretation |
| --- | --- |
| VK\_None | The element is not made visible to the user. |
| VK\_Debug | The element is made visible for debugging purposes. The element is not visible to end users. If the simulation environment supports the selection of different user roles, then the element is intended to be visible to ʺDebugʺ users only. |
| VK\_Expert | The element is made visible for expert users.  The element is not visible to end users. If the simulation environment supports the selection of different user roles, then the element is intended to be visible to ʺDebugʺ and ʺExpertʺ users. |
| VK\_All | The element is made visible to all users. (this is the default) |

From the list of published fields, the simulation environment is able to determine the state of a simulation and #re it (or to restore it when needed). This is called persistence. Persistence of SMP components can be handled in one of two ways:

* **External Persistence**: The simulation environment stores and restores the model’s state by directly accessing the fields that are published to the simulation environment, i.e. via the IPublication (See 5.3.9.1) interface.
* **Self‐Persistence**: The component can implement the IPersist (See 5.2.9) interface, which allows it to perform special operations during store and restore in addition to external persistence. Typically, self-persistence allows the persistence of dynamic data structures (e.g. events on the simulation schedule). Two approaches exist in this case for models to store their data:
  + Its state or parts of it can be stored/restored in the storage that is provided by the simulation environment via the IStorageReader (see 5.3.8.1) and IStorageWriter (see 5.3.8.2) interfaces provided by the simulation environment.
  + The component can query the filename and location of the storage file from the environment via the IStorageReader (see 5.3.8.1) and IStorageWriter (see 5.3.8.2) interfaces and store additional files in the same location. This mechanism is usually only needed by specialised models, for example embedded models that need to load on‐board software from a specific file.

SMP Runtime Environments supports both External and Self-Persistence. For models and components, only external persistence is a mandatory feature, while self-persistence is an additional optional mechanism.

## Dynamic invocation

SMP supports dynamic invocation allowing interaction between simulation environments and simulation models. This is typically used during execution allowing to control a simulation via scripting. It is a mechanism that makes the operations of a component available via a standardised interface.

In order to allow calling a named method with any number of parameters, a request object is created which contains all information for the method invocation. This request object is also used to transfer back a return value. The dynamic invocation concept standardises the request objects (IRequest interface, see 5.2.8.2). In addition, two methods are provided as part of IOperation to create and delete request objects. Getting an IOperation object can be done from either the IDynamicInvocation or the IPublication interface using the GetOperation method. The reason for offering the call in different interfaces is to minimise the number of round‐trips between a client (that calls a method) and a component that implements IDynamicInvocation:

* Creation of request objects from a client component that is located outside of the Simulation Environment can call first the GetOperation method of IDynamicInvocation to obtain the Operation object, which is followed by the CreateRequest method of IOperation.
* But for example, creation of request objects from a client component that is part of the Simulation Environment can use instead the GetOperation method of IPublication.

The sequence diagram in Figure 4‑8 shows all steps involved when using the IOperation CreateRequest() and DeleteRequest() methods.




Figure 4‑8: Sequence of calls for dynamic invocation of an Operation

The sequence diagram in Figure 4‑8, using a Client component and a Model implementing IDynamicInvocation, contains the following steps:

* 1. The Client calls the GetOperation() method of the Model to obtain the Operation that the Client wants to invoke.
  2. The Client calls the CreateRequest() method of the Operation to create a request object for the Operation.
  3. The Operation creates a Request object for the operation, using the published operation signature.
  4. The Operation returns the Request object via its IRequest interface to the Client.
  5. The Client calls the SetParameterValue() method of the Request object to set parameters to non‐default values.
  6. The Client calls the Invoke() operation of the Operation to invoke the corresponding operation.
  7. The Operation may delegate the Invoke handling to the Model Invoke method (Model should be the parent object of Operation). Delegation is possible if the Operation object has been created and published by the Model.
  8. The Model calls the GetParameterValue() method of the Request object to get operation parameters.
  9. The Model calls its internal method that corresponds to the invoked operation.
  10. The Model calls the SetReturnValue() operation of the Request object to set the return value.
  11. The Model and the Operation return control to the Client.
  12. The Client calls the GetReturnValue() operation of the Request object to get the return value.
  13. The Client calls the DeleteRequest() method of the Operation to delete the Request object.
  14. The Operation destroys the request object.
  15. The Operation returns control to the client.

Dynamic Invocation is also used for calling the Property getter and setter operations. The request object GetType method can be used to query the request type, which can be Invoke (i.e. request is related to an operation like described above), Get (i.e. request is related to a property getter) and Set (i.e. request is related to a property setter). The sequence diagram for invoking a property setter is shown in Figure 4‑9.




Figure 4‑9: Sequence of calls for dynamic invocation of a Property Setter

The sequence diagram in Figure 4‑9, using a Client component and a Model implementing IDynamicInvocation, contains the following steps:

* 1. The Client calls the GetProperty() method of the Model to obtain the Property that the Client wants to set.
  2. The Client calls the SetValue() method of the Property.
  3. The Property calls the SetParameterValue() method of the internal Request object, which should correspond to the property setter, to set the new value.
  4. The Property calls the Invoke() operation of the Model to invoke the corresponding method.
  5. The Model calls the GetName() and GetType() methods of the request object to determine the property to set.
  6. The Model calls the GetParameterValue() operation of the Request object to get the setter parameter.
  7. The Model calls its internal method that corresponds to the property setter.
  8. The Model return control to the Property.
  9. The Property returns control to the Client.

## Components meta data

### Catalogue

Meta data for SMP objects are stored in XML documents called the Catalogue. Having the SMP objects described in XML catalogues allows taking benefit from the XML language, for example:

* Generation of the catalogues from UML diagrams
* Generation of model documentation from the catalogue
* Generation of model skeleton code from the catalogue (See clause 6.1).

The content of a catalogue is hierarchically ordered in namespaces that may be nested. Inside each namespace many uniquely named instance of the following SMP features can be found:

* Type definitions including:
  + Exceptions
  + Data Types
* Interface specifications
* Component and model specifications including:
  + Event Sinks and Sources
  + Constants, Fields and Properties
  + Entry Points
  + Operations
  + Containment and inheritance
  + Interfaces, associations and references
* Attributes that can be attached to elements:
  + Fallible and Forcible
  + Min and Max limits for types
  + View/ViewKind information determines the visibility of the element

For all the elements above, meta data can be added like the description of each element or the engineering unit for type definitions. From this, it can be seen that the Catalogue definition provides a rich capability to describe the complete external interface of all SMP components. In fact, the interfaces as described in the SMP standard can as well be expressed in a catalogue. See ecss.smp.l1.smpcat as referenced in clause 5.4.1.2.1a.

### Package

A package describes how implementations of types defined in catalogues are packaged. This includes not only models, which may have different implementations in different packages, but as well all other user‐defined types.

### Configuration

A configuration document allows specifying arbitrary field values of component instances in the simulation hierarchy. This can be used to initialise or reinitialise the simulation.

## Model exchanges considerations

### Overview

One of the primary goals of SMP is to allow model exchanges based on the Package concept.

Model source code exchange is considered easier than binary exchange as some considerations are important to be taken into account when exchanging binary models.

The mapping of a Package to C++ defines which symbols a static or dynamic library of SMP has to expose. This enables binary distribution of models, where only the catalogues and/or header files (for the compiler) and the libraries (for the linker) are provided, but no implementation source code. Nevertheless, binary compatibility depends on a number of other constraints, which may even vary between operating systems and compilers.

### SMP Bundle

For distribution of a binary package SMP bundles are used. A SMP Bundle is an archive (e.g. a tar file on Linux, or a zip file on Windows) which provides the following elements:

* One or more SMDL packages.
* One or more package dynamic libraries, directly related to the SMDL packages.
* One or more package static libraries, directly related to the SMDL packages.
* All the SMP catalogues related to the SMDL packages.
* Optionally include other artefacts (SMDL configurations) and/or the related source code for all or parts of the included SMDL packages.

The related structure of folders and files within the bundle, and the names of folders and files are not standardised.

The added value of a Bundle is the additional SMP.MF Bundle Manifest file.

This Manifest is an ASCII file (aligned with the OSGi bundle manifest format) which contains key-value pairs with important meta data for the bundle.

# Interface requirements

## Common

### Primitive Types specification

ECSS-E-ST-40-07\_1630002

All SMP fields, parameters, constants and properties shall be of either a Primitive Type as per PrimitiveTypes.h in [SMP\_FILES], or a User Defined Type published to the Type Library.

1. This specification is compliant with the types specified in Table 5‑1.

ECSS-E-ST-40-07\_1630003

Mapping between SMP types, XML types and ISO/ANSI C++ types shall be as per Table 5‑1.

1. C++ mapping for primitive types is provided by PrimitiveTypes.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630004

Table 5‑1: Primitive Types

| SMP Type | XML mapping | C++ mapping | Description |
| --- | --- | --- | --- |
| Char8 | xsd:string | char | 8 bit character type to represent textual characters |
| String8 | xsd:string | const char\* | 8-bit character strings based on UTF-8 encoding, which is commonly used in XML |
| Bool | xsd:boolean | bool | Bool is a binary logical type with values true or false |
| Int8 | xsd:byte | int8\_t | 8 bit signed integer |
| UInt8 | xsd:unsignedByte | uint8\_t | 8 bit unsigned integer |
| Int16 | xsd:short | int16\_t | 16 bit signed integer |
| UInt16 | xsd:unsignedShort | uint16\_t | 16 bit unsigned integer |
| Int32 | xsd:int | int32\_t | 32 bit signed integer |
| UInt32 | xsd:unsignedInt | uint32\_t | 32 bit unsigned integer |
| Int64 | xsd:long | int64\_t | 64 bit signed integer |
| UInt64 | xsd:unsignedLong | uint64\_t | 64 bit unsigned integer |
| Float32 | xsd:float | float | IEEE 754 single-precision floating-point type with a length of 32 bits. |
| Float64 | xsd:double | double | IEEE 754 double-precision floating-point type with a length of 64 bits. |
| Duration | xsd:duration restricted to days, hours, minutes and seconds | int64\_t | Duration in nanoseconds.  See 5.1.1c for detailed specification. |
| DateTime | xsd:dateTime | int64\_t | Absolute time in nanoseconds.  See 5.1.1d for detailed specification |

ECSS-E-ST-40-07\_1630005

The Duration type as per Table 5‑1 shall be used for specifying a duration, as follows:

It is expressed in nanoseconds;

It is stored in a signed 64 bit integer;

Positive values correspond to positive durations;

Negative values correspond to negative durations.

* 1. 1 Nanoseconds is the lowest level of granularity supported for time in SMP.
  2. 2 The duration type allows specifying values roughly between ‐290 years and 290 years.
  3. 3 The duration type allows expression of relative time, hence “negative duration” implies a relative time in the past.

ECSS-E-ST-40-07\_1630006

The DateTime type as per Table 5‑1 shall be used for absolute time values, as follows:

It is expressed in nanoseconds, relative to the reference time of 01.01.2000, 12:00, Modified Julian Date (MJD) 2000+0.5;

It is stored in a signed 64 bit integer;

Positive values correspond to times after the reference time;

Negative values correspond to time values before the reference time.

* 1. 1 Nanoseconds is the lowest level of granularity supported for time in SMP.
  2. 2 DateTime allows specifying time values roughly between 1710 and 2290.

ECSS-E-ST-40-07\_1630007

An SMP Simple Field shall be of simple type.

ECSS-E-ST-40-07\_1630008

The AnySimple type shall hold a Primitive Type as per AnySimple.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630009

The AnySimpleArray type shall be an array of AnySimples as per AnySimpleArray.h in [SMP\_FILES].

### Time Kinds

ECSS-E-ST-40-07\_1630010

Simulation time shall be used for keeping the progress of time with respect to the start of the simulation, with the following properties:

Simulation time is a non-negative Duration type;

Simulation time is initialised to 0 at the beginning of the Building state as per Table 4‑1;

Simulation time changes only when:

The simulation is progressing in the Executing state;

As a result of restoring a simulation state;

As a result of ITimeKeeper SetSimulationTime.

It is not specified how quickly simulation time is progressed when the simulator is in Executing state;

Simulation time is part of a simulation state, that can be stored and restored.

ECSS-E-ST-40-07\_1630011

Mission time shall be used for keeping the progress of relative time with respect to a Mission Start time, with the following properties:

Mission time is initialised to 0 at the beginning of the Building state as per Table 4‑1;

Mission Time is calculated as a fixed offset between the current Epoch time and the given Mission start time according to the following formula: MissionTime = EpochTime – MissionStartTime;

The Mission time progresses with Epoch time;

The Mission time offset from Epoch time, the Mission start time changes by calls to:

the ITimeKeeper SetMissionTime method;

the ITimeKeeper SetMissionStartTime method.

Mission time only progresses when the simulation environment is in Executing state;

Mission time is stored and restored in the storing and restoring states;

Mission time is expressed as a Duration type.

ECSS-E-ST-40-07\_1630012

Zulu time shall be time dependent on the system clock of the host machine or an external clock source expressed, with the following properties:

Zulu time is expressed as a DateTime type;

Zulu time is not stored to and restored from simulation states.

1. High Real Time systems sometimes use an external clock source instead of the local system clock of host machine.

ECSS-E-ST-40-07\_1630013

Epoch time shall be time dependent on the Simulation time with a fixed offset, with the following properties:

Epoch time is expressed as a DateTime type;

Epoch time is stored to and restored from simulation states.

1. Epoch time progresses with Simulation time.

ECSS-E-ST-40-07\_1630014

Epoch time may be changed with the ITimeKeeper SetEpochTime method.

* 1. 1 ITimeKeeper SetEpochTime is defined in clause 5.3.2.
  2. 2 Mission Time is affected by the ITimeKeeper SetEpochTime method.

### Path string

ECSS-E-ST-40-07\_1630015

An SMP path string shall be a representation of a valid route from an SMP object in the hierarchy to another SMP object.

* 1. 1 Examples of valid path strings:
     + /Satellite/Receivers/Receiver1
     + /Logger
     + /Logger/
     + ../../Transmitters/Transmitter4
     + ./Satellite/../Satellite//Receivers/
  2. 2 Examples of invalid path strings:
     + “/..”, parent of root object do not exist
     + “…”, meaning of triple dots not defined.

ECSS-E-ST-40-07\_1630016

Both Absolute and Relative path strings shall be supported and distinguished as follows:

Paths starting with a delimiter are absolute paths from the simulation root object;

Paths not starting with a delimiter are relative paths from the current object.

ECSS-E-ST-40-07\_1630017

The delimiter between component names in the path string shall be ”/”.

ECSS-E-ST-40-07\_1630018

The delimiters between components and its children objects that are not components shall be either “/” or “.”.

1. This allows “Component.Operation()” to be used as path.

ECSS-E-ST-40-07\_1630019

Trailing delimiters shall be allowed in path strings.

ECSS-E-ST-40-07\_1630020

It shall be possible to reference the parent object by the “..” string.

ECSS-E-ST-40-07\_1630021

It shall be possible to reference the current object by:

the “.” string

an empty string “”

1. This allows the following to be used as path to operations of current object:
   * + .Operation()
     + ./Operation()

ECSS-E-ST-40-07\_1630022

The path string shall allow an element in an array to be identified by “[n]” trailing the array name where “n” is the zero based element index, with no delimiter.

1. This allows the following to be used for addressing element 2 of an array “MyArray” in MyModel:
   * + MyModel/MyArray[2]
     + MyModel.MyArray[2]

### Universally Unique Identifiers (UUID)

ECSS-E-ST-40-07\_1630023

All SMP types shall have a unique UUID as per Uuid.h in [SMP\_FILES].

* 1. 1 The UUID follows the specification from Open Group (http://pubs.opengroup.org/onlinepubs/9629399/apdxa.htm)
  2. 2 The UUID is a 128 bit long unique identifier.
  3. 3 The UUID allows for example to:
     + Uniquely identify types defined in catalogues so that can be bound with implementations defined within packages.
     + Uniquely identify linked elements within a Catalogue.

### Exception specification

ECSS-E-ST-40-07\_1630024

All SMP exceptions shall inherit from the Exception class as per Exception.h in [SMP\_FILES] providing the following information:

The description of the exception;

The name of the exception;

The exception message;

The sender of the exception when the exception originates from an SMP Object.

1. This covers both exceptions defined in this standard and user defined exceptions.

## Components and Objects interfaces

### Object Specification (IObject)

ECSS-E-ST-40-07\_1630025

All SMP objects shall provide the following features as per IObject.h in [SMP\_FILES]:

If the object is not an array element, a name of the object as follows:

Not be empty;

Start with a letter;

Contain only letters, digits, and underscore (ʺ\_ʺ);

Not be an ISO/ANSI C++ keyword.

If the object is an array element, the name shall be “[i]“ where “i” is a zero based element index;

A description of the object;

The parent object as follows:

An IObject pointer to the parent if the object has a parent;

A nullptr if the object does not have a parent.

A collection of contained or child objects, each accessed by its name.

* 1. 1 The Object description may be empty.
  2. 2 All SMP elements inherit from the IObject interface including:
     + Entry Points
     + Event Sinks and Sources
     + Fields
     + Containers
     + References
     + Failures
     + Components
     + Composites
     + Factories
     + Types
     + Properties
     + Operations

ECSS-E-ST-40-07\_1630026

All SMP objects with the same parent that are to be resolved by the Resolver shall have a unique name.

ECSS-E-ST-40-07\_1630027

The validity of the SMP name shall be checked when an SMP object is created, with the following behaviour:

If an object with an invalid name is created, it throws a InvalidObjectName exception as per InvalidObjectName.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630028

The Entry Points, Event Sinks, Event Sources, Fields, Properties, Operations, Containers, References, and Failures that are contained in respectively an EntryPointPublisher, EventConsumer, EventProvider, Component, Composite, Aggregate or FallibleModel shall have the respective object as their parent.

ECSS-E-ST-40-07\_1630029

Name, Description and Parent of an SMP object as specified in 5.2.1a shall never change during its lifetime.

### Collection Specification (ICollection)

ECSS-E-ST-40-07\_1630030

All SMP Collections of SMP elements shall implement the ICollection interface as per ICollection.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630031

The ICollection at method shall return the element with the given position or name, with the following behaviour:

If no element exists with the given position or name, it returns nullptr.

ECSS-E-ST-40-07\_1630032

The ICollection size method shall return the number of elements in the collection.

ECSS-E-ST-40-07\_1630033

The ICollection empty method shall return true if the collection contains zero elements, and false otherwise.

ECSS-E-ST-40-07\_1630034

The ICollection begin method shall return the collection begin iterator.

ECSS-E-ST-40-07\_1630035

The ICollection end method shall return the collection end iterator.

### Component Specification

#### Component (IComponent)

ECSS-E-ST-40-07\_1630036

All SMP Components shall implement the IComponent interface as per IComponent.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630037

The IComponent GetState method shall return the current state of the component as per ComponentStateKind.h in [SMP\_FILES], specified in Table 5‑2.

ECSS-E-ST-40-07\_1630038

Table 5‑2: Component states

| Name | Description |
| --- | --- |
| CSK\_Created | The Created state is the initial state of a component. Component creation is done by an external mechanism, e.g. by factories.  This state is entered automatically after the component has been created.  This state is left via the Publish() state transition. |
| CSK\_Publishing | In Publishing state, the component is allowed to publish features. This includes publication of fields, operations and properties. In addition, the component is allowed to create other components.  This state is entered via the Publish() state transition.  This state is left via the Configure() state transition. |
| CSK\_Configured | In Configured state, the component has performed initial configuration. This configuration can be done by external components, or internally by the component itself, e.g. by reading data from an external source.  This state is entered via the Configure() state transition.  This state is left via the Connect() state transition. |
| CSK\_Connected | In Connected state, the component is connected to the simulator. In this state, neither publication nor creation of other components is allowed anymore. Configuration performed via loading of SMDL configuration file and/or calling of initialisation entry point are performed in this state.  This state is entered via the Connect() state transition.  This state is left via the Disconnect() state transition or on simulation termination. |
| CSK\_Disconnected | In Disconnected state, the component is disconnected from the simulator, and all references to it are deleted, so that it can be deleted.  This state is entered via the Disconnect() state transition.  This is the final state of a component, and only left on deletion. |

ECSS-E-ST-40-07\_1630039

The IComponent Publish method shall be used by components to publish all publishable fields, properties and operations, with the following argument and behaviour:

Argument:

“receiver” giving a pointer to the IPublication instance for the component.

Behaviour:

If the component is not in Created state, then it throws an InvalidComponentState exception as per InvalidComponentState.h in [SMP\_FILES];

If the component is in Created state, then it enters the Publishing state;

After entering Publishing state, it publishes its fields, properties and operations using the provided receiver argument;

While in publishing state, it can create new components;

* 1. 1 Components can override the implementation of operations and properties from their base components, hence it is possible that the same property and operation are published multiple times. In this case, the last call to Publish overrides the previous calls.
  2. 2 Newly created components are in Created state. The simulator is responsible for the triggering of state transitions of new components.

ECSS-E-ST-40-07\_1630040

The IComponent Configure method shall be used to perform initial configuration of the component, with the following arguments and behaviour:

Arguments:

“logger” giving a pointer to the ILogger instance for the component, to provide the possibility to log messages during its configuration;

“linkRegistry” giving a pointer the ILinkRegistry instance for the component, to provide the possibility to register links.

Behaviour:

If the component is not in Publishing state, it throws an InvalidComponentState exception as per InvalidComponentState.h in [SMP\_FILES];

If the component is in Publishing state, it creates and configures other features and even other components using the field values of its published fields as sole source of configuration information for the creation of such components;

After completing the configuration actions, the component enters Configured state.

ECSS-E-ST-40-07\_1630041

The IComponent Connect method shall allow the components to connect to the simulator environment and other components, with the following argument and behaviour:

Argument:

“simulator” giving a pointer to the ISimulator interface as per ISimulator.h in [SMP\_FILES] to access services from the simulation environment.

Behaviour:

If the Component is not in Configured state, it throws an InvalidComponentState exception as per InvalidComponentState.h in [SMP\_FILES];

If called in Configured state, the component enters Connected state;

After entering Connected state, it connects to simulation services used by the component, if any.

1. It is guaranteed that all models have been created, published and configured before the Connect method of any component is called.

ECSS-E-ST-40-07\_1630042

The IComponent Disconnect method shall disconnect the component from the simulation environment and any other components, with the following behaviour:

If the Component is not in Connected state, it throws an InvalidComponentState exception as per InvalidComponentState.h in [SMP\_FILES];

If called in Connected state, the component enters Disconnected state;

After entering Disconnected state, the component disconnects from simulation services by deleting all references of these services in the component.

ECSS-E-ST-40-07\_1630043

The IComponent GetField method shall provide access to the IField interface for fields of the component, taking the following argument and behaviour:

Argument:

“fullName” giving the path of the field for whom it returns the IField interface.

Behaviour:

If the passed fullName does not exist, it returns nullptr;

If the passed field name exists and it is a field of simple type it returns its ISimpleField interface;

If the passed field name exists and it is an array field it returns its IArrayField or ISimpleArrayField interface;

If the passed field name exists and it is a structure field it returns its IStructureField interface.

1. This includes fields of structures and items of arrays.

ECSS-E-ST-40-07\_1630044

The IComponent GetFields method shall return a collection of the component fields as per FieldCollection in FieldCollection.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630045

The IComponent GetUuid method shall return a reference to the UUID of the component, as per Uuid.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630046

The IComponent GetSimpleValue method shall return a simple type value with the following arguments and behaviour:

Argument:

“fullName” giving the path of the simple field or of an item of a simple array field for which it returns the value.

Behaviour:

If the passed fullName does not exist, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed fullName exists and it is not a value of simple type, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed fullName exists and it is a value of simple type, it returns its value as an AnySimple as per AnySimple.h in [SMP\_FILES].

1. Simple values can include as well simple array items or structure simple type sub-fields.

ECSS-E-ST-40-07\_1630047

The IComponent SetSimpleValue method shall set a simple type value with the following arguments and behaviour:

Argument:

“fullName” giving the path of the simple field or of an item of a simple array field for which it sets the value;

“value” giving the value to be set as an AnySimple as per AnySimple.h in [SMP\_FILES].

Behaviour:

If the passed fullName does not exist, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed fullName exists and it is not a value of simple type, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed value type does not match the type of the target field, it throws an InvalidFieldValue exception as per InvalidFieldValue.h in [SMP\_FILES];

If the passed fullName exists and it is a value of simple type, it sets the field value to the value given in the arguments.

1. Simple values can include as well simple array items or structure simple type sub-field.

ECSS-E-ST-40-07\_1630048

The IComponent GetSimpleArrayValue method shall return the value of a simple array with the following arguments and behaviour:

Argument:

“fullName” giving the path of the simple array field or of a simple array value, which can be part of a field, for which it returns the values;

“values” containing the returned array item values as an AnySimpleArray as per AnySimpleArray.h in [SMP\_FILES];

“length” giving the number of items that the values array can contain;

“startIndex” giving the start index within the simple array values from which values are returned.

Behaviour:

If the passed fullName does not exist or is not the name of a simple array field or of a simple array value, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed fullName is valid as per (a) and it has a size not compatible with the requested range as given by the startIndex and length arguments, it throws an InvalidArraySize exception as per InvalidArraySize.h in [SMP\_FILES];

If the passed fullName exists and the field is valid with regards to (a) and (b), it fills in the values argument with the array item values.

ECSS-E-ST-40-07\_1630049

The IComponent SetSimpleArrayValue method shall set the value of a simple array with the following arguments and behaviour:

Argument:

“fullName” giving the path of the simple array field or of a simple array value, which can be part of a field, for which it sets the values;

“values” containing the array item values to be set as an AnySimpleArray as per AnySimpleArray.h in [SMP\_FILES];

“length” giving the number of items that the values array can contain;

“startIndex” giving the start index within the simple array values from which values are to be set.

Behaviour:

If the passed fullName does not exist or is not the name of a simple array field or of a simple array value, it throws an InvalidFieldName exception as per InvalidFieldName.h in [SMP\_FILES];

If the passed fullName is valid as per (a) and it has a size not compatible with the requested range given by the startIndex and length arguments, it throws an InvalidArraySize exception as per InvalidArraySize.h in [SMP\_FILES];

If one of the passed values has a type that does not match the type of the target field, it throws an InvalidFieldValue exception as per InvalidFieldValue.h in [SMP\_FILES];

If the passed fullName exists and the field is valid with regards to (a), (b) and (c), it sets the array item values to the values argument.

ECSS-E-ST-40-07\_1630050

The IComponent AddChild method shall add a new child object to the component with the following arguments and behaviour:

Arguments:

“child” giving the child object to add to the component;

“collection” giving the collection under the component to which the child object is added.

Behaviour:

It returns false if the given collection is not a valid collection under the IComponent object;

It returns false if the child object is already present in the given collection;

Otherwise, it returns true if the child object is successfully added.

ECSS-E-ST-40-07\_1630051

The IComponent RemoveChild method shall remove a child object from the component with the following arguments and behaviour:

Arguments:

“child” giving the child object to remove from the component;

“collection” giving the collection under the component from which the child object is removed.

Behaviour:

It returns false if the given collection is not a valid collection under the IComponent object;

It returns false if the child object is not present in the given collection;

It returns false if the given collection does not correspond to the collection in which the child object was added with the AddChild method;

Otherwise, it returns true if the child object is successfully removed.

1. It is not required to call this method when the component and the collections are destroyed.

ECSS-E-ST-40-07\_1630052

The IComponent IsChildInCollection method shall check if a name is registered as a child object under the component with the following arguments and behaviour:

Arguments:

“child” giving the child object name to check;

“collection” giving the collection under the component in which the child name is checked.

Behaviour:

It returns false if the given collection is not a valid collection under the IComponent object;

It returns the child IObject pointer if a child object with the given name is found in the given collection;

Otherwise, it returns nullptr if no such child object is found.

#### Model (IModel)

ECSS-E-ST-40-07\_1630053

All SMP Components which contain the implementation of the simulations functional behaviour shall implement the IModel interface as per IModel.h in [SMP\_FILES].

#### Service (IService)

ECSS-E-ST-40-07\_1630054

All SMP components which implement a service to be used by other SMP models shall implement the IService interface as per IService.h in [SMP\_FILES].

1. This includes both standard services specified in this standard and user defined services.

ECSS-E-ST-40-07\_1630055

All SMP components which implement the IService interface shall ensure their state is fully persisted in a simulation state and restored on Restore.

#### Linking Component (ILinkingComponent)

ECSS-E-ST-40-07\_1630056

All SMP Components which require dynamic removal of links at runtime shall implement the ILinkingComponent interface as per ILinkingComponent.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630057

The ILinkingComponent RemoveLinks method shall remove all links to the passed component stored in the LinkingComponent itself, taking the following argument:

“target” giving the reference to the linked component.

1. The result of this removal is that the LinkingComponent can no longer access the target component removed.

### Aggregation

#### Aggregation interface (IAggregate)

ECSS-E-ST-40-07\_1630058

All SMP Components which are referencing other components shall implement the IAggregate interface as per IAggregate.h in [SMP\_FILES].

1. The IReference interface is the referencing mechanism used by the aggregation interface.

ECSS-E-ST-40-07\_1630059

The IAggregate GetReference method shall return the reference matching the given name, with the following argument and behaviour:

Argument:

“name” giving name identifying the reference.

Behaviour:

If no reference matching the given name is found, it returns a nullptr reference.

1. The returned IReference object has the IAggregate as its parent.

ECSS-E-ST-40-07\_1630060

The IAggregate GetReferences method shall return an ordered collection of all references, with the following behaviour:

If the aggregation does not hold any reference, it returns an empty collection;

If at least one reference is contained, it returns a collection ordered according to the order in which the references have been added to the aggregate.

1. Returned IReference objects have the IAggregate as their parent.

#### Reference Interface (IReference)

ECSS-E-ST-40-07\_1630061

All references returned by an aggregate shall implement the IReference interface as per IReference.h in [SMP\_FILES].

1. A reference is a named object.

ECSS-E-ST-40-07\_1630062

The IReference GetComponent method shall return a reference to the component matching the given name with the following argument and behaviour:

Argument:

“name” giving the name of the referenced component to be returned.

Behaviour:

If no component matching the given name argument is found, it returns a nullptr reference;

If multiple components matching the given name argument are found, it returns one of the references.

1. Multiple components with the same name, but with a different parent (and hence path) can end up in a single reference. In this case, retrieving a component by name is not safe, as any of the components that match the name can be returned.

ECSS-E-ST-40-07\_1630063

The IReference GetComponents method shall return an ordered collection of all the referenced components with the following behaviour:

If no component is referenced, it returns an empty collection;

If at least one component is contained, it returns a collection ordered according to the order in which the components have been added using the AddComponent method.

ECSS-E-ST-40-07\_1630064

The IReference AddComponent method shall add a component to the collection of referenced components, with the following argument and behaviour:

Argument:

“component” giving a reference to the component to be added.

Behaviour:

If the maximum supported number of referenced components is reached, it throws a ReferenceFull exception as per ReferenceFull.h in [SMP\_FILES];

If the reference interface implementation is expecting the given component to inherit from another type it throws an InvalidObjectType exception as per InvalidObjectType.h in [SMP\_FILES].

1. A (typed) reference can attempt to type-cast a component to a specific type, to ensure that all components within the reference inherit from this common base type.

ECSS-E-ST-40-07\_1630065

The IReference RemoveComponent method shall remove a component from the collection of referenced components, with the following argument and behaviour:

Argument:

“component” giving a reference to the component to be removed.

Behaviour:

If the minimum number of component(s) referenced by this object is reached, it throws a CannotRemove exception as per CannotRemove.h in [SMP\_FILES];

If the component to remove is not referenced, it throws a NotReferenced exception as per NotReferenced.h in [SMP\_FILES].

1. RemoveComponent ensures that the right component is identified also if several components with the same name exist in the reference, as it takes a reference to the component as argument, and not the name.

ECSS-E-ST-40-07\_1630066

The IReference GetCount method shall return the number of components in the collection of referenced components.

ECSS-E-ST-40-07\_1630067

The IReference GetUpper method shall return the upper limit, with the following behaviour:

If a maximum number has been defined, it returns the maximum number;

If no maximum number has been defined, it returns -1.

1. The usage of -1 is consistent with the use of upper bounds in UML, where a value of -1 represents no limit (typically shown as \*)

ECSS-E-ST-40-07\_1630068

The IReference GetLower method shall return the minimum number of components in the collection or 0 when not defined.

1. The lower bound can be used to validate a model hierarchy. If a collection specifies a Lower value above its current Count, then it is not properly configured. An external component can use this information to validate the configuration before executing it.

### Composition

#### Composition interface (IComposite)

ECSS-E-ST-40-07\_1630069

All SMP Objects which contain Components shall implement the IComposite interface as per IComposite.h in [SMP\_FILES].

* 1. 1 The IContainer interface (see 5.2.5.1c.2) is the component container used by the composition interface.
  2. 2 Composition is the counter part of the IObject GetParent() method and allows traversing the tree of components from parent to child components.

ECSS-E-ST-40-07\_1630070

The IComposite GetContainer method shall return the container matching the given name with the following argument and behaviour:

Argument:

“name” giving the name of the container to be returned.

Behaviour:

If no container matching the given argument name is found, it returns a nullptr reference.

1. The returned IContainer object has the IComposite as its parent.

ECSS-E-ST-40-07\_1630071

The IComposite GetContainers method shall return an ordered collection of all the containers with the following behaviour:

If the composite does not hold any container, it returns an empty collection;

If at least one container is contained, it returns a collection ordered according to the order in which the containers have been added to the composite.

1. Returned IContainer objects have the IComposite as their parent.

#### Container interface (IContainer)

ECSS-E-ST-40-07\_1630072

All SMP Objects which represent a composition of child Components shall implement the IContainer interface as per IContainer.h in [SMP\_FILES].

* 1. 1 The container components life-cycle coincides with its parent one.
  2. 2 The container is a named Object as per 5.2.1.
  3. 3 The container allows adding children to a parent object.
  4. 4 Each container holds objects of only one type.

ECSS-E-ST-40-07\_1630073

The IContainer GetComponent method shall return the component matching the given name, with the following argument and behaviour:

Argument:

“name” giving the name of the component to be returned.

Behaviour:

If no component matching the given name is found, it returns nullptr.

1. As the container does not support component name duplication, it is not possible to get naming conflict when performing query.

ECSS-E-ST-40-07\_1630074

The IContainer GetComponents method shall return an ordered collection of all the contained components with the following behaviour:

If no component is contained, it returns an empty collection;

If at least one component is contained, it returns a collection ordered according to the order in which the components have been added using the AddComponent method.

ECSS-E-ST-40-07\_1630075

The IContainer AddComponent method shall add a component to the collection of contained components, with the following argument and behaviour:

Argument:

“component” giving the component to be added.

Behaviour:

If the maximum supported number of components is reached, it throws a ContainerFull exception as per ContainerFull.h in [SMP\_FILES];

If a component with the same name and parent already exists, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES];

If the parent of the component to be added is not the composite that holds the Container, it throws an InvalidParent exception as per InvalidParent.h in [SMP\_FILES];

If the container interface implementation is expecting the given component to inherit from another type, it throws an InvalidObjectType exception as per InvalidObjectType.h in [SMP\_FILES].

1. A (typed) container can attempt to type-cast a component to a specific type, to ensure that all components within the container inherit from this common base type.

ECSS-E-ST-40-07\_1630076

The IContainer GetCount method shall return the number of components contained in the collection.

ECSS-E-ST-40-07\_1630077

The IContainer GetUpper method shall return the maximum number of components in the collection, with the following behaviour:

If the maximum number of elements for the collection has been defined, it returns the maximum number;

If the maximum number of elements for the collection has not been defined, it returns -1.

1. The usage of -1 is consistent with the use of upper bounds in UML, where a value of -1 represents no limit (typically shown as \*).

ECSS-E-ST-40-07\_1630078

The IContainer GetLower method shall return the minimum number of components in the collection or 0 when not defined.

1. The lower bound can be used to validate a model hierarchy. If a collection specifies a Lower value above its current Count, then it is not properly configured. An external component can use this information to validate the configuration before executing it.

ECSS-E-ST-40-07\_1630079

The IContainer DeleteComponent method shall delete a component from the collection of contained components, with the following argument and behaviour:

Argument:

"component" giving a reference to the component to be deleted.

Behaviour:

If the minimum number of component(s) contained by this object is reached, it throws a CannotDelete expection as per CannotDelete.h in [SMP\_FILES];

If the component to delete is not contained, it throws a NotContained exception as per NotContained.h in [SMP\_FILES];

If the component to delete is included, and the minimum number is not reached, then the component is removed from the collection, its Disconnect method is called and finally its destructor is called.

### Events

#### Sink of events interface (IEventSink)

ECSS-E-ST-40-07\_1630080

All SMP Objects which receive event notifications shall implement the IEventSink interface as per IEventSink.h in [SMP\_FILES].

1. The specification of event sinks ensures that notifications from the event sources they are subscribed to can be managed.

ECSS-E-ST-40-07\_1630081

The IEventSink GetEventArgType method shall provide the primitive type kind of the argument expected by the event sink when it is notified about a given event, with the following behaviour:

If no argument is expected, it returns PTK\_None.

* 1. 1 See 5.2.6.1c for the specification of how event sinks are notified.
  2. 2 This operation allows for type checking when subscribing (see 5.2.6.2b) event sinks to event sources.

ECSS-E-ST-40-07\_1630082

The IEventSink Notify method shall inform the object about the event, with the following arguments:

“sender” giving the reference to the event source calling the method;

“arg” giving context data together with the event notification.

1. See 5.2.6.2d for the specification of how event sources call this method.

#### Source of events interface (IEventSource)

ECSS-E-ST-40-07\_1630083

All SMP Objects which represent the source of event notifications shall implement the IEventSource interface as per IEventSource.h in [SMP\_FILES].

1. The specification of event sources ensures that event sinks (see 5.2.6.1) that wish to receive their notifications can subscribe to them.

ECSS-E-ST-40-07\_1630084

The IEventSource Subscribe method shall add the given event sink to the list of subscribed event sinks, with the following argument and behaviour:

Argument:

“eventSink” giving the reference to the event.

Behaviour:

If the given event sink is already subscribed to the event source, it throws an EventSinkAlreadySubscribed exception as per EventSinkAlreadySubscribed.h in [SMP\_FILES];

If the primitive type kind of the argument expected by the event sink is not semantically equivalent to the one of the event source as per Table 5‑4, it throws an InvalidEventSink exception as per InvalidEventSink.h in [SMP\_FILES].

1. Any event sink can only be subscribed once to each event source.

ECSS-E-ST-40-07\_1630085

The IEventSource Unsubscribe method shall remove the given event sink from the list of subscribed event sinks, with the following argument and behaviour:

Argument:

“eventSink” giving the event to be unsubscribed.

Behaviour:

If the given event sink is not subscribed to the event source, it throws an EventSinkNotSubscribed exception as per EventSinkNotSubscribed.h in [SMP\_FILES].

1. Any event sink can only be unsubscribed if it has been subscribed before.

ECSS-E-ST-40-07\_1630086

When the event source emits the event, it shall call the Notify method of all the subscribed event sinks in the same order as the sinks have been subscribed.

1. See 5.2.6.1 for specification of the event sinks interface.

ECSS-E-ST-40-07\_1630087

The IEventSource GetEventArgType method shall return the primitive type kind of the argument transmitted by the event source when it is emitting, with the following behaviour:

If no argument is transmitted, it returns PTK\_None.

* 1. 1 See 5.2.6.2d for the specification of how event sources emit.
  2. 2 This operation allows for type checking when subscribing (see 5.2.6.2b) event sinks to event sources.

ECSS-E-ST-40-07\_1630088

The IEventSource GetEventSinks method shall return an ordered collection of all the subscribed event sinks with the following behaviour:

If there is no subscribed event sink, it returns an empty collection;

If at least one event sink has subscribed, it returns a collection ordered according to the order in which the events have subscribed using the Subscribe method.

#### Consumer of events interface (IEventConsumer)

ECSS-E-ST-40-07\_1630089

All SMP Components which hold event sinks and want to allow external access to them shall implement the IEventConsumer interface as per IEventConsumer.h in [SMP\_FILES].

1. The publication of event sinks ensures that they can subscribe to other components’ event sources.

ECSS-E-ST-40-07\_1630090

The IEventConsumer GetEventSinks method shall return a collection of all the contained event sinks, with the following behaviour:

If no event sink is contained, it returns an empty collection;

If at least one Event Sink is contained in the collection, it returns a collection ordered according to the order in which the Event Sinks have been created in the owning component.

ECSS-E-ST-40-07\_1630091

The IEventConsumer GetEventSink method shall return the component’s event sink corresponding to the given name, with the following argument and behaviour:

Argument:

“name” giving the name of the Event Sink.

Behaviour:

If no event sink with the given name exists, it returns nullptr;

If an event sink with the given name exists, it returns the corresponding IEventSink object.

#### Provider of events interface (IEventProvider)

ECSS-E-ST-40-07\_1630092

All SMP Components which hold event sources and want to allow external access to them shall implement the IEventProvider interface as per IEventProvider.h in [SMP\_FILES].

1. The publication of event sources ensures that other component’s event sinks can subscribe to them.

ECSS-E-ST-40-07\_1630093

The IEventProvider GetEventSources method shall return a collection of all the contained event sources, with the following behaviour:

If no event source is contained, it returns an empty collection;

If at least one Event Source is contained in the collection, it returns a collection ordered according to the order in which the Event Sources have been created in the owning component.

ECSS-E-ST-40-07\_1630094

The IEventProvider GetEventSource method shall return the component’s event source corresponding to the given name, with the following argument and behaviour:

Argument:

“name” giving the name of event source to be returned

Behaviour:

If no event source with the given name exists, it returns nullptr;

If an event source with the given name exists, it returns the corresponding IEventSource object.

### Entry points

#### Entry points calling interface (IEntryPoint)

ECSS-E-ST-40-07\_1630095

All SMP Objects which represent a schedulable entry point shall implement the IEntryPoint interface as per IEntryPoint.h in [SMP\_FILES].

1. The specification of entry points ensures that the scheduler or the event manager can trigger them when the relevant events are emitted.

ECSS-E-ST-40-07\_1630096

The IEntryPoint Execute method shall be called when the triggering event is emitted.

#### Entry Points publisher interface (IEntryPointPublisher)

ECSS-E-ST-40-07\_1630097

All SMP components which hold entry points and want to allow external access to them shall implement the IEntryPointPublisher interface as per IEntryPointPublisher.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630098

The IEntryPointPublisher GetEntryPoints method shall return a collection of all the contained entry points, with the following behaviour:

If no entry point is contained, it returns an empty collection;

If at least one Entry Point is contained in the collection, it returns a collection ordered according to the order in which the Entry Points have been created in the owning component.

ECSS-E-ST-40-07\_1630099

The IEntryPointPublisher GetEntryPoint method shall return the component’s entry point corresponding to the given name, with the following argument and behaviour:

Argument:

“name” giving the name of the EntryPoint to be returned.

Behaviour:

If no entry point with the given name exists, it returns nullptr;

If an entry point with the given name exists, it returns the corresponding IEntryPoint object.

1. The “name” always identifies a unique EntryPoint, as a component cannot have several EntryPoints with same name.

### Dynamic Invocation

#### Dynamic invocation interface (IDynamicInvocation)

ECSS-E-ST-40-07\_1630100

All SMP Components which allow the simulation environment to invoke operations, property getters or property setters on them shall implement the IDynamicInvocation interface as per IDynamicInvocation.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630101

All operations and properties of simulation components callable through dynamic invocation shall be registered by the component using the IPublication interface.

1. See 5.2.12.2d for specification of the IPublication PublishOperation method to be used. Parameters of operations need to be of types registered in the type registry, which excludes operations with parameters of other types from dynamic invocation.

ECSS-E-ST-40-07\_1630102

The IDynamicInvocation Invoke method shall invoke the method referenced, with the following argument and behaviour:

Argument:

“request” giving the identification of the callable method, as a fully populated request object implementing IRequest (see 5.2.8.2).

Behaviour:

If the method specified by the request parameter is not callable through dynamic invocation, it throws an InvalidOperationName exception as per InvalidOperationName.h in [SMP\_FILES];

If the number of arguments specified by the request object does not match the number of parameters of the callable method, it throws an InvalidParameterCount exception as per InvalidParameterCount.h in [SMP\_FILES];

If the types of the arguments specified by the request object do not match the types of parameters of the callable method, it throws an InvalidParameterValue exception as per InvalidParameterValue.h in [SMP\_FILES];

If called with a valid request object, it calls the method identified in the request, passing the parameters provided in the request which are of parameter direction In or InOut;

After invoking the request, it stores the parameter values of parameters with parameter direction InOut, Out or Return into the requests object.

* 1. 1 The term “method” can refer either to an operation or a property getter or a property setter.
  2. 2 The Invoke operation is a void method as the result of the invocation is stored in the IRequest object (see 5.2.8.2).

ECSS-E-ST-40-07\_1630103

The IDynamicInvocation GetProperties method shall return a collection of the invokable properties of the component as per PropertyCollection in PropertyCollection.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630104

The IDynamicInvocation GetOperations method shall return a collection of the invokable operations of the component as per OperationCollection in OperationCollection.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630105

The IDynamicInvocation GetOperation method shall return the Operation object with the following arguments and behaviour:

Arguments:

“name” giving the Operation name to get.

Behaviour:

If the Operation with the given name argument does not exist, it returns nullptr;

If the Operation with the given name argument exists, it returns the corresponding IOperation object.

ECSS-E-ST-40-07\_1630106

The IDynamicInvocation GetProperty method shall return the Property object with the following arguments and behaviour:

Arguments:

“name” giving the Property name to get.

Behaviour:

If the Property with the given name argument does not exist, it returns nullptr;

If the Property with the given name argument exists, it returns the corresponding IProperty object.

#### IRequest

ECSS-E-ST-40-07\_1630107

All SMP Request objects which are used in dynamic invocation shall implement the IRequest interface as per IRequest.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630108

The IRequest GetName method shall return the name of the callable operation if GetType return RT\_Invoke or the property name if GetType returns RT\_Get or RT\_Set.

1. For an Operation, requests are usually created by calling the IOperation CreateRequest method (see 5.2.14.1f) so the name returned is the Operation name. For a Property, the name returned is always the Property name.

ECSS-E-ST-40-07\_1630109

The IRequest GetParameterCount method shall return the number of parameters of the request object.

1. This operation only considers parameters of direction in, out or in/out, but not of type return.

ECSS-E-ST-40-07\_1630110

The IRequest GetParameterIndex method shall return the index of a specified parameter, with the following argument and behaviour:

Argument:

“name” giving the name of the parameter for which the index is returned.

Behaviour:

If the name corresponds to the name of a parameter in the parameter collection, it returns the 0-based index of the parameter in this collection;

If no parameter with the given name exists, it returns -1.

1. This operation only considers parameters of direction in, out or in/out, but not of type return.

ECSS-E-ST-40-07\_1630111

The IRequest SetParameterValue method shall store the value for a parameter, with the following arguments and behaviour:

Arguments:

“index” giving the location of the parameter to be set;

“value” giving the new value of the parameter.

Behaviour:

If the index is less than zero, it throws an InvalidParameterIndex exception as per InvalidParameterIndex.h in [SMP\_FILES];

If the index is greater than or equal to the number of parameters of the request object, it throws an InvalidParameterIndex exception as per InvalidParameterIndex.h in [SMP\_FILES];

If the type of the given value is different than the type of the parameter at the given index, it throws an InvalidParameterValue exception as per InvalidParameterValue.h in [SMP\_FILES];

If both index and value are valid, it stores the new value into the parameter with the given index, so that its new value can be returned with future calls to GetParameterValue.

1. This operation only considers parameters of direction in, out or in/out, but not of type return.

ECSS-E-ST-40-07\_1630112

The IRequest GetParameterValue method shall return the value stored at the given index in the parameters collection, with the following argument and behaviour:

Argument:

“index” of the parameter for which the value is returned.

Behaviour:

If the given index is less than zero, it throws an InvalidParameterIndex exception as per InvalidParameterIndex.h in [SMP\_FILES];

If the index is greater than or equal to the number of parameters of the request object, it throws an InvalidParameterIndex exception as per InvalidParameterIndex.h in [SMP\_FILES];

If the index is valid, it returns the current value of the parameter.

* 1. 1 The current value is either the initial value from creation of the request object, or the value provided to the last successful call of the SetParameterValue method for the same index.
  2. 2 This operation only considers parameters of direction in, out or in/out, but not of type return.

ECSS-E-ST-40-07\_1630113

The IRequest SetReturnValue method shall allow to set a return value in the request with the following argument and behaviour:

Argument:

“value” giving the new value to be set for the return parameter.

Behaviour:

If the operation does not return a value, it throws a VoidOperation exception as per VoidOperation.h in [SMP\_FILES];

If the type of the provided value does not match the type of the return value of the operation, it throws an InvalidParameterValue exception as per InvalidParameterValue.h in [SMP\_FILES];

If the operation does return a value of the given type, the return value is stored into the request object, so that it can be retrieved with later calls to GetReturnValue.

ECSS-E-ST-40-07\_1630114

The IRequest GetReturnValue method shall return the return value of the callable operation in the request, with the following behaviour:

If the operation does not return a value, it throws a VoidOperation exception as per VoidOperation.h in [SMP\_FILES];

If the operation does return a value, it returns the current value of the return parameter.

1. The current value is either the initial value from creation of the request object, or the value provided to the last successful SetReturnValue call.

ECSS-E-ST-40-07\_1630115

The IRequest GetType method shall return the type of the request object as per RequestType.h in [SMP\_FILES], specified in Table 5‑3.

ECSS-E-ST-40-07\_1630116

Table 5‑3: Request Type

| Name | Description |
| --- | --- |
| RT\_Invoke | Request represents an Operation. |
| RT\_Get | Request represents a Property getter. |
| RT\_Set | Request represents a Property setter. |

### Persistence (IPersist)

ECSS-E-ST-40-07\_1630117

All SMP Objects which need self-persistence of data shall implement the IPersist interface as per IPersist.h in [SMP\_FILES].

1. Self-persistence is an optional interface as external persistence by the simulation environment is sufficient for most components.

ECSS-E-ST-40-07\_1630118

All Simulation objects which implement self-persistence shall read from the IStorageReader interface exactly the same amount of data and in the same order as it writes it to the IStorageWriter interface.

ECSS-E-ST-40-07\_1630119

The IPersist Restore method shall read persisted data from storage through the IStorageReader interface with the following argument and behaviour:

Argument:

“reader” giving a pointer to an IStorageReader interface where data can be read from.

Behaviour:

The operation restores exactly the same amount of data from the reader that was stored by the writer on Store;

If the operation cannot restore the data, it throws a CannotRestore exception as per CannotRestore.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630120

The IPersist Store method shall write persisted data to the storage through the IStorageWriter interface with the following argument and behaviour:

Argument:

“writer” giving a pointer to an IStorageWriter interface where data can be written to.

Behaviour:

The operation stores exactly the amount of data to the writer than what it restores from a reader on Restore;

If the operation cannot store the data, it throws a CannotStore exception as per CannotStore.h in [SMP\_FILES].

### Failures

#### Failure interface (IFailure)

ECSS-E-ST-40-07\_1630121

All SMP Objects which represent a failure shall implement the IFailure interface as per IFailure.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630122

The IFailure Fail method shall set the state of the failure to “failed”.

ECSS-E-ST-40-07\_1630123

The IFailure Unfail method shall set the state of the failure to “not failed”.

ECSS-E-ST-40-07\_1630124

The IFailure IsFailed method shall return the failure state of the failure with the following behaviour:

If the state is “failed”, it returns true;

If the state is not “failed”, it returns false.

#### Model failure state interface (IFallibleModel)

ECSS-E-ST-40-07\_1630125

All Simulation models which can be failed through a list of possible failures shall implement the IFallibleModel interface as per IFallibleModel.h in [SMP\_FILES].

* 1. 1 This is an optional interface.
  2. 2 The simulation environment does not automatically persist the state of each failure, as it is the responsibility of the models to store the failure state in persisted data.

ECSS-E-ST-40-07\_1630126

The IFallibleModel GetFailures method shall return the list of possible failures for this simulation model.

ECSS-E-ST-40-07\_1630127

The IFallibleModel GetFailure method shall return a failure instance from the list of possible failures, with the following argument and behaviour:

Argument:

“name” giving the name of the failure.

Behaviour:

If none of the failures in the list of possible failures matches the given name, it returns nullptr;

If a failure matching the given name exists, it returns the pointer to the IFailure instance.

ECSS-E-ST-40-07\_1630128

The IFallibleModel IsFailed method shall return the failure state of the model, with the following behaviour:

If at least one of the failures returns true for its IFailure::IsFailed among the list of possible failures for this simulation model, it returns true;

If none of the failures returns true for its IFailure::IsFailed among the list of possible failures for this simulation model, it returns false.

### Fields

#### ISimpleField

ECSS-E-ST-40-07\_1630129

All SMP Fields of simple type shall implement the ISimpleField interface as per ISimpleField.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630130

The ISimpleField GetValue method shall return the field value stored in an AnySimple as per AnySimple.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630131

The ISimpleField SetValue method shall store the value in the field with the following argument and behaviour:

Argument:

“value” giving the new value to the field as an AnySimple as per AnySimple.h in [SMP\_FILES].

Behaviour:

If the given value simple type kind does not match the simple type kind of the field, then it throws the InvalidFieldValue exception as per InvalidFieldValue.h in [SMP\_FILES];

If the given value simple type kind does match the simple type kind of the field, then it changes the field value to the given value.

ECSS-E-ST-40-07\_1630132

The ISimpleField GetPrimitiveTypeKind method shall return the primitive type kind of the field’s type as per 5.3.10.2b.

#### IStructureField

ECSS-E-ST-40-07\_1630133

All SMP Fields which represent a structured data shall implement the IStructureField interface as per IStructureField.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630134

The IStructureField GetField method shall return the field as an IField, with the following argument and behaviour:

Argument:

“name” given the field name for which the IField interface is returned.

Behaviour:

If the field name is unknown to the structure, it returns nullptr;

Otherwise, it returns the corresponding IField object.

ECSS-E-ST-40-07\_1630135

The IStructureField GetFields method shall return the list of fields of the structure as per FieldCollection in FieldCollection.h in [SMP\_FILES].

#### IArrayField

ECSS-E-ST-40-07\_1630136

All SMP fields which represent an array where each array item is to be retrieved individually as a Field shall implement the IArrayField interface as per IArrayField.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630137

The IArrayField GetItem method shall return the array item as an IField as per IField.h in [SMP\_FILES] with the following argument and behaviour:

Argument:

“index” giving the location of the item for which the IField pointer is returned.

Behaviour:

If the given index is outside the array size, it returns nullptr;

Otherwise, it returns the array item at the given index as an IField object.

ECSS-E-ST-40-07\_1630138

The IArrayField GetSize method shall return the number of array items.

#### ISimpleArrayField

ECSS-E-ST-40-07\_1630139

All SMP fields which represent an array of simple type items where individual array items are not to be retrieved as Field shall implement the ISimpleArrayField interface as per ISimpleArrayField.h in [SMP\_FILES].

1. This enables an efficient implementation especially of large arrays as a single object, rather than having each array item represented by an individual object. The implications are that such array items cannot be retrieved as Object or Field, e.g. via GetField(), and are hence not available in operations that require individual objects or fields.

ECSS-E-ST-40-07\_1630140

The ISimpleArrayField GetSize method shall return the number of array items.

ECSS-E-ST-40-07\_1630141

The ISimpleArrayField GetValue method shall return the corresponding array item value stored in an AnySimple as per AnySimple.h in [SMP\_FILES] with the following argument and behaviour:

Argument:

“index” giving the location of the item for which the value is returned.

Behaviour:

If the given index is outside the array size, it throws an InvalidArrayIndex as per InvalidArrayIndex.h in [SMP\_FILES];

Otherwise, it returns the item value corresponding to the given index as an AnySimple.

ECSS-E-ST-40-07\_1630142

The ISimpleArrayField SetValue method shall set the corresponding array item value stored with the following arguments and behaviour:

Arguments:

“index” giving the location of the item for which the value is set;

“value” giving the new value for the array item.

Behaviour:

If the given index is outside the array size, it throws an InvalidArrayIndex as per InvalidArrayIndex.h in [SMP\_FILES];

If the given value simple type kind does not match the simple type kind of the corresponding array item, then it throws an InvalidFieldValue as per InvalidFieldValue.h in [SMP\_FILES];

If the given value simple type kind does match the simple type kind of the corresponding array item, then it stores the given AnySimple value into the item value corresponding to the given index.

ECSS-E-ST-40-07\_1630143

The ISimpleArrayField GetValues method shall return all the array item values stored in an AnySimpleArray as per AnySimpleArray.h in [SMP\_FILES] with the following arguments and behaviour:

Arguments:

“length” giving the length of the return array for values;

“values” giving an array of allocated storage for which the return values are put;

“startIndex” giving the 0-based start index in the array from which values are returned.

Behaviour:

If the given value array size does not match the ArrayField size, it throws an InvalidArraySize as per InvalidArraySize.h in [SMP\_FILES];

Otherwise, it copies the range of item values, given by the startIndex and length arguments, into the given AnySimpleArray.

ECSS-E-ST-40-07\_1630144

The ISimpleArrayField SetValues method shall allow setting all values of an array with the following arguments and behaviour:

Arguments:

“length” giving the length of the array with values to be set;

“values” giving an array of values to be set in the array;

“startIndex” giving the 0-based start index in the array from which values are set.

Behaviour:

If the given length does not match the ArrayField length, it throws a InvalidArraySize as per InvalidArraySize.h in [SMP\_FILES];

If any of the given values simple type kind does not match the array item simple type kind, then it throws an InvalidArrayValue as per InvalidArrayValue.h in [SMP\_FILES];

If any of the given values simple type kind does match the array item simple type kind, then it stores the given values into the corresponding array item values, considering the range given by the startIndex and length arguments.

#### IField

ECSS-E-ST-40-07\_1630145

All SMP fields shall implement the IField interface as per IField.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630146

The IField GetView method shall return the View Kind for the field.

1. See Table 4‑2 for specification of View Kind.

ECSS-E-ST-40-07\_1630147

The IField IsState method shall return true if the field State property is true, false otherwise.

ECSS-E-ST-40-07\_1630148

The IField IsInput method shall return true if the field is an Input field, false otherwise.

ECSS-E-ST-40-07\_1630149

The IField IsOutput method shall return true if the field is an Output field, false otherwise.

ECSS-E-ST-40-07\_1630150

The IField GetType method shall return the associated field type or nullptr if the field has not been published or has not been successfully published to the Simulation Environment.

#### IForcibleField

ECSS-E-ST-40-07\_1630151

All SMP simple fields which allow forcing of the field value shall implement the IForcibleField interface as per IForcibleField.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630152

The IForcibleField Force method shall force the field value so that it does not change until Unforce is called with the following argument and behaviour:

Argument:

“value” giving the forced value to be returned by GetValue until Unforce is called.

Behaviour:

If the given value simple kind does not match the field simple type kind, then it throws an InvalidFieldValue as per InvalidFieldValue.h in [SMP\_FILES];

If the given value simple kind does match the field simple type kind, then it stores the given value as the value to return by GetValue.

1. The handling of the forced field value within a model is not specified in this standard.

ECSS-E-ST-40-07\_1630153

The IForcibleField Unforce method shall remove the forcing or freezing condition on the field so that GetValue called on the field returns the current field value.

1. The handling of the forced field value within a model is undefined.

ECSS-E-ST-40-07\_1630154

The IForcibleField Freeze method shall force the field to its current field value so that it no longer changes until Unforce is called.

ECSS-E-ST-40-07\_1630155

The IForcibleField IsForced method shall return true if field is forced or freezed, otherwise it returns false.

#### IOutputField

ECSS-E-ST-40-07\_1630156

All SMP output fields that support pushing their values to connected fields shall implement the IOutputField interface as per IOutputField.h in [SMP\_FILES].

1. Dataflow connections are allowed for primitive and simple type fields, which can include array items, sub-fields of complex type fields, as well as for complex type fields, which include arrays, structures and classes.

ECSS-E-ST-40-07\_1630157

The IOutputField Connect method shall connect the field to an input field to create a dataflow connection between the two fields giving the following argument and behaviour:

Argument:

“target” giving the input field this output data flow field is connected to.

Behaviour:

If the target is already connected to this output field, it throws a FieldAlreadyConnected exception as per FieldAlreadyConnected.h in [SMP\_FILES];

If Connect is called several times for an output field, it connects the output field to a list of input fields allowing the same output to push values to several input fields;

If the input and output field have the same type UUID, then the connection is considered to be strict compatible and it connects successfully;

If the input and output field are of semantically equivalent types as per Table 5‑4, then the connection is considered to be of equivalent types and it connects successfully;

If the input and output are of non-equivalent or non-strict compatible types, it throws an InvalidTarget exception as per InvalidTarget.h in [SMP\_FILES];

If connection is successful, it invokes the Push method immediately, triggering an update of the connected input field with the current value of the output field.

* 1. 1 to item (c) and (d): The specification of semantically equivalent type ensures that no information can be lost in transfer of data from output to input.
  2. 2 The input field is a passive part of the transfer since the output is pushing the values to the input.
  3. 3 The input field can be connected to several output fields.
  4. 4 to item (f): The call of the Push allows to synchronise the Input value with the Output value immediately after the connection is established.
  5. 5 For arrays and structs, each array and struct element can implement IOutputField. In this case, each element can be connected with its own Connect call.
  6. 6 The target field, that plays the role of the “input” in the data flow connection, can have any combination of Input and Output attributes because Push supports setting the value for any target field.

ECSS-E-ST-40-07\_1630158

The IOutputField Push method shall push the field value to all connected input fields.

1. This is also called propagation of the value to all the connected consumer models.

ECSS-E-ST-40-07\_1630159

Table 5‑4: Semantically equivalent types for connections

| Type | Semantically equivalent types |
| --- | --- |
| Char8 | Char8 |
| String | String of same length |
| Bool | Bool |
| Signed integers | Signed integer with same size |
| Unsigned integers | Unsigned integer with same size |
| Float | Float with same size |
| Array | Array with same length and each element are of semantically equivalent types. |
| Struct | Struct with:   * identical number of elements * same order of elements * each element is of semantically equivalent types |
| Duration | Duration  Signed 64-bits integer with the same semantics |
| DateTime | DateTime  Signed 64-bits integer with the same semantics |
| Enumeration | Same enumeration type definition |

ECSS-E-ST-40-07\_1630160

The IOutputField Disconnect method shall disconnect the field from a connected input field giving the following argument and behaviour:

Argument:

“target” giving the input field this output data flow field is to be disconnected from.

Behaviour:

If the target is not connected to this output field, it throws a FieldNotConnected exception as per FieldNotConnected.h in [SMP\_FILES];

If the target is connected to this output, the disconnection is successful;

If Disconnect is called several times for an output field, it disconnects the output field from the list of input fields.

ECSS-E-ST-40-07\_1630161

The IOutputField IsAutomatic method shall return true if the output field is capable to push its value upon change automatically to connected fields.

ECSS-E-ST-40-07\_1630162

The IOutputField IsAutomatic method shall return false if pushing its value to connected fields is performed by the Simulation Environment.

1. Usually, push is called during the execution of a simulation event. Hence, this corresponds to a scheduled field propagation.

ECSS-E-ST-40-07\_1630163

If the IsAutomatic method returns true, upon the output field value change, the output field shall call automatically the IOutputField Push method.

* 1. 1 Calling Push from outside of the field, e.g. by the Simulation Environment, is possible to perform manually the value propagation from the output field to the input field.
  2. 2 Since the responsibility of calling the Push operation is not delegated to the component owning the field nor to the simulation environment, the propagation happens “automatic”, hence this interaction method is called “automatic data propagation”.

ECSS-E-ST-40-07\_1630164

The IOutputField GetInputFields method shall return an ordered collection of all the connected input fields with the following behaviour:

If there is no connected input field, it returns an empty collection;

If at least one input field is connected, it returns a collection ordered according to the order in which the input fields have connected using the Connect method.

### Requirements on utilization of Simulation Environments interfaces by components

#### ILogger interface utilization

ECSS-E-ST-40-07\_1630165

The LogMessageKind type as per Services/LogMessageKind.h in [SMP\_FILES] shall be used to store the Log Message Kind as returned from the results of ILogger::QueryLogMessageKind.

ECSS-E-ST-40-07\_1630166

All SMP models and services shall use the predefined LogMessageKinds as defined in Table 5‑7 for messages of message type Information, Event, Warning, Error or Debug.

#### IPublication interface

ECSS-E-ST-40-07\_1630167

All Arrays published as a single array via the IPublication PublishArray method shall be without any padding.

1. This implies that array element with index i (0-based) is assumed to be stored at address of index 0 + i\*sizeof(primitiveType).

ECSS-E-ST-40-07\_1630168

When publishing arrays via the IPublishField PublishArray method that require each element to be published individually, the following steps shall be followed:

Call the IPublishField PublishArray method giving the following arguments:

Name of array;

Description of Array.

The PublishArray method returns a pointer to an IPublishField interface;

Use the returned IPublishField interface to publish each of the elements of the array.

1. In case of a multi-dimensional array, step 1-3 in 5.2.12.2b can be repeated iteratively.

ECSS-E-ST-40-07\_1630169

When publishing a structure via the IPublishField PublishStructure method, the following steps shall be followed:

Call the IPublishField PublishStructure method giving the following arguments:

Name of Structure;

Description of Structure.

The PublishStructure method returns a pointer to an IPublishField interface;

Use the returned IPublishField interface to publish each of the elements of the structure.

1. In case of nested structures, steps 1-3 above can be repeated iteratively.

ECSS-E-ST-40-07\_1630170

The IPublication PublishOperation method shall allow publishing an operation as per following procedure:

Call the IPublication PublishOperation method giving the following arguments:

Name of Operation;

Description of Operation;

Its view state.

The IPublication PublishOperation method returns a pointer to an IPublishOperation interface;

Use the returned IPublishOperation interface to publish each of the parameters and the return value of the operation.

1. See clause 5.3.9.2 for specification of the IPublishOperation interface.

#### ISimulator interface

ECSS-E-ST-40-07\_1630171

All user defined services shall be added to the simulation using the ISimulator AddService method.

### Properties

#### IProperty

ECSS-E-ST-40-07\_1630172

The IProperty GetAccess method shall return the property Access Kind as specified in Table 5‑5.

ECSS-E-ST-40-07\_1630173

Table 5‑5: Property Access Kind values

| Name | Intended interpretation |
| --- | --- |
| AK\_ReadWrite | Read/Write access. Both getter and setter are available for the property |
| AK\_ReadOnly | Read-Only access. Only the getter is available for the property |
| AK\_WriteOnly | Write-Only access. Only the setter is available for the property |

ECSS-E-ST-40-07\_1630174

The IProperty GetView method shall return the View Kind for the property.

1. See Table 4‑2 for specification of View Kind.

ECSS-E-ST-40-07\_1630175

The IProperty GetValue method shall return the value of a property as per the following behaviour:

If the property access type is Write-Only, it throws the InvalidAccess exception;

If the property type is not a simple type, it returns an AnySimple object as per AnySimple.h in [SMP\_FILES] where the type is set to PTK\_None;

If the property type is a simple type, it returns the corresponding AnySimple object.

1. to item 2: See PrimitiveTypes.h in [SMP\_FILES] for the definition of PTK\_None.

ECSS-E-ST-40-07\_1630176

The IProperty SetValue method shall set the value of a property as per the following behaviour:

If the property access type is Read-Only, it throws the InvalidAccess exception;

If the property type is not a simple type or if the property type is a simple type and if the given value simple type kind does not match the simple type kind of the property, then it throws the InvalidPropertyValue exception as per InvalidPropertyValue.h in [SMP\_FILES];

If all checks above are successful, it sets the property to the corresponding AnySimple object.

1. to item 2: See PrimitiveTypes.h in [SMP\_FILES] for the definition of PTK\_None.

ECSS-E-ST-40-07\_1630177

The IProperty GetPrimitiveType method shall return the property equivalent primitive type if it is a simple type property or PTK\_None if it is not a simple type property.

### Operations

#### IOperation

ECSS-E-ST-40-07\_1630178

All SMP operations shall implement the IOperation interface as per IOperation.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630179

The IOperation GetParameters method shall return the operation collection of IParameter objects, that excludes the return parameter and that is ordered identically to the operation signature.

ECSS-E-ST-40-07\_1630180

The IOperation GetParameter method shall return the operation Parameter that has the given name passed in the argument or nullptr if that parameter does not exist.

ECSS-E-ST-40-07\_1630181

The IOperation GetReturnParameter method shall return the return parameter for a non-void operation or nullptr for a void operation.

ECSS-E-ST-40-07\_1630182

The IOperation GetView method shall return the View Kind for the operation.

1. See Table 4‑2 for specification of View Kind.

ECSS-E-ST-40-07\_1630183

The IOperation CreateRequest method shall return the IRequest object for the operation or nullptr if the operation does not support dynamic invocation.

1. It is the responsibility of the caller of the CreateRequest method to call the DeleteRequest method when the IRequest object is not used anymore.

ECSS-E-ST-40-07\_1630184

The IOperation Invoke method shall dynamically invoke the operation described in the passed IRequest argument with the following behaviour:

It throws InvalidOperationName as per InvalidOperationName.h in [SMP\_FILES] if the operation does not exist or if the operation does not allow dynamic invocation;

It throws InvalidParameterCount as per InvalidParameterCount.h in [SMP\_FILES] if the operation is invoked with the wrong number of parameters;

It throws InvalidParameterValue as per InvalidParameterValue.h in [SMP\_FILES] if the operation is invoked with at least one wrong parameter type;

Otherwise, it calls the operation passing the given parameters in the request object.

ECSS-E-ST-40-07\_1630185

The IOperation DeleteRequest method shall delete the IRequest object created with the CreateRequest method.

#### IParameter

ECSS-E-ST-40-07\_1630186

The IParameter GetType method shall return the parameter Type or nullptr if the parameter has not been published or has not been successfully published to the Simulation Environment.

ECSS-E-ST-40-07\_1630187

The IParameter GetDirection method shall return the parameter Direction as specified in Table 5‑6.

ECSS-E-ST-40-07\_1630188

Table 5‑6: Parameter Direction Kind values

| Name | Intended interpretation |
| --- | --- |
| PDK\_In | The parameter is read-only to the operation, i.e. its value must be specified on call, and cannot be changed inside the operation. |
| PDK\_Out | The parameter is write-only to the operation, i.e. its value is unspecified on call, and must be set by the operation. |
| PDK\_InOut | The parameter value must be specified on call, and may be changed by the operation. |
| PDK\_Return | The parameter value represents the operation's return value. |

## Simulation Environment interfaces

### Logger (ILogger interface)

ECSS-E-ST-40-07\_1630189

The Simulation Environment shall provide a component implementing the ILogger interfaces as per Services/ILogger.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630190

The component implementing the ILogger interface shall maintain a list mapping the defined Log Message Kinds to names and IDs, including and possibly extending Table 5‑7.

ECSS-E-ST-40-07\_1630191

The ILogger QueryLogMessageKind method shall translate from the name of the message kind to the identifier of the message kind, with the following argument and behaviour:

Argument:

“messageKindName” giving a case sensitive string containing the name of the log message kind.

Behaviour:

If the given name matches one of the predefined LogMessageKind as specified in Table 5‑7, it returns the corresponding LogMessageKind ID as per Table 5‑7;

If the given name does not match any LogMessageKind in Table 5‑7 nor any of the log message kinds in the maintained mapping, it returns a new LogMessageKind ID as a unique identifier matching the given name;

If the given name does not match any LogMessageKind in Table 5‑7 but it matches one of the entries in the maintained mapping of log message kinds, it returns the corresponding LogMessageKind ID from the mapping.

ECSS-E-ST-40-07\_1630192

Table 5‑7: Default Log Message Kinds

| Name | ID | Description |
| --- | --- | --- |
| Debug | 4 | To be used for messages that can help during investigations of anomalous behaviours, but that regular users in nominal situations are not interested in seeing. |
| Error | 3 | To be used for error messages that the simulation or the model developer thinks are to be conveyed to the user when anomalous situations happen, that almost surely can lead to an anomalous simulation. |
| Warning | 2 | To be used for messages that the simulation or the model developer thinks are to be conveyed to the user when anomalous situations happen, that deserves users’ attention, but that non-necessarily lead to an anomalous simulation. |
| Event | 1 | To be used for log messages that the simulation or the model developer thinks are to be conveyed to the user upon certain events (the definition of ’event’ is open and simulation or model developer driven). |
| Information | 0 | The message contains general information. |

ECSS-E-ST-40-07\_1630193

The list mapping the defined log message kinds to the defined LogMessageKind IDs shall be part of persisted data and saved/restored to/from simulation states.

1. This implies that the list of log message kinds and associated names are part of the simulation state and that models can store log message kinds they need and not continuously ask which LogMessageKind corresponds to a given LogMessageKind name. This leads to more efficient implementations.

ECSS-E-ST-40-07\_1630194

The ILogger Log method shall log a message, with the following arguments:

“sender” giving the originator of the message;

“message” giving the text to be logged;

“kind” giving the registered log message kind for this message as returned from ILogger::QueryLogMessageKind method.

If the LogMessageKind ID was not previously registered by using ILogger::QueryLogMessageKind, then it registers the passed LogMessageKind with text set to the passed number, followed by the sender’s Path in the model hierarchy. It is recommended that the implementation writes a Warning message in the logbook to notify creation of a new LogMessageKind.

1. This implicit registration of a new LogMessageKind ID allows to quickly identify models in a simulation that are logging using custom unregistered LogMessageKinds.

### Time Keeper (ITimeKeeper)

ECSS-E-ST-40-07\_1630195

The simulation environment shall provide a component implementing the ITimeKeeper interface as per ITimeKeeper.h in [SMP\_FILES].

* 1. 1 The ITimeKeeper gives access to the Time Keeper Service.
  2. 2 The ITimeKeeper is used to maintain all the simulation times.

ECSS-E-ST-40-07\_1630196

The ITimeKeeper SetEpochTime method shall set the simulation Epoch Time, with the following argument and behaviour:

Argument:

“epochTime” giving the new epoch time;

Behaviour:

After setting the EpochTime, it emits a SMP\_EpochTimeChanged global SMP event.

* 1. 1 See Table 5‑8 for details on EpochTimeChanged global Event.
  2. 2 This method changes the offset between the Simulation time and the Epoch time.

ECSS-E-ST-40-07\_1630197

The ITimeKeeper SetMissionStartTime method shall set a new start time for Mission time, with the following argument and behaviour:

Argument:

“missionStart” giving the new Epoch time for which the Mission time is zero.

Behaviour:

After changing the MissionStartTime, it emits the SMP\_MissionTimeChanged global SMP Event.

1. This method changes the offset between the Epoch time and the Mission time.

ECSS-E-ST-40-07\_1630198

The ITimeKeeper SetMissionTime method shall set the Mission time, with the following argument and behaviour:

Argument:

“MissionTime” giving the new Mission time at the current Epoch time.

Behaviour:

After changing the MissionTime, it emits the SMP\_MissionTimeChanged global SMP Event.

1. This method changes the offset between the Epoch time and the Mission time.

ECSS-E-ST-40-07\_1630199

The ITimeKeeper SetSimulationTime method shall advance the Simulation time in the time frame between the call to emit a PreSimTimeChange event and the end of the call to emit a PostSimTimeChange event as per Table 5‑8, with the following argument and behaviour:

Argument:

“SimulationTime” giving the new simulation time

Behaviour:

If SetSimulationTime method is called outside a PreSimTimeChange as per Table 5‑8, then the method returns without updating the Simulation Time;

If the given simulation time is less than the current simulation time, it throws an InvalidSimulationTime as per Services/InvalidSimulationTime.h in [SMP\_FILES] and the Simulation Time is not updated;

If the new simulation time is larger than the time of the next event on the scheduler, it throws an InvalidSimulationTime as per Services/InvalidSimulationTime.h in [SMP\_FILES] and the Simulation Time is not updated;

If SetSimulationTime method is called inside the time frame between the PreSimTimeChange and PostSimTimeChange events as per Table 5‑8, then the simulation time is updated to the given simulation time.

* 1. 1 SetSimulationTime method has no effect if called outside the time frame of the PreSimTimeChange-PostSimTimeChange global events as per Table 5‑8.
  2. 2 SetSimulationTime method does not result in emissions of PreSimTimeChange and PostSimTimeChange global events as per Table 5‑8.
  3. 3 SetSimulationTime provides a direct mean for Models (thus, not part of the Simulation Environment) to set the simulation time, which is normally updated by the Scheduler. For example, this method can be used by an executing processor emulator model to synchronize its own time with the kernel simulation time.

ECSS-E-ST-40-07\_1630200

The ITimeKeeper GetSimulationTime method shall return the Simulation time.

ECSS-E-ST-40-07\_1630201

The ITimeKeeper GetEpochTime method shall return the current Epoch time.

ECSS-E-ST-40-07\_1630202

The ITimeKeeper GetMissionTime method shall return the Mission time.

ECSS-E-ST-40-07\_1630203

The TimeKeeper GetMissionStartTime method shall return the Mission Start Time.

ECSS-E-ST-40-07\_1630204

The ITimeKeeper GetZuluTime method shall return the Zulu time.

### Scheduler (IScheduler)

ECSS-E-ST-40-07\_1630205

The simulation environment shall provide a Scheduler component implementing the IScheduler interface as per Services/IScheduler.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630206

The Scheduler shall allow Events to be added to the scheduler with a repeat count with the following behaviour:

An Event with repeat=0 is non-cyclic and executes only once;

An Event with repeat=0 is removed automatically after its triggering;

An Event with repeat>0 is cyclic, and repeats ‘repeat’ times;

An Event with repeat>0 is removed automatically after it has been triggered ‘repeat+1’ times;

An Event with repeat<0 is cyclic forever;

An Event with repeat<0 is never removed from the scheduler unless explicitly requested using the RemoveEvent() method.

ECSS-E-ST-40-07\_1630207

The Scheduler shall allow to specify the cycle time between each call for cyclic Events with the following behaviour:

For non-cyclic Events, the cycle time parameter is stored, but not used;

For cyclic Events, the cycle time is a Duration;

For cyclic Simulation Time Events, an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES] is thrown if the cycle time is a value less than -1 or is 0;

For cyclic Simulation Time Events, if after the event execution the Cycle Time is -1 and repeat count is not 0, then the event is not re-posted on the timeline;

For cyclic Epoch/Mission/Zulu Time Events, an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES] is thrown if the cycle time is a value less than 1.

1. to item 1: The cycle time can become relevant if a subsequent call to SetEventRepeat is received before the Event is removed from the scheduler.

ECSS-E-ST-40-07\_1630208

Events added to the scheduler by AddSimulationTimeEvent, AddMissionTimeEvent, AddEpochTimeEvent and AddZuluTimeEvent shall be executed according to a “first posted, first executed” strategy where the posting order of Events are determined based on the order of the Add call.

1. This implies that the posting order is not affected by a change in Epoch time or Mission Time.

ECSS-E-ST-40-07\_1630209

The IScheduler AddSimulationTimeEvent method shall add an Event to the scheduler, with the following arguments and behaviour:

Arguments:

“entryPoint” giving the Entry Point to be called when the Event is executed;

“simulationTime” giving the relative time from now until the first call of the Entry Point;

“cycleTime“ giving the cycle time of the Event as specified in 5.3.3c;

“repeat“ giving the Event repetition count as specified in 5.3.3b.

Behaviour:

If the provided Simulation Time is more than MAX\_INT – ‘current simulation time’, it throws an InvalidEventTime exception as per Services/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If the provided Simulation Time is a negative value less than -1, it throws an InvalidEventTime exception as per Services/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If Repeat is not zero and CycleTime is a value less than -1 or is 0, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If the provided Simulation Time is -1, the event is created but not posted on the timeline;

After adding the new Event to the scheduler, it returns the EventId as per Services/EventId.h in [SMP\_FILES] identifying the added Event.

* 1. 1 The execution order follows the general priority rules given in requirement 5.3.3d.
  2. 2 to item (a): MAX\_INT is the maximum integer value for the type Smp::Duration.
  3. 3 to item (a): ‘Current simulation time’ is the value returned by the TimeKeeper GetSimulationTime method as specified in 5.3.2f.
  4. 4 to item (d): an event not posted on the timeline will be posted only when SetEventSimulationTime is used to define a valid execution time.

ECSS-E-ST-40-07\_1630210

The IScheduler AddMissionTimeEvent method shall add an Event to the scheduler with the following arguments and behaviour:

Arguments:

“entryPoint“ giving the Entry Point to be called when the Event is executed;

“missionTime“ giving the mission time of the first call of the Entry Point;

“cycleTime“ giving the cycle time of the Event as specified in 5.3.3c;

“repeat“ giving the Event repetition count as specified in 5.3.3b.

Behaviour:

If the Mission Time is less than the current mission time, it throws an InvalidEventTime exception as per Servives/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If Repeat is not zero and CycleTime is a value less than 1, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

After adding the new Event to the scheduler, it returns the EventId as per Services/EventId.h in [SMP\_FILES] identifying the added Event.

1. The execution order follows the general priority rules given in requirement 5.3.3d.

ECSS-E-ST-40-07\_1630211

The IScheduler AddEpochTimeEvent method shall add an Event to the scheduler, with the following arguments and behaviour:

Arguments:

“entryPoint“ giving the Entry Point to be called when the Event is executed;

“epochTime“ giving the epoch time of the first call of the Entry Point;

“cycleTime“ giving the cycle time of the Event as specified in 5.3.3c;

“repeat“ giving the Event repetition count as specified in 5.3.3b.

Behaviour:

If the Epoch Time is less than the current epoch time it throws an InvalidEventTime exception as per Services/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If Repeat is not zero and CycleTime is a value less than 1, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

After adding the new Event to the scheduler, it returns the EventId as per Services/EventId.h in [SMP\_FILES] identifying the added Event.

1. The execution order follows the general priority rules given in requirement 5.3.3d.

ECSS-E-ST-40-07\_1630212

The IScheduler AddZuluTimeEvent method shall add an Event to the scheduler, with the following arguments and behaviour:

Arguments:

“entryPoint“ giving the Entry Point to be called when the Event is executed;

“zuluTime“ giving the Zulu time of the first call of the Entry Point;

“cycleTime“ giving the cycle time of the Event as specified in 5.3.3c;

“repeat“ giving the Event repetition count as specified in 5.3.3b.

Behaviour:

If the given Zulu Time is less than the current Zulu time, it throws an InvalidEventTime exception as per Services/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If Repeat is not zero and CycleTime is a value less than 1, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

After adding the new Event to the scheduler, it returns the EventId as per Services/EventId.h in [SMP\_FILES] identifying the added Event.

1. The execution order follows the general priority rules given in requirement 5.3.3d.

ECSS-E-ST-40-07\_1630213

The IScheduler AddImmediateEvent method shall add an immediate simulation time event to the scheduler with the current simulation time as execution time returning an EventId as per Services/EventId.h in [SMP\_FILES], with the following argument and behaviour:

Argument:

“entryPoint” giving the Entry Point to be called when the Event is executed.

Behaviour:

The scheduled event is inserted at the end of the list of immediate events; the list of immediate events is processed in order of insertion and before any non-immediate event;

After adding the new Event to the scheduler, it returns the EventId identifying the added Event.

* 1. 1 Calls to AddImmediateEvent differs to calls to AddSimulationTimeEvent method with repeat=0, cycleTime=0 and simulationTime=0 since the event is scheduled at the front instead of the end of the list of scheduled events for the current simulation time.
  2. 2 It cannot be assumed that Events added via AddImmediateEvent are the next Event executed, as other Events can have been scheduled with AddImmediateEvent prior to this Event, and hence are executed first.
  3. 3 To execute an entry point immediately without going through the scheduler, the Execute() method of the EntryPoint can be called directly.

ECSS-E-ST-40-07\_1630214

The EventId returned when adding an event shall be unique throughout the entire duration of the simulation implying that EventIds cannot be reused after the Event has been executed.

1. The EventId must only be unique within the Scheduler context; the Event Manager service uses the same EventId type, but uniqueness across services is not required.

ECSS-E-ST-40-07\_1630215

The IScheduler RemoveEvent method shall remove an already scheduled Event from the Scheduler, with the following argument and behaviour:

Argument:

“event” giving the unique identifier of the Event.

Behaviour:

If the given EventId does not identify an Event currently in the Scheduler, it throws an InvalidEventId exception as per InvalidEventId.h in [SMP\_FILES];

If the EventId is identical to the current executing Event in the schedule, then it still proceeds to finish normally; however, it is not executed again, as if its repeat count changed to 0 via SetEventRepeat;

If the EventId is not identical to the current executing Event in the schedule, then the Event is simply removed from the scheduler and never executed, regardless of its remaining repetitions.

1. To item (b): setting the repeat count to 0 implies that the Event is removed from the scheduler immediately after it is executed.

ECSS-E-ST-40-07\_1630216

The IScheduler SetEventSimulationTime method shall update the Simulation time of the next execution of an Event with the following arguments and behaviour:

Arguments:

“event” giving the unique identifier of the Event;

“simulationTime” giving the relative time from now until the next execution of the Event.

Behaviour:

If the Event identified by the given EventId is not scheduled on Simulation time, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Event identified by the given EventId is an immediate event, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Simulation Time is less than -1, the Event is never executed but instead removed immediately from the scheduler;

If the Simulation Time is -1, the Event is removed from the timeline, but not removed from the scheduler;

When the Simulation time of the next execution of an Event is updated, it takes effect on all future repeats of this Event as per the remaining “repeat” count and respecting the given cycle-time between each repeat;

When called during the execution of the targeted event, the provided Simulation time is used as the time for the next execution.

1. to item (f): that means that the provided Simulation time value overrides the normal next computed value, which is ‘current simulation time + cycle time’.

ECSS-E-ST-40-07\_1630217

The IScheduler SetEventMissionTime method shall update the Mission time of the next execution of an Event with the following arguments and behaviour:

Arguments:

“event” giving the unique identifier of the Event;

“missionTime” giving the time of the next execution of the Event.

Behaviour:

If the given EventId is not currently on the scheduler, it throws an InvalidEventId exception as per InvalidEventId.h in [SMP\_FILES];

If the Event identified by the given EventId is not scheduled on Mission time, it throws an InvalidEventId exception as per InvalidEventId.h in [SMP\_FILES];

If the mission time is before the current mission time, the Event is never executed but instead removed immediately from the scheduler;

When the Mission time of the next execution of an Event is updated, it takes effect on all future repeats of this Event as per the remaining “repeat” count and respecting the given cycle-time between each repeat.

ECSS-E-ST-40-07\_1630218

The IScheduler SetEventEpochTime method shall update the Epoch time of the next execution of an Event, with the following arguments and behaviour:

Arguments:

“event” giving the unique identifier of the Event;

“epochTime” giving the time of the next execution of the Event.

Behaviour:

If the given EventId is not currently on the scheduler, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Event identified by the given EventId is not scheduled on Epoch time, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the epoch time is before the current epoch time, the Event is never executed but instead removed immediately from the scheduler;

When the Epoch time of the next execution of an Event is updated, it takes effect on all future repeats of this Event as per the remaining “repeat” count and respecting the given cycle-time between each repeat.

ECSS-E-ST-40-07\_1630219

The IScheduler SetEventZuluTime method shall update the Zulu time of the next execution of an Event, with the following arguments and behaviour:

Arguments:

“event” giving the unique identifier of the Event;

“zuluTime” giving the time of the next execution of the Event.

Behaviour:

If the given EventId is not currently on the scheduler, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Event identified by the given EventId is not scheduled on Zulu time, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Zulu time is before the current Zulu time, the Event is never executed but instead removed immediately from the scheduler;

When the Zulu time of the next execution of an Event is updated, it takes effect on all future repeats of this Event as per the remaining “repeat” count and respecting the given cycle-time between each repeat.

ECSS-E-ST-40-07\_1630220

The IScheduler SetEventCycleTime method shall allow to update the cycle time of an already scheduled Event, with the following arguments and behaviour:

Arguments:

“event” giving the unique identifier of the Event;

“cycleTime” giving the new cycle time of the Event as specified in 5.3.3c.

Behaviour:

If the given EventId is not currently on the scheduler, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the Repeat count of the Event is not zero and CycleTime is a value less than -1 or is 0, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES] and the CycleTime is not updated.

1. The CycleTime can be set also for immediate events and events with repeat count equal to 0, as the repeat can be updated with SetEventRepeat afterwards.

ECSS-E-ST-40-07\_1630221

The IScheduler SetEventRepeat method shall allow to update the repeat count of an Event already scheduled with the following arguments and behaviour:

Arguments:

“event” as a unique identifier of the Event;

“repeat” giving the number of the Event repetitions as specified in 5.3.3b.

Behaviour:

If the given EventId is not currently on the scheduler, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If the given repeat count is not zero and CycleTime of the Event is a value less than -1 or is 0, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES] and the corresponding event repeat Count is not updated;

If the given repeat count is greater than 0 and the given EventId is identical to the one currently executing, then the scheduler executes the Event for the given repeat count, excluding the current execution;

If the given repeat count is 0, the Event is removed immediately after its execution is finished.

ECSS-E-ST-40-07\_1630222

The IScheduler GetCurrentEventId method shall return an EventId as per Services/EventId.h in [SMP\_FILES], with the following behaviour:

If an Event is currently executing, it returns the EventId of the currently executing Event;

If no scheduled Event is currently executing, it returns -1.

1. A scheduled Event is not executing if GetCurrentEventId is called as part of the SMP global events (See clause 5.3.4).

ECSS-E-ST-40-07\_1630223

The IScheduler GetNextScheduledEventTime method shall return the Simulation Time of the execution of the next scheduled Simulation Time, Epoch Time or Mission Time Event.

* 1. 1 Events scheduled in Zulu Time are not considered, as these Events do not have a fixed defined Simulation Time.
  2. 2 In case of Zulu Events executed, other Events may schedule Events prior to the time returned, hence the Scheduler does not guarantee that no other Events may be executed prior to the time returned from GetNextScheduledEventTime().

ECSS-E-ST-40-07\_1630224

The complete state of the Scheduler, including Events scheduled using ZuluTime, shall be part of persisted data and saved/restored to/from simulation states.

* 1. 1 Zulu time events posted with absolute Zulu time are restored with the same Zulu time. The events with a Zulu time in the past are not executed; if all cycles of a Zulu time event are in the past, it is simply removed from the Scheduler.
  2. 2 Zulu time events posted with relative Zulu time are "moved" when restoring, such that the delays of the remaining executions from the "now" Zulu time at time of storing is equal to the delays of the remaining executions from the "now" Zulu time at time of restoring.

ECSS-E-ST-40-07\_1630225

When the SMP\_EpochTimeChanged global SMP event is emitted, the events already scheduled with Epoch time shall behave as follows:

Non-cyclic events with Epoch Time equal to or in the future of the new Epoch Time, are executed according to the Epoch Time they were originally scheduled;

Non-cyclic events with Epoch Time prior the new Epoch Time, are removed from the scheduler and not executed;

For Cyclic Events, any repeat that falls prior the new Epoch Time is not executed and any positive repeat count is reduced according to the number of skipped executions;

For Cyclic Events, any repeat that is equal or after the new Epoch Time is executed according to the original Epoch Time of the repeats.

ECSS-E-ST-40-07\_1630226

When the SMP\_MissionTimeChanged global SMP event is emitted, the events already scheduled with Mission time shall behave as follows:

Non-cyclic events with Mission time equal to or in the future of the new Mission Time, are executed according to the Mission Time they were originally scheduled;

Non-cyclic events with Mission time prior the new Mission Time, are removed from the scheduler and not executed;

For Cyclic Events, any repeat that falls prior the new Mission Time is not executed and any positive repeat count is reduced according to the number of skipped executions;

For Cyclic Events, any repeat that is equal or after the new Mission Time is executed according to the original Mission Time of the repeats.

ECSS-E-ST-40-07\_1630227

When the simulator is in Standby state, the scheduler shall behave as follows:

Events scheduled on simulation time including immediate Events, epoch and mission time are not processed;

Events scheduled on Zulu time are executed.

ECSS-E-ST-40-07\_1630228

When SetEventSimulationTime is called for the event that is currently executing, the time set shall take precedence over the cycle time configured in the event.

1. Meaning that the next execution occurs at the specified time and not at the time deduced from the event cycle time.

ECSS-E-ST-40-07\_1630229

When SetEventSimulationTime is called for the event that is currently executing, and the repetition left for the events is zero, an error shall be emitted.

* 1. 1 This call causes a contradiction, as the command is setting the time of the next execution, when there is no such execution.
  2. 2 This can be guarded by calling SetEventRepeat with a non-zero value before SetEventSimulationTime.

ECSS-E-ST-40-07\_1630230

The value -1 shall be a valid value for event execution time and event cycle time.

1. The event will not be executed until a SetEventSimulationTime is called to set a "reasonable" time on the event.

ECSS-E-ST-40-07\_1630231

When SetEventRepeat is called for the event that is currently executing, the value shall be used as for deciding the re-scheduling and then decremented.

1. This means that setting repeat to 1 will cause the event to be repeated exactly once after the current execution.

ECSS-E-ST-40-07\_1630232

The IScheduler IsEventScheduled method shall check if an event is in the scheduler or not, with the following argument and behaviour:

Argument:

“eventId” as a unique identifier of the Event.

Behaviour:

It returns true if the corresponding event has been scheduled but its start time does not yet elapse; or if it is not yet removed by RemoveEvent; or if it is currently executing; or if it has not yet finished its repeat count;

It returns false in any other case that does not satisfy (a).

1. Any EventId for which IsEventScheduled returns true is considered safe to pass to the other methods taking an EventId in parameter (like RemoveEvent) regardless of the time kind of the related event.

ECSS-E-ST-40-07\_1630233

The IScheduler AddRelativeZuluTimeEvent method shall add an Event to the scheduler, with the following arguments and behaviour:

Arguments:

“entryPoint“ giving the Entry Point to be called when the Event is executed;

“zuluTimeDelay“ giving the Zulu time delay from now until the first call of the Entry Point;

“cycleTime“ giving the cycle time of the Event as specified in requirement 5.3.3c;

“repeat“ giving the Event repetition count as specified in requirement 5.3.3b.

Behaviour:

If the given Zulu Time delay is less than zero, it throws an InvalidEventTime exception as per Services/InvalidEventTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

If Repeat is not zero and CycleTime is a value less than 1, it throws an InvalidCycleTime exception as per Services/InvalidCycleTime.h in [SMP\_FILES], the Event is not added to the scheduler and never executed;

After adding the new Event to the scheduler, it returns the EventId as per Services/EventId.h in [SMP\_FILES] identifying the added Event.

### Event Manager (IEventManager)

ECSS-E-ST-40-07\_1630234

The simulation environment shall provide an Event Manager component implementing the IEventManager interface as per Services/IEventManager.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630235

The IEventManager QueryEventId method shall return the Event identifier for an Event, with the following argument and behaviour:

Argument:

“eventName” giving the name of the Event.

Behaviour:

If called with an empty name, it throws an InvalidEventName exception as per Services/InvalidEventName.h in [SMP\_FILES];

If called with the name of one of the pre-defined Event types as in Table 5‑8, it returns the corresponding EventId as in Table 5‑8;

If called with a non-empty event name different from all pre-defined event types as in Table 5‑8, it returns an event identifier different from all pre-defined event identifiers in Table 5‑8;

If called with the same name again in the context of a restored simulation, it returns always the same event identifier.

1. This implies that the EventManager maintains a global list of events that is persisted in the simulation state and restored when needed.

ECSS-E-ST-40-07\_1630236

The Event Manager shall maintain a list of pairs of unique event identifiers and entry points.

1. The event identifier must only be unique within the Event Manager context; the Scheduler service uses the same EventId type, but uniqueness across services is not required.

ECSS-E-ST-40-07\_1630237

The Event Manager shall initialise the list of pairs to be empty at creation time.

ECSS-E-ST-40-07\_1630238

The IEventManager Subscribe method shall allow to subscribe an entry point to a global event identifier, with the following arguments and behaviour:

Arguments:

“event” giving the ID of the event to be subscribed;

“entryPoint” giving a pointer to the entry point to be called when the event is emitted.

Behaviour:

If called with a pair of event identifier and entry point that is not currently in the internal list, it adds this pair to the internal list;

If called with a pair of event identifier and entry point that is already in the internal list, it throws an EntryPointAlreadySubscribed exception as per Services/EntryPointAlreadySubscribed.h in [SMP\_FILES];

If called with an event identifier that does not exist, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630239

The IEventManager Unsubscribe method shall remove a pair from the list, with the following arguments and behaviour:

Arguments:

“event” giving the ID of the event to be unsubscribed;

“entryPoint” giving a pointer to the entry point to be unsubscribed.

Behaviour:

If called with a pair of event identifier and entry point that is currently in the internal list, it removes this pair to the internal list;

If called with a pair of event identifier and entry point that is not in the internal list, it throws an EntryPointNotSubscribed exception as per Services/EntryPointNotSubscribed.h in [SMP\_FILES];

If called with an invalid event identifier, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630240

The IEventManager Emit method shall emit a specific global event to all the subscribed entry points, with the following arguments and behaviour:

Arguments:

“event” giving the ID of the event to be emitted;

“synchronous” giving if the event is emitted synchronously to all subscribed entry points.

Behaviour:

If the eventId is unknown to the Event Manager, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP\_FILES];

If called with an event identifier for which pairs with entry points exist in the list, then these entry points are called;

If more than one entry point is called, then the order of the calls is the order of subscription using the Subscribe method;

If called with the synchronous flag set to false, the calls to the entry points are asynchronous, such that the call to the Emit method is not blocked from returning while waiting for calls to subscribed entry points to return;

If called with the synchronous flag set to true, the calls to the entry points are synchronous, such that the call to the Emit method is blocked from returning until the calls to all subscribed entry points return.

ECSS-E-ST-40-07\_1630241

The SMP predefined global events shall only be emitted in the conditions outlined in Table 5‑8 and only by the Simulation Environment.

ECSS-E-ST-40-07\_1630242

The SMP predefined global events shall be emitted with the synchronous flag set as per Table 5‑8.

ECSS-E-ST-40-07\_1630243

While an event for a simulator state transition is emitted using the IEventManger Emit call, subscribed entry points shall not trigger another simulation state transition.

ECSS-E-ST-40-07\_1630244

Entry point subscription or unsubscription during the execution of the IEventManger Emit call shall be taken into account the next time Emit is called.

ECSS-E-ST-40-07\_1630245

Table 5‑8: Condition for emitting predefined global events

| Name | EventId | Condition for emitting | Synchronous flag |
| --- | --- | --- | --- |
| SMP\_LeaveConnecting | 1 | When leaving the Connecting state with an automatic state transition to Initializing state | True |
| SMP\_EnterInitialising | 2 | When entering the Initialising state with an automatic state transition from Connecting state, or with the Initialise() state transition | True |
| SMP\_LeaveInitialising | 3 | When leaving the Initialising state with an automatic state transition to Standby state | True |
| SMP\_EnterStandby | 4 | When entering the Standby state with:   * an automatic state transition from Initialising, Storing or Restoring state * the Hold() state transition command from Executing state | True |
| SMP\_LeaveStandby | 5 | When leaving the Standby state with:   * the Run() state transition command to Executing state * the Store() state transition command to Storing state * the Restore() state transition command to Restoring state * the Initialise() state transition command to Initialising state | True |
| SMP\_EnterExecuting | 6 | When entering the Executing state with the Run() state transition command from Standby state | True |
| SMP\_LeaveExecuting | 7 | When leaving the Executing state with the Hold() state transition command to Standby state | True |
| SMP\_EnterStoring | 8 | When entering the Storing state with the Store() state transition command from Standby state | True |
| SMP\_LeaveStoring | 9 | When leaving the Storing state with an automatic state transition to Standby state | True |
| SMP\_EnterRestoring | 10 | When entering the Restoring state with the Restore() state transition command from Standby state | True |
| SMP\_LeaveRestoring | 11 | When leaving the Restoring state with an automatic state transition to Standby state | True |
| SMP\_EnterExiting | 12 | When entering the Exiting state with the Exit() state transition command from Standby state | True |
| SMP\_EnterAborting | 13 | When entering the Aborting state with the Abort() state transition command from any other state | True |
| SMP\_EpochTimeChanged | 14 | When changing the epoch time with the SetEpochTime() method of the time keeper service | True |
| SMP\_MissionTimeChanged | 15 | When changing the mission time with one of the SetMissionTime() and SetMissionStartTime() methods of the time keeper service | True |
| SMP\_EnterReconnecting | 16 | When entering the Reconnecting state with the Reconnect() state transition from Standby state | True |
| SMP\_LeaveReconnecting | 17 | When leaving the Reconnecting state with an automatic state transition to Standby state | True |
| SMP\_PreSimTimeChange | 18 | When all events have been executed by the Scheduler for a specific Simulation Time, but before the TimeKeeper changes the Simulation time to the time of next event | True |
| SMP\_PostSimTimeChange | 19 | When the simulation time has been changed by the Time Keeper, but before any events have been executed by the Scheduler | True |

### Resolver (IResolver)

ECSS-E-ST-40-07\_1630246

The simulation environment shall provide a Resolver component implementing the IResolver interface as per Services/IResolver.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630247

The IResolver ResolveAbsolute method shall return a reference to a Component, Field, Property, Operation, Failure, Event Sink, Event Source or Entry Point object in the simulation, with the following argument and behaviour:

Argument:

“absolutePath” giving the absolute path string of the object.

Behaviour:

If the “absolutePath” does not give the path to an object, it returns nullptr;

If no object with the given path can be found, it returns nullptr;

If “absolutePath” resolves to an object, it returns the IObject reference to the object.

* 1. 1 To allow keeping names as short as possible, and avoid dependency on the name of the simulator itself, absolute paths contain the name of either a top-level Model or Service, but not the name of the simulator, although the simulator itself is the top-level object. In fact, resolution of the absolute path “/” returns the ISimulator object itself.
  2. 2 The specification of path string is given in clause 5.1.3.

ECSS-E-ST-40-07\_1630248

The Resolver ResolveRelative method shall return a reference to an object in the simulation with the following arguments and behaviour:

Arguments:

“relativePath” giving a path string representing the relative path to the object;

“relativeRoot” being the object relative to which the path is resolved.

Behaviour:

If “relativePath” does not resolve to any object, it returns nullptr;

If “relativePath” resolves to an object, it returns an IObject reference to the object.

1. The specification of path string is given in clause 5.1.3.

### Link Registry (ILinkRegistry)

ECSS-E-ST-40-07\_1630249

The simulation environment shall provide a Link Registry service implementing the ILinkRegistry interface as Services/ILinkRegistry.h in [SMP\_FILES].

* 1. 1 The link registry maintains a global collection of links between components, supports adding, fetching and removing all links to a given target.
  2. 2 The links include Interface Links, Event Links and Field Links.

ECSS-E-ST-40-07\_1630250

The ILinkRegistry AddLink method shall increment the link count between two components, with the following arguments and behaviour:

Arguments:

“source” giving the source component;

“target” giving the target component.

Behaviour

The link count between both components is incremented by one, taking note of a new link that has been created.

1. This method can be called several times with the same arguments, when a source component has several links to the same target component.

ECSS-E-ST-40-07\_1630251

The ILinkRegistry GetLinkCount method shall return the link count between the given source and target, with the following arguments:

“source” giving the source component;

“target” giving the target component.

ECSS-E-ST-40-07\_1630252

The ILinkRegistry RemoveLink method shall decrement the link count between the two components, with the following arguments and behaviour:

Arguments:

“source” giving the source component;

“target” giving the target component.

Behaviour:

If the link count between both components is positive, it is decremented by one, taking note that a link has been removed, and true is returned;

If the link count between both components is 0, false is returned.

* 1. 1 Existing links have been previously added to the service using the AddLink() method.
  2. 2 This method can be called several times with the same arguments, when several links from the source component to the same target component are removed.

ECSS-E-ST-40-07\_1630253

The ILinkRegistry GetLinkSources method shall return the collection of source components for which a link to the given target component has been added to the registry.

ECSS-E-ST-40-07\_1630254

The ILinkRegistry CanRemove method shall return whether all source components linking to the given target can be asked to remove their link(s), with the following argument and behaviour:

Argument:

“target” giving the target component of the link.

Behaviour:

If all source components linking to the given target can be asked to remove their link(s), it returns true;

If at least one of the source components linking to the given target cannot be asked to remove its link(s), it returns false.

1. Components can be asked to remove their links if they implement the optional ILinkingComponent interface.

ECSS-E-ST-40-07\_1630255

The ILinkRegistry RemoveLinks method shall call the RemoveLinks method of all source components that implement the optional ILinkingComponent interface with the following argument:

“target” giving the component from which all links to be removed.

### Simulator (ISimulator)

ECSS-E-ST-40-07\_1630256

The simulation environment shall provide a Simulator Object implementing the ISimulator interface as per ISimulator.h in [SMP\_FILES].

* 1. 1 The ISimulator gives access to the simulation environment state and state transitions.
  2. 2 The ISimulator interface provides methods to add models and to add and retrieve simulation services.

ECSS-E-ST-40-07\_1630257

The Simulator Object shall have two containers as follows:

One “Models” container that holds simulation models with no upper limit on the number of Models to hold;

One “Services” container that holds simulation services with no upper limit on the number of Services to hold.

ECSS-E-ST-40-07\_1630258

The ISimulator interface shall be used to setup the simulation as per the following procedure:

Publish/Configure can be called multiple times, each time that new components are created;

First, the Publish method is called;

After returning from the Publish call, the Configure method is called.

After finishing the Publish/Configure calls sequence, the Connect method is called;

After returning from the Connect method, the Initialise method is called.

ECSS-E-ST-40-07\_1630259

The ISimulator Publish method shall call the Publish() method of all service and model instances in the component hierarchy that are in CSK\_Created state within the simulation as per following procedure:

If the simulation is not in Building state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

It traverses through the "Services" container of the simulator, as follows:

It calls the Publish() operation of each component in CSK\_Created state;

After calling Publish() on a service, it calls Publish() immediately on all its child components recursively.

After completing publication of the components in the “Services” container, it traverses through the "Models" container of the simulator as follows:

It calls the Publish() operation of each component in CSK\_Created state;

After calling Publish on a model, it calls Publish() immediately on all its child components recursively.

ECSS-E-ST-40-07\_1630260

The ISimulator Configure method shall call the Configure() method of all service and model instances in the component hierarchy that are in CSK\_Publishing state as per following procedure:

If the simulation is not in Building state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

It traverses through the "Services" container of the simulator. For each component, it performs the following procedure:

If the component is still in CSK\_Created state, it first calls the Publish() operation;

If the component is in CSK\_Published state, it calls the Configure() operation;

Then it immediately performs the same operation(s) recursively on all child components of the component.

After configuring the Services, it traverses through the "Models" container of the simulator. For each component, it performs the following procedure:

If the component is in CSK\_Created state, it first calls the Publish() operation;

If the component is in CSK\_Published state, it calls the Configure() operation;

Then it immediately performs the same operation(s) recursively on all child components of the component.

ECSS-E-ST-40-07\_1630261

The ISimulator Connect method shall call the Connect() method of all service and model instances in the component hierarchy that are in CSK\_Configured state as per the following procedure:

If the simulation is not in Building state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Connect method is called during the execution of the global event SMP\_LeaveConnecting, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

It traverses through the "Services" container of the simulator and performs the following actions:

If the component is in CSK\_Created state, it calls the Publish() operation;

If the component is in CSK\_Published state, it calls the Configure() operation;

If the component is in CSK\_Configured state, it calls the Connect() operation;

Afterwards, it performs the same operation(s) recursively on all child components of the component.

After connecting the services, the operation traverses through the "Models" container of the simulator performing the following actions:

If the component is in CSK\_Created state, it calls the Publish() operation;

If the component is in CSK\_Published state, it calls the Configure() operation;

If the component is in CSK\_Configured state, it calls the Connect() operation;

Afterwards, it performs the same operation(s) recursively on all child components of the component.

After all component Connect() operations have been executed, it issues the global event “SMP\_LeaveConnecting” via the Event Manager;

After returning from the “SMP\_LeaveConnecting” global event, it changes the simulation state to Initialising state;

After entering Initialising state, it issues the global event “SMP\_EnterInitialising” via the Event Manager;

After returning from the “SMP\_EnterInitialising” global event, it calls the initialisation entry points for all models that have registered an initialisation entry point via the ISimulator AddInitEntryPoint method in the order the entry points were added;

After executing the entry points, it removes the entry points from the list so that in case Initialise() is called again, the same initialisation entry point is not called twice;

After calling all initialisation entry points, it issues the global event “SMP\_LeaveInitialising” via the Event Manager;

After returning from the “SMP\_LeaveInitialising” global event, it changes the simulation state to Standby state;

Finally, the global event “SMP\_EnterStandby” is issued via the Event Manager.

ECSS-E-ST-40-07\_1630262

The ISimulator Initialise method shall call all initialisation entry points within the simulation as per the following procedure:

If the simulation is not in Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Initialise method is called during the execution of the global event SMP\_LeaveStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, it issues the global event “SMP\_LeaveStandby” via the Event Manager;

After returning from the SMP\_LeaveStandby global event, the simulator state changes to Initialising state;

After entering Initialising state, it issues the global event “SMP\_EnterInitialising” via the Event Manager;

After returning from the SMP\_EnterInitialising global event, it executes all entry points added via the ISimulator AddInitEntryPoint method in the order they have been added by the AddInitEntryPoint call;

After executing the entry points, it removes the entry points from the list so that in case Initialise is called again, the same initialisation entry point is not called twice;

After all entry points have been executed, it issues the global event “SMP\_LeaveInitialising” via the Event Manager;

After returning from the “SMP\_LeaveInitialising” global event, it changes the simulation state to Standby state;

Finally, it issues the global event “SMP\_EnterStandby” via the Event Manager.

ECSS-E-ST-40-07\_1630263

The ISimulator Run method shall change the state from Standby to Executing as per the following procedure:

If the simulation is not in Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the Run method is called during the execution of the global event SMP\_LeaveStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the Run method is called during the execution of the global event SMP\_EnterStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, it issues the global event “SMP\_LeaveStandby” via the Event Manager;

After returning from the SMP\_LeaveStandby global event, it changes the simulation state to “Executing” state;

After entering Executing state, it issues the global event “SMP\_EnterExecuting” via the Event Manager.

ECSS-E-ST-40-07\_1630264

The ISimulator Hold method shall change the state from Executing to Standby with the following argument and procedure:

Argument:

“hardHold” given if the Simulation is halting immediately.

Procedure:

If the simulation is not in Executing state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If called during the execution of the global event SMP\_LeaveExecuting, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If called during the execution of the global event SMP\_EnterExecuting, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Executing state, it waits until the current executing event, if any, completes;

After the current executing event is completed and if the hardHold argument is “false”, it executes all events scheduled for the current simulation time;

After all events that need executing are completed, it issues the global event “SMP\_LeaveExecuting” via the Event Manager;

After returning from the SMP\_LeaveExecuting global event, it changes the simulation state to “Standby” state;

After entering Standby state, it issues the global event “SMP\_EnterStandby” via the Event Manager.

* 1. 1 Halting the simulation with “hardHold” to “true” can cause the simulation to halt when some models have reached the current simulation time, but others not. This is useful for debugging purposes.
  2. 2 Halting the simulation with “hardHold” to “false” ensures that all simulation models have executed up until a consistent simulation time. This is useful for hardware in the loop simulations.

ECSS-E-ST-40-07\_1630265

The ISimulator Store method shall store the current simulation state to file, with the following argument and procedure:

Argument:

“filename” giving the name including the full path of the file to be saved.

Procedure:

If the simulation is not in Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Store method is called during the execution of the global event SMP\_LeaveStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Store method is called during the execution of the global event SMP\_EnterStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, it issues the global event “SMP\_LeaveStandby” via the Event Manager;

After returning from the SMP\_LeaveStandby global event, it changes the simulation state to Storing state;

After entering Storing state, it issues the global event “SMP\_ EnterStoring” via the Event Manager;

After returning from the “SMP\_EnterStoring” event, it performs Self Persistence by calling the IPersist Store method on all simulation objects that implement the IPersist interface;

After Self Persistence is completed, it performs External Persistence by storing the simulation state in the file given by the “filename” argument;

After Store operation has been completed, it issues the global event “SMP\_LeaveStoring” via the Event Manager;

After returning from the “SMP\_LeaveStoring” event, it changes the simulation state to Standby state;

After entering Standby state, it issues the global event “SMP\_EnterStandby” via the Event Manager.

1. Self-Persistence is performed prior to External Persistence during store as it allows models to update its published data prior to storing it.

ECSS-E-ST-40-07\_1630266

The ISimulator Restore method shall restore a simulation state from file, with the following argument and procedure:

Argument:

“filename” giving the name including the full path of the file to restore.

Procedure:

If the simulation is not in Standby state, then it returns and no action is taken;

If called during the execution of the global event SMP\_LeaveStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If called during the execution of the global event SMP\_EnterStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, it issues the global event “SMP\_LeaveStandby” via the Event Manager;

After returning from the SMP\_LeaveStandby global event, the simulation state is changed to Restoring state;

After entering Restoring state, it issues the global event “SMP\_EnterRestoring” via the Event Manager.

After returning from the “SMP\_EnterRestoring” event, it performs External Persistence by restoring the simulation state from a file given by the “filename” argument;

After completing External Persistence, it performs Self Persistence by calling the IPersist Restore method of all simulation objects which implement the IPersist interface;

After Restore operation has been completed, it issues the global event “SMP\_LeaveRestoring” via the Event Manager;

After returning from the “SMP\_LeaveRestoring” event, the simulation state is changed to Standby;

After entering Standby state, it issues the global event “SMP\_EnterStandby” via the Event Manager.

1. Self-Persistence is performed after to External Persistence at restore as it allows models to use its published data during the self-persistence restoration.

ECSS-E-ST-40-07\_1630267

The ISimulator Reconnect method shall reconnect the component hierarchy starting at the root component given as parameter, with the following argument and procedure:

Argument:

“root” giving the component in the hierarchy for which the reconnect shall start from. If nullptr is passed, the whole simulator tree is reconnected.

Procedure:

If the simulation is not in Standby state, then the method throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Reconnect method is called during the execution of the global event SMP\_LeaveStandby, then the method throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If Reconnect method is called during the execution of the global event SMP\_EnterStandby, then the method throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, the global event “SMP\_LeaveStandby” is issued via the Event Manager;

After returning from the SMP\_LeaveStandby global event, the simulation state is changed to “Reconnecting” state;

After entering Reconnecting state, it issues the global event “SMP\_EnterReconnecting” via the Event Manager;

The simulation environment ensures that all models under the given Root component parameter are published, configured and connected;

After Reconnect operation has been completed, it issues the global event “SMP\_LeaveReconnecting” via the Event Manager;

After returning from the “SMP\_LeaveReconnecting” event, the simulation state is changed to Standby;

After entering Standby state, the global event “SMP\_EnterStandby” is issued via the Event Manager.

ECSS-E-ST-40-07\_1630268

The ISimulator Exit method shall trigger a normal termination of a simulation, as per following procedure:

If the simulation is not in Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If called during the execution of the global event SMP\_LeaveStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If called during the execution of the global event SMP\_EnterStandby, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Standby state, it issues the global event “SMP\_LeaveStandby” via the Event Manager;

After returning from the SMP\_LeaveStandby global event, it changes the simulation state to “Exiting” state;

After entering Exiting state, it issues the global event “SMP\_EnterExiting” via the Event Manager;

The Exit method triggers a normal termination of the simulation.

ECSS-E-ST-40-07\_1630269

The ISimulator Abort method shall trigger an abnormal termination of a simulation, as per following procedure:

When called, it issues the global event “SMP\_EnterAborting” via the Event Manager;

After returning from the “SMP\_EnterAborting” event, it changes the simulation state to Aborting state;

After entering Aborting state, it triggers an abnormal termination of the simulation.

1. This method can be called from any other state.

ECSS-E-ST-40-07\_1630270

The ISimulator GetState method shall return the current simulator state as per SimulatorStateKind in SimulatorStateKind.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630271

The ISimulator AddInitEntryPoint method shall add entry points to be executed in the Initialising state, as per following argument and behaviour:

Argument:

“entryPoint” giving a pointer to the entry point interface of the entry point to be added.

Behaviour:

If the simulation is not in Building, Connecting or Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the simulation is in Building, Connecting or Standby state, it adds the entry point to the list of entry points to be executed once the simulation reaches Initialising state.

The ownership of the entry point remains with the caller of AddInitEntryPoint.

1. This allows components to subscribe to a callback during initialization phase since there are only explicit methods defined for Publish, Configure and Connect. This simplifies implementation for models that do not require initialization.

ECSS-E-ST-40-07\_1630272

The ISimulator AddModel method shall add a model to the Models container of the simulator, with the following argument and behaviour:

Argument:

“model” giving the model to be added.

Behaviour:

If the Simulation is not in Standby, Building, Connecting or Initializing state, it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the name of the new model conflicts with the name of an existing model already added via AddModel, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES];

If the name of the new model conflicts with the name of an existing service already added via AddService, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES].

* 1. 1 The container for the models has no upper limit and thus the ContainerFull exception is never thrown.
  2. 2 The method never throws the InvalidObjectType exception, as it gets a component implementing the IModel interface.

ECSS-E-ST-40-07\_1630273

The ISimulator AddService method shall add a user-defined service to the Services container, with the following argument and behaviour:

Argument:

“service” giving the service to be added.

Behaviour:

If the Simulation is not in Building state, it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP\_FILES];

If the name of the new service conflicts with the name of an existing model already added via AddModel, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES];

If the name of the new service conflicts with the name of an existing service already added via AddService, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES].

* 1. 1 The container for the services has no upper limit and thus the ContainerFull exception is never thrown.
  2. 2 The method never throws the InvalidObjectType exception, as it gets a component implementing the IService interface.
  3. 3 It is recommended that custom services include a project or company acronym as prefix in their name, to avoid collision of service names.

ECSS-E-ST-40-07\_1630274

The ISimulator GetService method shall return the interface of a service with the following argument and behaviour:

Argument:

“name” giving the name of the service.

Behaviour:

If no service with the given name is found in the “Services” container as per 5.3.7ff, it returns nullptr;

If a service with the given name is found in the “Services” container as per 5.3.7ff, it returns a reference to that service.

1. For the mandatory services, it is recommended to use the dedicated convenience methods listed in requirements 5.3.7t to 5.3.7y, which are guaranteed to return valid references.

ECSS-E-ST-40-07\_1630275

The ISimulator GetLogger method shall return the interface of the mandatory logger service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630276

The ISimulator GetTimeKeeper method shall return the interface to the mandatory time keeper service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630277

The ISimulator GetScheduler method shall return the interface to the mandatory scheduler service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630278

The ISimulator GetEventManager method shall return the interface to the mandatory event manager service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630279

The ISimulator GetResolver method shall return the interface to the mandatory resolver service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630280

The ISimulator GetLinkRegistry method shall return the interface to the mandatory link registry service.

1. This is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.

ECSS-E-ST-40-07\_1630281

The ISimulator RegisterFactory method shall register a component factory, with the following argument and behaviour:

Argument:

“componentFactory” giving the factory to be registered.

Behaviour:

If another factory has been registered using the same unique identifier already, it raises a DuplicateUuid exception as per DuplicateUuid.h in [SMP\_FILES].

* 1. 1 The simulator can use this factory to create component instances of the component implementation in its CreateInstance() method.
  2. 2 This method is typically called early in the Building state to register the available component before the hierarchy of model instances is created.

ECSS-E-ST-40-07\_1630282

The ISimulator CreateInstance method shall create an instance of a component, with the following arguments and behaviour:

Arguments:

“uuid” giving a unique identifier of the component implementation to create;

“name” giving the name of the new instance;

“description” giving the description of the new instance;

“parent” giving the parent object of the new instance.

Behaviour:

If the “uuid” provided does not corresponds to a registered factory through the RegisterFactory method, it returns nullptr;

If the name provided is not a valid object name, it raises an InvalidObjectName exception as per InvalidObjectName.h in [SMP\_FILES];

If the parent provided is not a valid object, it raises an InvalidParent exception as per InvalidParent.h in [SMP\_FILES];

If the “uuid” provided corresponds to a registered model, and name and parent are valid, it returns a reference to the newly created model with name, description and parent set as provided.

1. This method is typically called during the Building state when building the hierarchy of models or in the Standby state when adding new components to the hierarchy of models.

ECSS-E-ST-40-07\_1630283

The ISimulator GetFactory method shall return the factory of the component with the following argument and behaviour:

Argument:

“uuid” giving a unique identifier of the component implementation.

Behaviour:

If a factory has been registered with the given “uuid”, it returns a pointer to the registered factory;

If no factory for the given “uuid” has been registered, it returns nullptr.

ECSS-E-ST-40-07\_1630284

The ISimulator GetFactories method shall return a collection of all registered facories as per FactoryCollection in FactoryCollection.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630285

The ISimulator GetTypeRegistry method shall return a reference to the Type Registry.

ECSS-E-ST-40-07\_1630286

The ISimulator LoadLibrary method shall load a library for a Package, with the following argument and behaviour:

Argument:

"libraryPath" to the library to load;

“flag” to describe visibility of the loaded library symbols for subsequently loaded libraries, whose type is an enumeration as per LibraryLoadingFlag.h in [SMP\_FILES], specified in Table 5‑9.

Behaviour:

If called with an invalid libraryPath, it throws a FileNotFound exception as per FileNotFound.h in [SMP\_FILES];

If called with an libraryPath pointing to a library without the GetSmpVersion() function, it throws an InvalidSmpVersion exception as per InvalidSmpVersion.h in [SMP\_FILES];

If called with an libraryPath pointing to a library without the Initialise() function, it throws an InvalidFile exception as per InvalidFile.h in [SMP\_FILES];

If called with an libraryPath pointing to a library without the Finalise() function, it throws an InvalidFile exception as per InvalidFile.h in [SMP\_FILES];

It loads this library into memory and calls the “GetSmpVersion()” function of the library;

If the “GetSmpVersion()” function return value does not match ECSS\_SMP\_VERSION as per Version.h in [SMP\_FILES], it throws an InvalidSmpVersion exception as per InvalidSmpVersion.h in [SMP\_FILES];

It loads this library into memory and calls the dynamic "Initialise()" function of this library;

If called with the LLF\_LOCAL or LLF\_GLOBAL flag, the value is converted to an equivalent value supported by the underlying operating system;

If called with the LLF\_AUTO flag, the appropriate value is determined by the ISimulator implementation;

If called with the file name of a library, it calls the dynamic "Finalise()" function of this library when in the simulator Exiting or Aborting state.

* 1. 1 to item (h): if there is no equivalent value in the underlying operation system, its value is ignored.
  2. 2 to item (h): under the Unix-like OS, LLF\_LOCAL and LLF\_GLOBAL correspond respectively to the RTLD\_LOCAL and RTLD\_GLOBAL flags in the dlopen() system call.
  3. 3 It is expected that the Operating System loads the library into memory only once even in case this method is called multiple times.

Table 5‑9: Library loading flags

| Name | Description |
| --- | --- |
| LLF\_AUTO | The library loading option will be selected by the simulation environment implementation. |
| LLF\_LOCAL | Symbols defined in this library will not be made available to resolve references in subsequently loaded libraries. |
| LLF\_GLOBAL | The symbols defined by this library will be made available for symbol resolution of subsequently loaded libraries. |

ECSS-E-ST-40-07\_1630287

The ISimulator GetContainers method shall return a ContainerCollection with two containers as follows:

One container called “Models” with all the models of the ISimulator;

One container called “Services” with all the services of the ISimulator.

ECSS-E-ST-40-07\_1630288

The ISimulator GetContainer method shall return the IContainer interface to the container, with the following argument and behaviour:

Argument:

“name” of the container to be returned.

Behaviour:

If called with “Models” as argument, it returns the reference to the Models container;

If called with “Services” as argument, it returns the reference to the Services container;

If called with anything else than “Models” or “Services”, it returns nullptr.

ECSS-E-ST-40-07\_1630289

The ISimulator GetParent shall return nullptr.

1. The Simulator is the root object in the simulator tree.

ECSS-E-ST-40-07\_1630290

The ISimulator GetName shall return a valid name.

### Persistence

#### Storage Reader Interface (IStorageReader)

ECSS-E-ST-40-07\_1630291

The simulation environment shall provide a component implementing the IStorageReader interface as per IStorageReader.h in [SMP\_FILES].

* 1. 1 The IStoragerReader interface provides functionality to read data from storage.
  2. 2 The IStoragerReader interface allows objects implementing the IPersist interface to restore their state.

ECSS-E-ST-40-07\_1630292

The IStorageReader Restore method shall restore data from storage, with the following arguments and behaviour:

Arguments:

“address” giving the address of memory block;

“size”, giving the size of the memory block.

Behaviour:

It reads from the storage a memory block of the given size at the given address.

ECSS-E-ST-40-07\_1630293

The IStorageReader GetStateVectorFileName method shall return the full name including the absolute path of the file currently in use by the Storage Reader.

ECSS-E-ST-40-07\_1630294

The IStorageReader GetStateVectorFilePath method shall return a full absolute path to the directory of the file currently in use.

1. The path can be used when reading additional files that correspond to the file read.

#### Storage Writer Interface (IStorageWrite)

ECSS-E-ST-40-07\_1630295

The simulation environment shall provide a component implementing the IStorageWriter interface as per IStorageWriter.h in [SMP\_FILES].

* 1. 1 The IStorageWriter interface provides functionality to write data to storage.
  2. 2 The IStorageWriter interface allows objects implementing the IPersist interface to store their state.

ECSS-E-ST-40-07\_1630296

The IStorageWriter Store method shall store data to storage by writing a memory block of data to the file with the following arguments:

“address” giving the address of memory block;

“size” giving the size of the memory block.

ECSS-E-ST-40-07\_1630297

The IStorageWriter GetStateVectorFileName method shall return the full name including the absolute path of the file currently in use by the Storage Writer.

ECSS-E-ST-40-07\_1630298

The IStorageWriter GetStateVectorFilePath method shall return a full absolute path to the directory of the file currently in use.

1. The path can be used when writing additional files that correspond to the file written.

### Publication

#### IPublication

ECSS-E-ST-40-07\_1630299

The simulation environment shall provide a component implementing the IPublication interface as per IPublication.h in [SMP\_FILES].

1. The IPublication interface provides functionality to allow publishing simulation model members, including fields, properties and operations.

ECSS-E-ST-40-07\_1630300

The IPublication GetTypeRegistry method shall return a reference to the Type Registry.

1. See clause 5.3.10 for details on the Type Registry.

ECSS-E-ST-40-07\_1630301

The IPublication PublishOperation method shall allow publishing of an operation, with the following arguments and behaviour:

Arguments:

“name” giving the operation name;

“description” giving the operation description;

“view” giving the visibility of the operation.

Behaviour:

If an Operation with the same Name is already published, it updates the “Description” and “View” of the previous publication, clears all published Parameters for the Operation, and returns the same IPublishOperation of the previously published Operation;

If an Operation with the same Name is not published, it creates a new IPublishOperation instance and returns it;

If the component that publishes the Operation does not implement IDynamicInvocation, it throws a NoDynamicInvocation exception as per NoDynamicInvocation.h in [SMP\_FILES].

* 1. 1 The returned IPublishOperation interface allows callers of PublishOperation to publish parameters and return value of the operation.
  2. 2 See clause 5.2.12.2 for details on how to publish a complete operation including its parameters.

ECSS-E-ST-40-07\_1630302

The IPublication PublishProperty method shall allow publishing a property, with the following arguments and behaviour:

Arguments:

“name“ giving the property name;

“description“ giving the property description;

“typeUuid“ giving the property type;

“accessKind“ giving the property access restrictions as per AccessKind.h in [SMP\_FILES] allowing the following values:

* + - 1. Read and write;
      2. Read only;
      3. Write only.

“view“ giving its view kind attribute as per ViewKind.h in [SMP\_FILES].

Behaviour:

If the given UUID is not a UUID of a registered type, it throws a TypeNotRegistered exception as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the given UUID is not an UUID of a Simple Type, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

If the component that publishes the Property does not implement IDynamicInvocation, it throws a NoDynamicInvocation exception as per NoDynamicInvocation.h in [SMP\_FILES];

If a Property with the same Name is already published, it updates the “description”, “uuid”, “accessKind” and “view” of the previous Property and returns the previous IProperty object;

Otherwise, it creates and returns a new IProperty object.

1. to item (a): The UUID stored in the TypeNotRegistered exception is the UUID given to PublishProperty.

ECSS-E-ST-40-07\_1630303

The IPublication GetProperties method shall return a collection of published properties as per PropertyCollection in PropertyCollection.h in [SMP\_FILES] that is identical to the collection of properties published through the PublishProperty() operations in 5.3.9.1d and 5.3.9.1i.

ECSS-E-ST-40-07\_1630304

The IPublication GetOperations method shall return a collection of published operations as per OperationCollection in OperationCollection.h in [SMP\_FILES] that is identical to the collection of operations published through the PublishOperation() operations in 5.3.9.1c and 5.3.9.1h.

ECSS-E-ST-40-07\_1630305

The IPublication Unpublish method shall release all data published earlier via the Publish operations.

1. This is called prior to deleting the component that has called into a specific IPublication instance.

ECSS-E-ST-40-07\_1630306

The IPublication PublishOperation method shall allow publishing an operation, with the following arguments and behaviour:

Arguments:

"operation" giving the IOperation object.

Behaviour:

If the operation parent object, obtained by calling the GetParent method on the operation argument, does not implement IDynamicInvocation, it throws a NoDynamicInvocation exception as per NoDynamicInvocation.h in [SMP\_FILES];

If an Operation with the same Name is already published, it stores the operation argument as a replacement of the previously published operation;

If an Operation with the same Name is not published, it stores the provided instance.

1. The ownership of the published operation remains with the publishing component.

ECSS-E-ST-40-07\_1630307

The IPublication PublishProperty method shall allow publishing a property, with the following arguments and behaviour:

Arguments:

"property" giving the IProperty object.

Behaviour:

If the property parent object, obtained by calling the GetParent method on the property argument, does not implement IDynamicInvocation, it throws a NoDynamicInvocation exception as per NoDynamicInvocation.h in [SMP\_FILES];

If a Property with the same Name is already published, it stores the property argument as a replacement of the previously published property;

If a Property with the same Name is not published, it stores the provided instance.

1. The ownership of the published property remains with the publishing component.

ECSS-E-ST-40-07\_1630308

The IPublication GetOperation method shall return the Operation object with the following arguments and behaviour:

Arguments:

“name” giving the Operation name to get.

Behaviour:

If the Operation with the given name argument does not exist, it returns nullptr;

If the Operation with the given name argument exists, it returns the corresponding IOperation object.

ECSS-E-ST-40-07\_1630309

The IPublication GetProperty method shall return the Property object with the following arguments and behaviour:

Arguments:

“name” giving the Property name to get.

Behaviour:

If the Property with the given name argument does not exist, it returns nullptr;

If the Property with the given name argument exists, it returns the corresponding IProperty object.

ECSS-E-ST-40-07\_1630310

All IPublication Publish methods shall throw an InvalidObjectName exception as per InvalidObjectName.h in [SMP\_FILES] if the name given in the arguments is invalid as per requirement 5.2.1a.

ECSS-E-ST-40-07\_1630311

All IPublication Publish methods shall throw a DuplicateName exception as per DuplicateName.h in [SMP\_FILES] if the name given in the arguments has already been published for another different SMP object kind within the same parent.

1. This requirement is a direct consequence of 5.2.1b.

#### IPublishOperation

ECSS-E-ST-40-07\_1630312

The simulation environment shall provide a component implementing the IPublishOperation interface as per Publication/IPublishOperation.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630313

The IPublishOperation PublishParameter method shall allow publishing parameters of an operation, with the following arguments and behaviour:

Arguments:

“name” giving the parameter name;

“description” giving the parameter description;

“typeUuid” giving the parameter type identifier in the Type Registry;

“direction” giving the parameter direction as per Publication/ParameterDirectionKind.h in [SMP\_FILES] allowing the following values:

* + - 1. “In” for read only parameters that are not changed by the operation;
      2. “Out” for write only parameters where no initial value is specified but the operation provides an output value;
      3. “InOut” for both read and write parameters;
      4. “Return” for the operation return value.

Behaviour:

If the name of the new parameter to be published is already used by another published parameter by the same Operation, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

If the given UUID is not a valid UUID of a registered type, it throws TypeNotRegistered as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the given UUID is not an UUID of a simple type, it throws InvalidType as per InvalidType.h in [SMP\_FILES]l

If the name of the new parameter to be published is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If the parameter to be published has direction Return and the Operation already has a published Parameter with direction Return, it throws InvalidParameterDirection as per Publication/InvalidParameterDirection.h in [SMP\_FILES].

#### IPublishField

ECSS-E-ST-40-07\_1630314

The simulation environment shall provide a component implementing the IPublishField interface as per Publication/IPublishField.h in [SMP\_FILES].

1. The IPublishField interface provides functionality to allow publishing simulation model fields.

ECSS-E-ST-40-07\_1630315

The first IPublishField PublishField overloaded method shall allow publishing of a primitive type field, with the following arguments and behaviour:

Arguments:

“name” giving the field name;

“description” giving the field description;

“address” giving the pointer to the address where the value of the field is found supporting the following pointer types:

Char8,

Bool,

Int8,

Int16,

Int32,

Int64,

UInt8,

UInt16,

UInt32,

UInt64,

Float32,

Float64.

“view” giving the fields view attribute as per ViewKind.h in [SMP\_FILES];

“state” given if the field is part of the simulation state when storing or restoring or not;

“input” giving if the field is an input field or not;

“output” giving if the field is an output field or not.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

Otherwise, it creates and returns a new IField object.

* 1. 1 The view kind attribute is specified in Table 4‑2.
  2. 2 There is no publishing call for String8 as it relies on dynamically allocated memory areas, hence cannot be published like the other primitive types.
  3. 3 Duration and DateTime cannot be supported in the same way, as they are not strong types (they are defined to be identical to Int64, but with a different semantic). For publication of Duration and DateTime, PublishField with UUID is used.

ECSS-E-ST-40-07\_1630316

The second IPublishField overloaded PublishField method shall allow publishing a field against a type found in the Type Registry, with the following arguments and behaviour:

Arguments:

“name” giving the field name;

“description” giving the field description;

“address” giving the field memory address;

“typeUuid” giving the field type;

“view” giving the fields view attribute as per ViewKind.h in [SMP\_FILES];

“state” given if the field is part of the simulation state when storing or restoring or not;

“input” giving if the field is an input field or not;

“output” giving if the field is an output field or not.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

If the given UUID is not a UUID of a valid registered type, it throws TypeNotRegistered as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the given UUID is the UUID of the String8 type or of an Array of String8 type, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

Otherwise, it creates and returns a new IField object.

* 1. 1 The UUID stored in the TypeNotRegistered exception is the UUID given to PublishField.
  2. 2 The view kind attribute is specified in Table 4‑2.

ECSS-E-ST-40-07\_1630317

The third IPublishField PublishField overloaded method shall allow publishing a field that implements IField, with the following argument and behaviour:

Argument:

“field” giving a pointer to the field IField interface.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES].

* 1. 1 All additional data defining the field is available via the operations supported by the IField interface.
  2. 2 The ownership of the published field remains with the publishing component.

ECSS-E-ST-40-07\_1630318

The IPublishField PublishArray method shall publish an array of simple types that can be mapped to a primitive type, with the following arguments and behaviour:

Arguments:

“name” giving the array name;

“description” giving the array description;

“count” giving the size of an array;

“address” giving the array memory address of the first element;

“type” giving the type of each array item;

“view” giving the array view attribute as per ViewKind.h in [SMP\_FILES];

“state” given if the array is part of the simulation state when storing or restoring or not;

“input” giving if the array is an input field or not;

“output” giving if the array is an output field or not.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

If the given type is String8, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

Otherwise, it creates and returns an ISimpleArrayField object.

ECSS-E-ST-40-07\_1630319

The IPublishField PublishArray method shall allow to publish arrays of any type by allowing each element of the array to be published individually, with the following arguments and behaviour:

Arguments:

“name” giving the array name;

“description” giving the array description.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

A pointer to an IPublishField object is returned.

* 1. 1 The returned IPublishField interface allows callers of PublishArray to publish each element of the array individually.
  2. 2 See clause 5.2.12.2 for details on how to publish each element individually.

ECSS-E-ST-40-07\_1630320

The IPublishField PublishStructure method shall allow publishing a structure by allowing each child element to be published individually, with the following arguments and behaviour:

Arguments:

“name” giving the struct name;

“description” giving the struct description.

Behaviour:

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

A pointer to an IPublishField object is returned.

* 1. 1 The returned IPublishField interface allows callers of PublishStructure to publish each element of the struct individually.
  2. 2 See clause 5.2.12.2 for details on how to publish each element individually.

ECSS-E-ST-40-07\_1630321

The IPublishField GetField method shall return an interface to a field, with the following argument and behaviour:

Argument:

“fullName“ giving the path relative to the component.

Behaviour:

If no field exists with the given fully qualified name, it returns nullptr;

If the field matching the given fully qualified name has a simple type, it returns an ISimpleField instance;

If the field matching the given fully qualified name is an Array Field, it returns an IArrayField instance;

If the field matching the given fully qualified name is a Structure Field, it returns an IStructureField instance;

If the field matching the given fully qualified name is a Simple Array Field, it returns an ISimpleArrayField instance;

If the field matching the given fully qualified name is an item of a simple Array Field, it returns nullptr;

If the field matching the given fully qualified name is an output field, it returns an IOutputField instance.

* 1. 1 to item (f): To get the corresponding simple value in this case, it is recommended to call IComponent.GetSimpleValue.
  2. 2 to item (g): The path relative to the component is constructed as per clause5.1.3. Examples:
     + MyStructuredField.InnerField
     + MyArrayField[2]
     + MyStructuredField.ArrayInnerField[2]

ECSS-E-ST-40-07\_1630322

The IPublishField GetFields method shall return a collection of published fields as per FieldCollection in FieldCollection.h in [SMP\_FILES] that is identical to the collection of fields published through the PublishField() operations in 5.3.9.3b to 5.3.9.3g.

### Type Registry

#### ITypeRegistry

ECSS-E-ST-40-07\_1630323

The simulation environment shall provide, via the IPublication interface, a Type Registry publication implementing the ITypeRegistry interface as Publication/ITypeRegistry.h in [SMP\_FILES].

1. This interface defines a registration mechanism for user defined types.

ECSS-E-ST-40-07\_1630324

The Type Registry shall contain all pre-defined SMP value types with their pre-defined universally unique identifiers as per ecss.smp.l1.smpcat in [SMP\_FILES].

1. It is not mandatory for the models to make use of the Type Registry.

ECSS-E-ST-40-07\_1630325

The ITypeRegistry GetType method shall return the interface to the requested primitive type, with the following argument:

“type” giving a primitive type kind.

1. This method can be used to map primitive types to the IType interface to treat all types identically.

ECSS-E-ST-40-07\_1630326

The ITypeRegistry GetType method shall return the interface to the requested type, with the following argument and behaviour:

Argument:

“typeUuid” giving the UUID for which the type is returned.

Behaviour:

If no type with the registered UUID is found, it returns nullptr.

1. This method can be used to find out whether a specific type has been registered before.

ECSS-E-ST-40-07\_1630327

The ITypeRegistry AddFloatType method shall return the interface to a new Float type, with the following arguments and behaviour:

Arguments:

“name” giving the name of the registered type;

“description” giving the description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type;

“minimum” giving the minimum value for float;

“maximum” giving the maximum value for float;

“minIncluded” giving whether the minimum value is valid or not;

“maxIncluded” giving whether the maximum value is valid or not;

“unit” giving the unit of the type;

“type” giving the primitive type to use for the Float type.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If the Primitive Type given is not a Float type, it throws an InvalidPrimitiveType exception as per Publication/InvalidPrimitiveType.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES].

* 1. 1 IComponent and IDynamicInvocation support fields, parameters and operations of Float types via the PTK\_Float32 and PTK\_Float64 primitive type, as a Float is mapped either to Float32 or Float64.
  2. 2 In the type registry, name duplication is possible as long as the UUID is unique.

ECSS-E-ST-40-07\_1630328

The ITypeRegistry AddIntegerType method shall return the interface to a new Integer type, with the following arguments and behaviour:

Arguments:

“name” giving the name of the registered type;

“description” giving the description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type;

“minimum” giving the minimum allowed value for integer;

“maximum” giving the maximum allowed value for integer;

“unit” giving the unit of the type;

“primitiveType” giving the primitive type to use for the Integer type.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If the Primitive Type given is not an Integer type, it throws an InvalidPrimitiveType exception as per Publication/InvalidPrimitiveType.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES].

1. IComponent and IDynamicInvocation support fields, parameters and operations of Integer types via the PTK\_Int primitive types, as an Integer is mapped to one of Int8 / Int16 / Int32 / Int64 / UInt8 / UInt16 / UInt32 / UInt64.

ECSS-E-ST-40-07\_1630329

The ITypeRegistry AddEnumerationType method shall return the interface to a new Enumeration type, with the following arguments and behaviour:

Arguments:

“name” giving the name of the registered type;

“description” giving the description of the registered type;

“typeUuid” giving the universally unique identifier (UUID) of the registered type.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630330

The ITypeRegistry AddArrayType method shall return the interface to a new Array type, with the following arguments and behaviour:

Arguments:

“name” giving the name of the registered type;

“description” giving the description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type;

“itemTypeUuid” giving the universally unique identifier of the Type of the array items;

“itemSize” giving the size of an array item in bytes, taking possible padding into account, as it can be used by the simulation environment to calculate the memory offset between array items;

“arrayCount” giving the number of elements in the array;

“simpleArray” giving a flag whether a field of this array type is to be implemented as ISimpleArrayField or as IArrayField.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If another type with the same typeUuid already is registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES];

If the itemTypeUuid is not yet registered, it throws a TypeNotRegistered exception as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If simpleArray is true and itemTypeUuid does not resolve in a simple type, it throws a InvalidArrayItemType exception as per Publication/ InvalidArrayItemType.h in [SMP\_FILES];

Otherwise, the array type is added to the Type Registry.

ECSS-E-ST-40-07\_1630331

The ITypeRegistry AddStringType method shall return the interface to a new String type, with the following arguments and behaviour:

Arguments:

“name” giving the name of the registered type;

“description” giving the description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type;

“length” giving the maximum length of the string.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630332

The ITypeRegistry AddStructureType method shall return the interface to a new Structure type that allows adding fields, with the following arguments and behaviour:

Arguments:

“name” giving name of the registered type;

“description” giving description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630333

The ITypeRegistry AddClassType method shall return the interface to a new Class type that allows adding fields, with the following arguments and behaviour:

Arguments:

“name” giving name of the registered type;

“description” giving description of the registered type;

“typeUuid” giving the universally unique identifier of the registered type;

"baseClassUuid" giving the universally unique identifier of the base class, or Uuid\_Void when the Class has no base Class.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If another type with the same UUID is already registered, it throws a TypeAlreadyRegistered exception as per Publication/TypeAlreadyRegistered.h in [SMP\_FILES];

If the baseClassUuid is not yet registered, it throws a TypeNotRegistered exception as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the baseClassUuid is not Uuid\_Void and is not an UUID of a Class Type, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

Otherwise the class type is added to the registry.

#### IType

ECSS-E-ST-40-07\_1630334

The simulation environment shall provide a class implementing the IType interface as per Publication/IType.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630335

The IType GetPrimitiveTypeKind method shall return the primitive type kind as per PrimitiveTypes.h in [SMP\_FILES] for types in the type registry as follows:

If the type cannot be mapped to a primitive type kind, it returns PTK\_None;

If the type is registered as a derived type of one of the primitive types, it returns the Primitive type kind;

If the type is one of the primitive types themselves, it returns the corresponding primitive type kind.

* 1. 1 The primitive types are specified in Table 5‑1.
  2. 2 Types that cannot be mapped to a primitive type include:
     + Arrays registered via ITypeRegistry AddArrayType;
     + Structures registered via ITypeRegistry AddStructureType;
     + Classes registered via ITypeRegistry AddClassType.
  3. 3 Derived types include:
     + Enumerations registered via ITypeRegistry AddEnumerationType;
     + Strings registered via ITypeRegistry AddStringType;
     + Integer types registered via the ITypeRegistry AddIntegerType;
     + Float types registered via the ITypeRegistry AddFloatType.

ECSS-E-ST-40-07\_1630336

The IType GetUuid method shall return the Universally Unique Identifier of the type.

ECSS-E-ST-40-07\_1630337

The IType Publish method shall allow publishing a new field in a receiver, with the following arguments and behaviour:

Arguments:

“receiver” giving the publishing interface to publish against;

“name” giving the name of instance;

“description” giving the description of instance;

“address” giving the address of instance;

“viewKind” giving the visibility of instance;

“state” giving if the instance is part of the simulation state or not;

“input” giving if writing to the instance is allowed;

“output” giving if reading from the instance is allowed.

Behaviour:

If the name of the new field to be published is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If the name of the new field to be published is already used by another published field in the same parent object, it throws DuplicateName as per DuplicateName.h in [SMP\_FILES];

If the UUID of the IType being published is not a valid registered type, it throws TypeNotRegistered as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the UUID of the IType being published is the UUID of the String8 type or of an Array of String8 type, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

Otherwise, it creates and returns a new IField object.

1. Using the IType Publish method is an alternative method to publish a field than using the IPublication publishing methods.

#### IStructureType

ECSS-E-ST-40-07\_1630338

The simulation environment shall provide a class implementing the IStructureType interface as per Publication/IStructureType.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630339

The IStructureType AddField method shall add a field to the structure, with the following arguments and behaviour:

Arguments:

“Name” giving the name of the field;

“Description” giving the description of the field;

“Uuid” giving the universally unique identifier of the field Type, as a value type;

“offset” giving the memory offset of field relative to the Structure;

“ViewKind” giving the visibility of the instance;

“state” giving if the instance is part of the simulation state or not;

“input” giving if the field is an input field or not;

“output” giving if the field is an output field or not.

Behaviour:

If the given Name is not a valid object name, it throws InvalidObjectName as per InvalidObjectName.h in [SMP\_FILES];

If the given Name is already used by another published field by the same StructureType, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES];

If the Uuid is not yet registered, it throws a TypeNotRegistered exception as per Publication/TypeNotRegistered.h in [SMP\_FILES];

If the given UUID is the UUID of the String8 type or of an Array of String8 type, it throws InvalidType as per InvalidType.h in [SMP\_FILES];

#### IClassType

ECSS-E-ST-40-07\_1630340

The simulation environment shall provide a class implementing the IClassType interface as per Publication/IClassType.h in [SMP\_FILES].

#### IArrayType

ECSS-E-ST-40-07\_1630341

The simulation environment shall provide a class implementing the IArrayType interface as per Publication/IArrayType.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630342

The IArrayType GetSize method shall return the number of elements in the array.

ECSS-E-ST-40-07\_1630343

The IArrayType GetItemType method shall return a pointer to the type that all array items have.

#### IEnumerationType

ECSS-E-ST-40-07\_1630344

The simulation environment shall provide a class implementing the IEnumerationType interface as per Publication/IEnumerationType.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630345

The IEnumerationType AddLiteral method shall add a literal entry to the enumeration given the following input arguments and behaviour:

Arguments:

“name” giving the name of the literal;

“description” giving the description of the field;

“value” giving the “value” of the literal.

Behaviour:

If the given Name is not a valid object name, it throws an InvalidObjectName exception as per InvalidObjectName.h in [SMP\_FILES];

If the given Name is already added as a literal to the enumeration, it throws a DuplicateName exception as per DuplicateName.h in [SMP\_FILES];

If the given Value is already added as a literal to the enumeration, it throws a DuplicateLiteral exception as per Publication/DuplicateLiteral.h in [SMP\_FILES].

#### IStringType

ECSS-E-ST-40-07\_1630346

The simulation environment shall provide a class implementing the IStringType interface as per Publication/IStringType.h in [SMP\_FILES].

1. A String type represents a null-terminated string that can contain a maximum number of Smp::Char8 characters. It is a type for which the IType GetPrimitiveTypeKind method returns PTK\_String8.

ECSS-E-ST-40-07\_1630347

The IStringType GetMaxLength method shall return the maximum length of the string, excluding the last null character.

1. A String Type has memory space to contain at most (GetMaxLength + 1) bytes.

#### Type Resolution requirements

##### General

A Type stored in the Type Registry can be resolved using the associated UUID. The Simulation Environment does type resolution whenever a method is called passing a type UUID parameter.

##### Requirements

ECSS-E-ST-40-07\_1630348

A Type registered with the Type Registry shall be resolvable using its UUID.

ECSS-E-ST-40-07\_1630349

All Primitive Types shall be resolvable.

1. See Table 5‑1 for the list of Primitive Types.

ECSS-E-ST-40-07\_1630350

A Simple Type shall be resolvable if it exists in the Type Registry.

1. A Simple type is a type for which the IType GetPrimitiveTypeKind method returns a value different from PTK\_None.

ECSS-E-ST-40-07\_1630351

An Array Type shall be resolvable if its item Type and itself exist in the Type Registry.

ECSS-E-ST-40-07\_1630352

A Structure Type shall be resolvable if all its child Field Types and itself exist in the Type Registry.

ECSS-E-ST-40-07\_1630353

A Class Type shall be resolvable if its base class Type is resolvable; all its child Field Types, and itself exist in the Type Registry.

1. The base Class type is optional.

ECSS-E-ST-40-07\_1630354

The Simulation Environment shall resolve a complex type at registration of that type with the Type Registry.

* 1. 1 This approach, that consists thus in resolving the type completely at the moment where it is registered with the Type Registry, is called “eager resolution”.
  2. 2 In the eager resolution approach, resolution of a complex type resp. array, structure and class types, that depend on more than one type UUID (i.e their own UUID and UUIDs of resp. the items of an array, the sub-fields of a structure or a class, the base class of a class) succeeds if and only if all dependent type UUIDs have been well registered with the Type Registry.
  3. 3 In the eager resolution approach, resolution of a simple type succeeds if the unique type UUID has been well registered with the Type Registry.

### Component Factory (IFactory)

ECSS-E-ST-40-07\_1630355

The simulation environment shall provide a class implementing the IFactory interface as per IFactory.h in [SMP\_FILES].

ECSS-E-ST-40-07\_1630356

The IFactory GetUuid method shall return the UUID of the component that will be created by this factory.

ECSS-E-ST-40-07\_1630357

The IFactory CreateInstance method shall create an instance of the component with the following arguments:

“name” giving the name of the instance to be created;

“description” giving the description of the instance to be created;

“parent” giving a pointer to the parent object of the instance to be created.

ECSS-E-ST-40-07\_1630358

The IFactory DeleteInstance method shall delete an existing component with the following argument:

“instance” given the IComponent interface to the component to be deleted.

ECSS-E-ST-40-07\_1630359

The IFactory GetTypeName method shall return the fully qualified C++ type name of the component type.

1. The fully qualified type name contains all namespaces and the name of the type, separated by two colons ("::").

### Event loop requirements

#### General

The event loop corresponds to the main thread of the Simulation Environment that executes the simulation events and that updates the simulation time. A standard behaviour of the event loop can be specified. An event loop executes all time kind events when the simulator is in the Executing state. Another event loop executing only the Zulu time event must be considered when the simulator is in the Standby state.

#### Requirements

ECSS-E-ST-40-07\_1630360

In the simulator Executing state, one iteration of the Simulation Environment event loop shall execute the following sequence of actions:

Emit the PreSimTimeChange global event via the Event Manager;

Accept SetSimulationTime as per requirement5.3.2e;

Emit the PostSimTimeChange global event via the Event Manager;

Change Simulation Time to the current next event time;

Perform actions to maintain synchronization of simulation time with Zulu time;

While there are events scheduled at or before the current simulation or Zulu time, execute the event.

* 1. 1 to item 5: synchronisation between simulation time and Zulu time is necessary only if imposed by the simulation timing constraints, which are usually set by the simulation environment.
  2. 2 to item 5: how synchronization between simulation time and Zulu time is performed is outside the scope of this standard. For example, delays can be inserted in the event loop if simulation speed is too fast with regards to the Zulu time.
  3. 3 to item 6: event could be either immediate or simulation time, immediate events take priority over simulation time events.
  4. 4 to item 6: this while loop can be empty if events are removed during Pre/PostSimTimeChange. Same in the case where the SetEventSimulationTime is called to change the event execution time.

ECSS-E-ST-40-07\_1630361

In the simulator Standby state, one iteration of the Simulation Environment event loop shall perform the following sequence:

Wait to reach the time of the next scheduled Zulu time event;

While there are events scheduled at or before the current Zulu time, execute the Zulu time event.

1. In the Standby state, only Zulu time events are executed as specified in requirement 5.3.3w.

### Threading requirements

ECSS-E-ST-40-07\_1630362

Unless specified otherwise in the implementation, methods of Models shall be called from the simulation thread.

1. The simulation thread is the operating system thread that executes all EntryPoints scheduled through the Scheduler or subscribed through the EventManager.

ECSS-E-ST-40-07\_1630363

Methods of the Simulation Environment services, which are the Logger, Scheduler, TimeKeeper, Event Manager, Resolver and Link Registry may be called from any thread.

## Meta data

### Catalogue

#### File format specification

ECSS-E-ST-40-07\_1630364

The Catalogue file shall be in conformance with the Catalogue file DRD of Annex A.

#### Validation rules

##### General

ECSS-E-ST-40-07\_1630365

All user defined catalogues shall link to the SMP catalogue in file xml/ecss.smp.l1.smpcat in [SMP\_FILES] for all standard SMP elements defined in this standard.

* 1. 1 The ecss.smp.l1.smpcat contains the complete meta data model for all elements of [SMP\_FILES] expressed in an SMP catalogue.
  2. 2 The usage of a common standardized SMP catalogue ensures that common types and other elements have the same UUID across all platform, hence allows model integration.

ECSS-E-ST-40-07\_1630366

No recursive Types shall be specified.

1. Models, interfaces, entry points, fields, etc… are Types in the catalogue, so these Types cannot be typed as, be derived from or use themselves at any level of their specification.

ECSS-E-ST-40-07\_1630367

Types that are used in another Type shall be visible for that Type.

ECSS-E-ST-40-07\_1630368

XLinks in documents shall not result in recursively linked documents.

ECSS-E-ST-40-07\_1630369

The xlink:href attribute shall be a valid URI locator on the form "<Document>[#<Fragment>]", where <Document> is the linked XML file and <Fragment> is an optional named element defined in that file.

1. In case the named element is defined within the same file, i.e. the link is local to the file, the <Document> part of the locator can be omitted.

ECSS-E-ST-40-07\_1630370

The xlink:title attribute shall always contain the Name of the referenced named element.

##### Types

ECSS-E-ST-40-07\_1630371

The size of an array shall be a positive number.

ECSS-E-ST-40-07\_1630372

The PrimitiveType for a Float may only point to Float32 or Float64.

ECSS-E-ST-40-07\_1630373

Float Minimum shall be less than Float Maximum if MinInclusive is false or MaxInclusive is false.

ECSS-E-ST-40-07\_1630374

Float Minimum shall be less or equal to Float Maximum if MinInclusive is true and MaxInclusive is true.

ECSS-E-ST-40-07\_1630375

The length of a string shall be larger or equal to zero.

ECSS-E-ST-40-07\_1630376

The length of a String Value shall not exceed the size of the corresponding String type.

ECSS-E-ST-40-07\_1630377

The PrimitiveType for an Integer shall point to Int8, Int16, Int32, Int64, UInt8, UInt16, UInt32 or UInt64.

ECSS-E-ST-40-07\_1630378

For Integer types, the Minimum shall be less or equal to the Integer Maximum.

ECSS-E-ST-40-07\_1630379

The type for an AttributeType shall point to a ValueType.

ECSS-E-ST-40-07\_1630380

The Type link for an Attribute shall point to an AttributeType.

ECSS-E-ST-40-07\_1630381

The default value of an AttributeType shall be not empty.

ECSS-E-ST-40-07\_1630382

The Value of an Attribute shall not be empty.

##### Named Element

ECSS-E-ST-40-07\_1630383

A Named Element Name shall be unique in its context.

ECSS-E-ST-40-07\_1630384

A Named Element Id shall be unique in its Document.

ECSS-E-ST-40-07\_1630385

A Named Element Id shall not be empty.

ECSS-E-ST-40-07\_1630386

A Named Element Name shall not be an ISO/ANSI C++ keyword.

ECSS-E-ST-40-07\_1630387

A Named Element Name shall only contain letters, digits, and the underscore.

ECSS-E-ST-40-07\_1630388

A Type UUID shall be unique.

##### Container and associations

ECSS-E-ST-40-07\_1630389

A Container lower bound shall be a positive number or 0.

ECSS-E-ST-40-07\_1630390

A Container lower bound shall be less or equal to the container upper bound, if present.

ECSS-E-ST-40-07\_1630391

A Container upper bound shall be ‐1 or larger or equal to the container lower bound.

ECSS-E-ST-40-07\_1630392

The Type link of an Association shall point to a Language Type.

ECSS-E-ST-40-07\_1630393

The Type link of a Container shall point to a Reference Type.

ECSS-E-ST-40-07\_1630394

The Type link of a Reference shall point to an Reference Type.

##### Enumeration

ECSS-E-ST-40-07\_1630395

Enumeration Literal Names shall be unique within an Enumeration.

ECSS-E-ST-40-07\_1630396

Enumeration Literal Values shall be unique within an Enumeration.

##### Entry Point

ECSS-E-ST-40-07\_1630397

Entry Point Output fields shall be output type fields.

ECSS-E-ST-40-07\_1630398

Entry Point Input fields shall be input type fields.

ECSS-E-ST-40-07\_1630399

Entry Point Input and Output fields shall be located in the same Model or a base model.

##### Properties

ECSS-E-ST-40-07\_1630400

A Property’s Attached Field shall have the type of Property’s Type, or a type derived thereof.

ECSS-E-ST-40-07\_1630401

A Property’s Attached Field shall be located in the same Class or a base class.

ECSS-E-ST-40-07\_1630402

The Type link of a Property shall point to a Language Type.

ECSS-E-ST-40-07\_1630403

A Property of an Interface shall be public.

ECSS-E-ST-40-07\_1630404

A Property of an Interface shall not be static.

##### References

ECSS-E-ST-40-07\_1630405

A Reference lower bound shall be larger than zero.

ECSS-E-ST-40-07\_1630406

A Reference lower bound shall be less or equal to Reference upper bound, if present.

ECSS-E-ST-40-07\_1630407

A Reference upper bound shall be ‐1, larger or equal to Reference lower bound.

##### Fields

ECSS-E-ST-40-07\_1630408

The Type link for a Field shall point to a ValueType.

ECSS-E-ST-40-07\_1630409

A Field of a Structure shall be public.

##### Operations

ECSS-E-ST-40-07\_1630410

An Operation of an Interface shall be public.

ECSS-E-ST-40-07\_1630411

An Operation of an Interface shall not be static.

ECSS-E-ST-40-07\_1630412

The Type link of a Parameter of the Operation shall point to a Language Type.

ECSS-E-ST-40-07\_1630413

The value of a parameter shall be inside the range defined for the corresponding type.

ECSS-E-ST-40-07\_1630414

Each operation shall have only one parameter with the return type attribute set.

##### Constructors

ECSS-E-ST-40-07\_1630415

Constructors shall not have any return parameters.

ECSS-E-ST-40-07\_1630416

Constructors shall not have Const, Virtual or Static attributes.

##### Events

ECSS-E-ST-40-07\_1630417

The EventArgs link for an EventType shall only point to a SimpleType.

ECSS-E-ST-40-07\_1630418

The Type link of an EventSource shall point to an EventType.

ECSS-E-ST-40-07\_1630419

The Type link of an EventSink shall point to an EventType.

#### Requirements on utilization of Catalogue

ECSS-E-ST-40-07\_1630420

The design of simulation Models and related Sub-Elements shall be defined via a catalogue, or a set of catalogues when their use is required in model exchange.

1. For example, model catalogues provide information about Fields and Properties that can be configured for a given model in a simulator.

ECSS-E-ST-40-07\_1630421

Catalogues shall not have circular dependencies.

ECSS-E-ST-40-07\_1630422

Each Model in a simulation shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630423

Each user-defined Service in a simulator shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630424

Each Interface between components shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630425

Each Type used in an interface or component shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630426

Each Field of a model or service that is of a type defined in a catalogue shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630427

Each public Property of an interface, model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630428

Each public Operation of an interface, model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630429

Each Entry Point of a model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630430

Each Event Source of a model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630431

Each Event Sink of a model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630432

Each Container of a model or service shall be defined in a catalogue.

ECSS-E-ST-40-07\_1630433

Each Reference of a model or service shall be defined in a catalogue.

### Package

#### File format specification

ECSS-E-ST-40-07\_1630434

The Package file shall be in conformance with the Package file DRD of Annex B.

#### Validation rules

ECSS-E-ST-40-07\_1630435

There shall be no clashes of Type names in packages.

ECSS-E-ST-40-07\_1630436

For each Model implementation, a different UUID shall be used.

### Configuration data

#### File format

ECSS-E-ST-40-07\_1630437

Files containing configuration data for published fields should be in conformance with the Configuration file DRD of Annex C.

1. The usage of the SMP Configuration file format is optional.

#### Validation rules

ECSS-E-ST-40-07\_1630438

All path strings in configuration files shall be valid SMP path strings.

1. Valid SMP path strings are specified in clause 5.1.3

ECSS-E-ST-40-07\_1630439

All field values set shall be valid values for the field type it refers to.

ECSS-E-ST-40-07\_1630440

All path strings in configuration files shall identify either a simple field, or an array item of a simple array field.

1. For a simple field, the Resolver can resolve the path. For an item of a simple array field, the Resolver can only resolve the array field.

# Implementation mapping

## C/C++ Standard

### General

Although only the C++ mapping is relevant for this standard, C has to be considered as well because C and C++ syntax and keywords (important for e.g. choosing correct SMP object names) are in general identical.

This standard is not bound to a specific C/C++ standard version. It requires only that the used C and C++ standard versions are at least resp. C11 (ISO/IEC 9899:2011) and C++ 11 (ISO/IEC 14882:2011).

In the [SMP\_FILES], indication is given for the C++ standard versions that these C++ header files are compatible with.

In practice, the C++ standard version and the C standard version (the latter if relevant), have to be defined and agreed between exchange partners at the level of the simulation project, that is using this standard.

### Requirements

ECSS-E-ST-40-07\_1630441

The C++ standard version relevant to SMP shall be at least C++11 as per ISO/IEC 14882:2011.

ECSS-E-ST-40-07\_1630442

The C standard version relevant to SMP shall be at least C11 as per ISO/IEC 9899:2011.

ECSS-E-ST-40-07\_1630443

The C/C++ standard versions used in SMP projects shall be defined and agreed on a project basis.

## Catalogue to C++

### Mapping templates

1. Syntax and expression rules used in the specification of C++ mapping templates:
   1. Parts omitted to shorten the template and ease the reading are replaced by ‘…’.
   2. Information from the catalogue to be mapped in the C++ code is specified by means of placeholders encased within dollar ‘$’ symbols. For example, $Component.Name$ for the value of the field ‘Name’ of some ‘Component’ element referred in the context the template is applicable. In case an element belongs in a sequence with a number ‘N’ of occurrences, $...Element[i]...$ refers to the ‘i-th’ occurrence of the sequence where ‘i’ could take any value between ‘1’ and ‘N-1’.
   3. Fully qualified names for types are specified by means of the ‘TypeName($Type$)’ expression. For example, for a given type ‘MyType’ defined within two levels of nested namespaces would refer to ‘::Namespace1::Namespace2::MyType’.
   4. Optional code is specified encased within the square bracket ‘[‘ and ‘]’ symbols. For example, ‘[static]’ where the use of ‘static’ might be subject to some conditions. Exception is where ‘[...]’ is used for the elements in an array as per rule a.2. above.
   5. Alternative code is specified by means of the ‘|’ separator symbol where exactly one of several options is required. For example, ‘A|B|C’ if either ‘A’, ‘B’ or ‘C’ is to be used in the code.
2. Table 6‑1 and Table 6‑2 contain the C++ declaration and defintition templates and are referred to from requirements of clause 6.1.

ECSS-E-ST-40-07\_1630444

Table 6‑1: C++ declaration templates

| Template | C++ mapping |
| --- | --- |
| Constant | static constexpr|const TypeName($Constant.Type$) $Constant.Name$ = $Constant.Value$; |
| Field | [static ][mutable ]TypeName($Field.Type$) $Field.Name$; |
| Association | [const ][static ][mutable ]TypeName($Association.Type$)[\*] $Association.Name$; |
| Parameter | [const ]TypeName($Parameter.Type$)[\*|&] $Parameter.Name$[ = $Parameter.Default$] |
| Property Getter | [virtual ] [static ][const ]TypeName($Property.Type$)[\*|&] get\_$Property.Name$()[ const][ = 0]; |
| Property Setter | [virtual ][static ]void set\_$Property.Name$([const ]TypeName($Property.Type$)[\*|&] value)[ = 0]; |
| Operation | [virtual ][static ] void|TypeName($Operation.Parameter[i].Type$)[\*|&] $Operation.Name$(void|...)[ const][ = 0]; |
| Operator | [virtual ][static ] void|TypeName($Operation.Parameter[i].Type$)[\*|&] operator $Operation.Operator.OperatorKind$(void|...)[ const][ = 0]; |
| Constructor | $Owner.Name$(void|...)[= delete]; |
| Entry Point | Smp::IEntryPoint\* $EntryPoint.Name$; |
| Event Sink | Smp::IEventSink\* $EventSink.Name$; |
| Event Source | Smp::IEventSource\* $EventSource.Name$; |
| Container | Smp::IContainer\* $Container.Name$; |
| Reference | Smp::IReference\* $Reference.Name$; |
| Uuid | extern const Smp::Uuid Uuid\_$Type.Name$; |
| Global Registry | [static] void \_Register\_$Type.Name$( Smp::Publication::ITypeRegistry\* registry); |
| Scoped Registry | [static] void \_Register( Smp::Publication::ITypeRegistry\* registry); |
| Enumeration | enum class $Enumeration.Name$ : Smp::Int32 { ... }; |
| Literal | $Enumeration.Literal.Name$ = $Enumeration.Literal.Value$; |
| Integer | typedef $Integer.PrimitiveType$|Smp::Int32 $Integer.Name$; |
| Float | typedef $Float.PrimitiveType$|Smp::Float64 $Float.Name$; |
| String | struct $String.Name$ { Smp::Char8 internalString[$String.Length$+1]; }; |
| Array | struct $Array.Name$ { TypeName($Array.ItemType$) internalArray[$Array.Size$]; }; |
| Structure | struct $Structure.Name$ { ... }; |
| Class | class $Class.Name$ [ : public TypeName($Class.Base.Name$)] { ... }; |
| Exception | class $Exception.Name$ :  public TypeName($Exception.Base.Name$)|Smp::Exception { ... }; |
| Interface | class $Interface.Name$ [ : virtual public TypeName($Interface.Base[1].Name$),  ...,  TypeName($Interface.Base[N].Name$)] { ... }; |
| Model | class $Model.Name$ : [ public TypeName($Model.Base.Name$),] [ virtual public TypeName($Model.Interface[1].Name$),  ...,  TypeName($Model.Interface[N].Name$),] [ virtual public Smp::IEntryPointPublisher,] [ virtual public Smp::IEventConsumer,] [ virtual public Smp::IEventProvider,] [ virtual public Smp::IComposite,] [ virtual public Smp::IAggregate,]  [ virtual public Smp:: IFallibleModel,] virtual public Smp::IModel { ... }; |
| Service | class $Service.Name$ : [ public TypeName($Service.Base.Name$),] [ virtual public TypeName($Service.Interface[1].Name$),  ...,  TypeName($Service.Interface[N].Name$),] [ virtual public Smp::IEntryPointPublisher,] [ virtual public Smp::IEventConsumer,] [ virtual public Smp::IEventProvider,] virtual public Smp::IService { ... }; |

ECSS-E-ST-40-07\_1630445

Table 6‑2: C++ definition templates

| Template | C++ mapping |
| --- | --- |
| Uuid | Smp::Uuid Uuid\_$Type.Name$ = $Type.Uuid$; |
| Simple | TypeName($Variable.Type$) $Variable.Name$ = $Variable.Value.Value$|$Variable.Value.Literal$; |
| Array | TypeName($Variable.Type$) $Variable.Name$ = {{ $Variable.ItemValue[1].Value$|$Variable.ItemValue[1].Literal$, ..., $Variable.ItemValue[N].Value$|$Variable.ItemValue[N].Literal$ }}; |
| Structure | TypeName($Variable.Type$) $Variable.Name$ = { $Variable.FieldValue[1].Value$|$Variable.FieldValue[1].Literal$, ..., $Variable.FieldValue[N].Value$|$Variable.FieldValue[N].Literal$ }; |
| Property Getter | return $Property.AttachedField.Name$; |
| Property Setter | $Property.AttachedField.Name$ = value; |

### Namespaces and files

ECSS-E-ST-40-07\_1630446

All elements shall be declared within the exact same namespace as in the Catalogue.

ECSS-E-ST-40-07\_1630447

Each type shall be declared in a dedicated header file as follows:

The hierarchy of namespaces defines the file location with one directory level per namespace level in the hierarchy;

The type name defines the file name.

ECSS-E-ST-40-07\_1630448

Header files shall allow multiple inclusion by implementing ‘#include’ guards.

ECSS-E-ST-40-07\_1630449

Header files shall avoid circular dependencies by using forward declaration.

### Element and Type Visibility Kind

ECSS-E-ST-40-07\_1630450

Visibility kind attributes shall be mapped to ISO/ANSI C++ member access specifiers as follows:

If the attribute is explicitly defined, mapping is as per Table 6‑3;

If the attribute is undefined, the default “Private” visibility kind is used with mapping as per Table 6‑3.

ECSS-E-ST-40-07\_1630451

Table 6‑3: C++ mapping for the Visibility kind attribute

| Visibility kind | Description | C++ mapping |
| --- | --- | --- |
| Private | Local to the parent Type. | private |
| Protected | Local to the parent Type and derived Types thereof. | protected |
| Public | Global. | public |

### Mapping of elements

#### Value elements

ECSS-E-ST-40-07\_1630452

Simple value elements shall be mapped to ISO/ANSI C++ variable’s values as follows:

Syntax as per “Simple” template in Table 6‑2;

If the element value is of EnumerationValue type, mapping is done using the Literal attribute instead of the Value one.

ECSS-E-ST-40-07\_1630453

Array value elements shall be mapped to ISO/ANSI C++ variable’s values as follows:

Syntax as per “Array” template in Table 6‑2;

If the element items are of EnumerationValue type, mapping is done using their Literal attribute instead of the Value one.

ECSS-E-ST-40-07\_1630454

Structure value elements shall be mapped to ISO/ANSI C++ variable’s values as follows:

Syntax as per “Structure” template in Table 6‑2;

For the element fields of EnumerationValue type, mapping is done using the Literal attribute instead of the Value one.

#### Constant

ECSS-E-ST-40-07\_1630455

Constant elements shall be mapped to ISO/ANSI C++ member variables as per “Constant” template in Table 6‑1.

ECSS-E-ST-40-07\_1630456

The value of the Constant member variable shall be defined as per mapping of the Value attribute.

1. See clause 6.2.4.1 for details on the mapping of Value attributes.

ECSS-E-ST-40-07\_1630457

The access specifier of the Constant member variable shall be defined as follows:

If the member variable belongs in a C++ structure, the member is public;

If the member variable does not belong in a C++ structure, the mapping of the Visibility attribute is used.

* 1. 1 See clause 6.2.3 for details on the mapping of Visibility attributes.
  2. 2 The access specifier applies to Classes, Models, Services and Interfaces.

#### Field

ECSS-E-ST-40-07\_1630458

Field elements shall be mapped to ISO/ANSI C++ member variables as per “Field” template in Table 6‑1.

ECSS-E-ST-40-07\_1630459

The initial value of the Field member variable shall be defined as per mapping of the Default attribute.

1. See clause 6.2.4.1 for details on the mapping of Value attributes.

ECSS-E-ST-40-07\_1630460

The access specifier of the Field member variable shall be defined as follows:

If the member variable belongs in a C++ structure, the member is public;

If the member variable does not belong in a C++ structure, the mapping of the Visibility attribute is used.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630461

The Static attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Field C++ mapping:

If set to “true”, then the C++ field includes the ‘static’ specifier as per “Field” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630462

The Mutable attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Field C++ mapping:

If set to “true”, then the C++ field includes the ‘mutable’ specifier as per “Field” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

#### Association

ECSS-E-ST-40-07\_1630463

Association elements shall be mapped to ISO/ANSI C++ member variables as per “Association” template in Table 6‑1;

ECSS-E-ST-40-07\_1630464

The access specifier of the Association member variable shall be defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630465

The ByPointer attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Association C++ mapping:

If set to “true”, then the C++ mapping of the type includes the ‘\*’ specifier as per “Association” template in Table 6‑1;

If not set, then the C++ mapping of the type includes the specifier corresponding to the type referenced in the Type attribute as per Table 6‑4;

If set to “false”, then the C++ mapping of the type does not include the ‘\*’ specifier.

ECSS-E-ST-40-07\_1630466

Table 6‑4: C++ mapping of Association depending on ByPointer attribute

|  | C++ mapping | | | |
| --- | --- | --- | --- | --- |
| **Native Type** | **Value Type** | **Value Reference** | **Reference Type** |
| Specifier without ByPointer |  |  |  | \* |
| Specifier with ByPointer=”true” | \* | \* | \* | \* |
| Specifier with ByPointer=”false” |  |  |  |  |

ECSS-E-ST-40-07\_1630467

The Const attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Association C++ mapping:

If set to “true”, then the C++ mapping includes the ‘const’ specifier as per “Association” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630468

The Static attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Association C++ mapping:

If set to “true”, then the C++ mapping includes the ‘static’ specifier as per “Association” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630469

The Mutable attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Association C++ mapping:

If set to “true”, then the C++ mapping includes the ‘mutable’ specifier as per “Association” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

#### Parameter

ECSS-E-ST-40-07\_1630470

Parameter elements shall be mapped to ISO/ANSI C++ as follows:

If the Direction kind attribute is ‘return’, the parameter is the return type of a C++ member method;

If the Direction kind attribute is not ‘return’, the parameter is an argument of a C++ member method with default value given by the Default attribute;

Syntax is for arguments as per “Parameter” and for the return type as per “Operation” templates in Table 6‑1;

For the C++ type specifier the mapping of the Direction kind attribute corresponding to the type referenced in the Type attribute as per Table 6‑5 is used.

1. to item 2: the Default attribute must contain a valid C++ expression for assigning a default value to a C++ method parameter. As it will be rendered unchanged in the generated C++ code, its content will be validated directly by the C++ compiler. For example, the Default attribute can be the C++ “nullptr” keyword.

ECSS-E-ST-40-07\_1630471

Table 6‑5: C++ mapping for the Direction kind attribute

| Direction kind | C++ mapping | | | |
| --- | --- | --- | --- | --- |
| **Native Type** | **Value Type** | **Value Reference** | **Reference Type** |
| in |  |  | const | const & |
| out | \* | \* |  | \* |
| inout | \* | \* |  | \* |
| return |  |  |  | \* |

ECSS-E-ST-40-07\_1630472

The ByReference attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Parameter C++ mapping:

If set to “true”, then the C++ mapping includes the ‘&’ specifier as per “Parameter” template in Table 6‑1, irrespectively of Table 6‑5;

If not set, then the C++ mapping is done according to Table 6‑5;

If set to “false”, then the C++ mapping does not include the ‘&’ specifier, irrespectively of Table 6‑5.

ECSS-E-ST-40-07\_1630473

The Const attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Parameter C++ mapping:

If set to “true”, then the C++ mapping includes the ‘const’ specifier as per “Parameter” template in Table 6‑1, irrespectively of Table 6‑5;

If not set, then the C++ mapping is done according to Table 6‑5;

If set to “false”, then the C++ mapping does not include the ‘const’ specifier, irrespectively of Table 6‑5.

ECSS-E-ST-40-07\_1630474

The ByPointer attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Parameter C++ mapping:

If set to “true”, then the C++ mapping includes the ‘\*’ specifier as per “Parameter” template in Table 6‑1, irrespectively of Table 6‑5;

If not set, then the C++ mapping is done according to Table 6‑5;

If set to “false”, then the C++ mapping does not include the ‘\*’ specifier, irrespectively of Table 6‑5.

1. It is invalid to have both the ByReference attribute and the ByPointer attribute set to ”true” for the same parameter.

#### Property

ECSS-E-ST-40-07\_1630475

Property elements shall be mapped to ISO/ANSI C++ member methods as follows:

If the Access attribute is not defined, or it is defined with value equal to ‘readWrite’ or ‘readOnly’, a getter member method is created with syntax as per “Property Getter” template in Table 6‑1;

If the Access attribute is not defined, or it is defined with value equal to ‘readWrite’ or ‘writeOnly’, a setter member method is created with syntax as per “Property Setter” template in Table 6‑1;

ECSS-E-ST-40-07\_1630476

The access specifier of the Property member methods shall be defined as follows:

If the Operation belongs in an Interface, the member is public;

If the Operation does not belong in an Interface, the mapping of the Visibility attribute is used.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630477

If the AttachedField element is defined, the body of the Property getter and setter member methods shall be respectively mapped as per “Property Getter” and “Property Setter” templates in Table 6‑2.

ECSS-E-ST-40-07\_1630478

The ByReference attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping of the type includes the ‘&’ specifier;

If not set, or if set to “false”, then the C++ mapping of the type does not include the ‘&’ specifier.

ECSS-E-ST-40-07\_1630479

The ByPointer attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping of the type includes the ‘\*’ specifier;

If not set, then the C++ mapping of the type includes the specifier corresponding to the type referenced in the Type attribute as per Table 6‑6;

If set to “false”, then the C++ mapping of the type does not include the ‘\*’ specifier.

ECSS-E-ST-40-07\_1630480

Table 6‑6: C++ mapping for Property depending on ByPointer attribute

|  | C++ mapping | | | |
| --- | --- | --- | --- | --- |
| **Native Type** | **Value Type** | **Value Reference** | **Reference Type** |
| Specifier without ByPointer |  |  |  | \* |
| Specifier with ByPointer=”true” | \* | \* | \* | \* |
| Specifier with ByPointer=”false” |  |  |  |  |

ECSS-E-ST-40-07\_1630481

The Static attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping includes the ‘static’ specifier as per “Property Getter” and “Property Setter” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630482

The Virtual attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping includes the ‘virtual’ specifier as per “Property Getter” and “Property Setter” template in Table 6‑1;

If not set, then the C++ mapping includes the ‘virtual’ specifier as per “Property Getter” and “Property Setter” template in Table 6‑1 if the property belongs to an Interface, Model or Service and is not static;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630483

The Abstract attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping includes the ‘=0’ pure specifier as per “Property Getter” and “Property Setter” template in Table 6‑1;

If not set, then the C++ mapping includes the ‘=0’ pure specifier as per “Property Getter” and “Property Setter” template in Table 6‑1 if the property belongs to an Interface;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630484

The ConstGetter attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping includes the ‘const’ specifier at the end, as per “Property Getter” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630485

The Const attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Property C++ mapping:

If set to “true”, then the C++ mapping includes the ‘const’ specifier at the beginning, as per “Property Getter” and "Property Setter" templates in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

#### Operation

ECSS-E-ST-40-07\_1630486

Operation elements shall be mapped to ISO/ANSI C++ member methods as follows:

If neither the Operator nor the Constructor attribute is set, syntax is as per “Operation” template in Table 6‑1;

If the Operator attribute is set, syntax is as per “Operator” template in Table 6‑1;

If the Constructor attribute is set, syntax is as per “Constructor” template in Table 6‑1.

* 1. 1 Operator and Constructor attributes cannot be both set at the same time for a given Operation element as they are mutually exclusive.
  2. 2 Constructor methods inherit the name from the element the Operation is member of, therefore their own Name attribute is ignored.

ECSS-E-ST-40-07\_1630487

Operation elements shall have at maximum one Parameter element, or none in case the Constructor attribute is set, with Direction attribute equal to ‘return’.

ECSS-E-ST-40-07\_1630488

Parameter elements belonging to the Operation element shall be mapped as follows:

Syntax as per mapping of Parameter elements;

If there is no Parameter element with Direction attribute equal to ‘return’, the return type of the Operation member method is ‘void’;

If there is no Parameter element with Direction attribute different than ‘return’, the only argument of the Operation member method is ‘void’;

If there is more than one Parameter element with Direction attribute different than ‘return’, they are mapped in sequence as comma-separated arguments for the Operation member method.

1. See clause 6.2.4.5 for details on the mapping of Parameter elements.

ECSS-E-ST-40-07\_1630489

The access specifier of the Operation C++ member method shall be defined as follows:

If the Operation belongs in an Interface, the member is public;

If the Operation does not belong in an Interface, the mapping of the Visibility attribute is used.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630490

The Static attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Operation C++ mapping:

If set to “true”, then the C++ mapping includes the ‘static’ specifier as per “Operation” or “Operator” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

1. Constructor methods are not affected by the Static attribute.

ECSS-E-ST-40-07\_1630491

The Virtual attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Operation C++ mapping:

If set to “true”, then the C++ mapping includes the ‘virtual’ specifier as per “Operation” or “Operator” template in Table 6‑1;

If not set, then the C++ mapping includes the ‘virtual’ specifier as per “Operation” or “Operator” template in Table 6‑1 if the Operation belongs to an Interface, Model or Service and is not static;

If set to “false”, then it has no effect.

1. Constructor methods are not affected by the Virtual attribute.

ECSS-E-ST-40-07\_1630492

The Abstract attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Operation C++ mapping:

If set to “true”, then the C++ mapping includes the ‘=0’ pure specifier as per “Operation” or “Operator” template in Table 6‑1;

If not set, then the C++ mapping includes the ‘=0’ pure specifier as per “Operation” or “Operator” template in Table 6‑1 if the Operation belongs to an Interface;

If set to “false”, then it has no effect.

1. Constructor methods are not affected by the Abstract attribute.

ECSS-E-ST-40-07\_1630493

The Const attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Operation C++ mapping:

If set to “true”, then the C++ mapping includes the ‘const’ specifier as per “Operation” or “Operator” template in Table 6‑1;

If not set, then it has no effect;

If set to “false”, then it has no effect.

1. Constructor methods are not affected by the Const attribute.

ECSS-E-ST-40-07\_1630494

The Operator attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Operation C++ mapping:

If set, then the C++ mapping of the Operator kind referenced in the Operator attribute as per Table 6‑7 is used;

If not set, it has no effect.

ECSS-E-ST-40-07\_1630613

Table 6‑7: C++ mapping for the Operator attribute kinds

| Operator kind | Description | C++ mapping |
| --- | --- | --- |
| None | Undefined. |  |
| Positive | Positive value of instance. | +x |
| Negative | Negative value of instance. | -x |
| Assign | Assigns new value to instance. | x = a |
| Add | Adds value to instance. | x += a |
| Subtract | Subtracts value to instance. | x -= a |
| Multiply | Multiplies instance with value. | x \*= a |
| Divide | Divides instance by value. | x /= a |
| Remainder | Remainder of instance for value. | x %= a |
| Greater | Compares whether instance is greater than value. | x > a |
| Less | Compares whether instance is less than value. | x < a |
| Equal | Compares whether instance is equal to value. | x == a |
| NotGreater | Compares whether instance is not greater than value. | x <= a |
| NotLess | Compares whether instance is not less than value. | x >= a |
| NotEqual | Compares whether instance is not equal to value. | x != a |
| Indexer | Returns indexed value of instance. | x[a] |
| Sum | Returns sum of two values. | a + b |
| Difference | Returns difference of two values. | a - b |
| Product | Returns product of two values. | a \* b |
| Quotient | Returns quotient of two values. | a / b |
| Module | Returns remainder of two values. | a % b |

#### EntryPoint

ECSS-E-ST-40-07\_1630495

EntryPoint elements shall be mapped to ISO/ANSI C++ member pointer variables as per “EntryPoint” template in Table 6‑1.

ECSS-E-ST-40-07\_1630496

The access specifier of the EntryPoint member variable shall be public.

ECSS-E-ST-40-07\_1630497

The EntryPoint member variable shall point to an implementation of the Smp::IEntryPoint interface.

#### EventSink

ECSS-E-ST-40-07\_1630498

EventSink elements shall be mapped to ISO/ANSI C++ member pointer variables as per “EventSink” template in Table 6‑1.

ECSS-E-ST-40-07\_1630499

The access specifier of the EventSink member variable shall be public.

ECSS-E-ST-40-07\_1630500

The EventSink member variable shall point to an implementation of the Smp::IEventSink interface.

ECSS-E-ST-40-07\_1630501

If the EventType of an EventSink has an EventArgs, the implementation of the Notify method of the Smp::IEventSink interface shall expect to receive an “arg” parameter of simple type as defined by the type of the EventArgs.

1. See clause 5.2.6.1 for the details of the Notify method of the Smp::IEventSink interface.

#### EventSource

ECSS-E-ST-40-07\_1630502

EventSource elements shall be mapped to ISO/ANSI C++ member pointer variables as per “EventSource” template in Table 6‑1.

ECSS-E-ST-40-07\_1630503

The access specifier of the EventSource member variable shall be public.

ECSS-E-ST-40-07\_1630504

The EventSource member variable shall point to an implementation of the Smp::IEventSource interface.

ECSS-E-ST-40-07\_1630505

If the EventType of an EventSource has an EventArgs, the implementation of the Emit method of the Smp::IEventSource interface shall expect to pass an “arg” parameter of simple type as defined by the type of the EventArgs.

1. See clause 5.2.6.2 for the details of the Emit method of the Smp::IEventSource interface.

#### Container

ECSS-E-ST-40-07\_1630506

Container elements shall be mapped to ISO/ANSI C++ member pointer variables as per “Container” template in Table 6‑1.

ECSS-E-ST-40-07\_1630507

The access specifier of the Container member variable shall be public.

ECSS-E-ST-40-07\_1630508

The Container member variable shall point to an implementation of the Smp::IContainer interface.

ECSS-E-ST-40-07\_1630509

If the Type element of the Container points to a reference type, then the implementation of the AddComponent method of the Smp::IContainer interface shall expect the component parameter to be derived from this Type.

1. See clause 5.2.5.2 for the details of the AddComponent method of the Smp::IContainer interface.

#### Reference

ECSS-E-ST-40-07\_1630510

Reference elements shall be mapped to ISO/ANSI C++ member pointer variables as per “Reference” template in Table 6‑1.

ECSS-E-ST-40-07\_1630511

The access specifier of the Reference member variable shall be public.

ECSS-E-ST-40-07\_1630512

The Reference member variable shall point to an implementation of the Smp::IReference interface.

ECSS-E-ST-40-07\_1630513

If the Type element of the Reference points to a reference type, then the implementation of the AddComponent method of the Smp::IReference interface shall expect the component parameter to be derived from this Type.

1. See clause 5.2.4.2 for the details of the AddComponent method of the Smp::IReference interface.

### Basic Value Types

#### Common specification

ECSS-E-ST-40-07\_1630514

For each type, a universally unique identifier (UUID) variable shall be declared as per “Uuid” template in Table 6‑1.

ECSS-E-ST-40-07\_1630515

The value of the universally unique identifier (UUID) variable shall be defined as per “Uuid” template in Table 6‑2.

ECSS-E-ST-40-07\_1630516

For each type, a method to register the type in the registry shall be defined as per “Global Registry” template in Table 6‑1.

ECSS-E-ST-40-07\_1630517

If the type belongs to a Reference Type, the access specifier of the C++ member variables, types and methods related to the type shall be defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

#### Enumeration

ECSS-E-ST-40-07\_1630518

Enumeration types shall be mapped to ISO/ANSI C++ enumerated types as per “Enumeration” template in Table 6‑1.

ECSS-E-ST-40-07\_1630519

Literal elements shall be mapped to ISO/ANSI C++ enumeration literals with value assignment as per “Literal” template in Table 6‑1.

ECSS-E-ST-40-07\_1630520

Literal elements shall be declared within the exact same Enumeration type as in the Catalogue.

#### Integer

ECSS-E-ST-40-07\_1630521

Integer types shall be mapped to ISO/ANSI C++ type definitions as follows:

Syntax is as per “Integer” template in Table 6‑1;

If it references a specific type, the same is used for the declaration;

If it does not reference a type, the default Int32 primitive type as per Table 5‑1 is used for the declaration.

#### Float

ECSS-E-ST-40-07\_1630522

Float types shall be mapped to ISO/ANSI C++ type definitions as follows:

Syntax is as per “Float” template in Table 6‑1;

If it references a specific type, the same is used for the declaration;

If it does not reference a type, the default Float64 primitive type as per Table 5‑1 is used for the declaration.

#### String

ECSS-E-ST-40-07\_1630523

String types shall be mapped to ISO/ANSI C++ structures as per “String” template in Table 6‑1.

1. Using a structure with a single internalString array field (rather than using an array) allows passing String types by value.

ECSS-E-ST-40-07\_1630524

Values of String Type shall be mapped to ISO/ANSI C++ as null-terminated const char\* strings ("C strings") with UTF-8 encoding.

#### Array

ECSS-E-ST-40-07\_1630525

Array types shall be mapped to ISO/ANSI C++ structures as per “Array” template in Table 6‑1.

1. Using a structure with a single internalArray array field (rather than using an array) allows passing Array types by value.

### Compound Value Types

#### Common specification

ECSS-E-ST-40-07\_1630526

For each type, a universally unique identifier (UUID) variable shall be declared as per “Uuid” template in Table 6‑1.

ECSS-E-ST-40-07\_1630527

The value of universally unique identifier (UUID) variables shall be defined as per “Uuid” template in Table 6‑2.

ECSS-E-ST-40-07\_1630528

For each type, a method to register the type in the registry shall be defined as follows:

Syntax is as per “Scoped Registry” template in Table 6‑1;

Method is declared as member of the C++ structure or class the type is mapped to.

ECSS-E-ST-40-07\_1630529

Constant and Field elements belonging to the type shall be mapped within the exact same C++ structure or class the type is mapped to.

1. See clause 6.2.4.1c.2 for details on the mapping of Constant elements and clause 6.2.4.3 for details on the mapping of Field elements.

ECSS-E-ST-40-07\_1630530

If the type belongs to a Reference Type, the access specifier of the C++ member variables, types and methods related to the type shall be defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

#### Structure

ECSS-E-ST-40-07\_1630531

Structure types shall be mapped to ISO/ANSI C++ structures as per “Structure” template in Table 6‑1.

#### Class

ECSS-E-ST-40-07\_1630532

Class types shall be mapped to ISO/ANSI C++ classes as follows:

Syntax as per “Class” template in Table 6‑1;

If the Base element is defined, the class inherits from the Base class.

ECSS-E-ST-40-07\_1630533

Class types shall have a default constructor whose access specifier is defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630534

Class types shall have a virtual destructor with the noexcept keyword whose access specifier is defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630535

If the Class type has the NoConstructor attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] set to "true", the constructor shall be declared with the delete keyword.

ECSS-E-ST-40-07\_1630536

If the Class type has the NoDestructor attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] set to "true", the destructor shall be declared with the default keyword.

ECSS-E-ST-40-07\_1630537

Association, Property and Operation elements belonging to the Class type shall be mapped within the exact same C++ class the type is mapped to.

1. See clause 6.2.4.4 for details on the mapping of Association elements, clause 6.2.4.6 for details on the mapping of Property elements and clause 6.2.4.7 for details on the mapping of Operation elements.

ECSS-E-ST-40-07\_1630538

If the Class type has the Abstract attribute set to “true”, the destructor shall be declared as pure virtual.

ECSS-E-ST-40-07\_1630539

The BaseClass attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Class C++ mapping:

If set, then the class includes an inheritance link to the base class that the attribute points to;

If not set, then it has no effect.

#### Exception

ECSS-E-ST-40-07\_1630540

Exception types shall be mapped to ISO/ANSI C++ classes as follows:

Syntax as per “Exception” template in Table 6‑1;

If the Base element is defined, the class inherits from the Base class;

If the Base element is not defined, the class inherits from the default Exception class.

ECSS-E-ST-40-07\_1630541

Exception classes shall have a default constructor whose access specifier is defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630542

Exception classes shall have a copy constructor whose access specifier is defined by the mapping of the Visibility attribute.

* 1. 1 Copy constructors are required to be able to catch exceptions by value.
  2. 2 See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630543

Exception classes shall have a virtual destructor whose access specifier is defined by the mapping of the Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

ECSS-E-ST-40-07\_1630544

Association, Property and Operation elements belonging to the Exception type shall be mapped within the exact same C++ class the type is mapped to.

1. See clause 6.2.4.4 for details on the mapping of Association elements, clause 6.2.4.6 for details on the mapping of Property elements and clause 6.2.4.7 for details on the mapping of Operation elements.

ECSS-E-ST-40-07\_1630545

If the Exception type has the Abstract attribute set to “true”, the destructor shall be declared as pure virtual.

ECSS-E-ST-40-07\_1630546

The BaseClass attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Exception C++ mapping:

If set, then the Exception includes an inheritance link to the base class that the attribute points to;

If not set, then it has no effect.

### Reference Types

#### Common specification

ECSS-E-ST-40-07\_1630547

For each type, a universally unique identifier (UUID) variable shall be declared as per “Uuid” template in Table 6‑1.

ECSS-E-ST-40-07\_1630548

The value of universally unique identifier (UUID) variables shall be defined as per “Uuid” template in Table 6‑2.

ECSS-E-ST-40-07\_1630549

Constant, Property and Operation elements belonging to the type shall be mapped within the exact same C++ class the type is mapped to.

1. See clause 6.2.4.2 for details on the mapping of Constant elements, clause 6.2.4.6 for details on the mapping of Property elements and clause 6.2.4.7 for details on the mapping of Operation elements.

ECSS-E-ST-40-07\_1630550

The access specifier of class constructors and destructors within the C++ class a type is mapped to shall be defined by the mapping of the type Visibility attribute.

1. See clause 6.2.3 for details on the mapping of Visibility attributes.

#### Interface

ECSS-E-ST-40-07\_1630551

Interface types shall be mapped to ISO/ANSI C++ abstract classes as follows:

Syntax as per “Interface” template in Table 6‑1;

If Base elements are defined, the class inherits from the Base classes;

All class member methods are declared as pure virtual.

ECSS-E-ST-40-07\_1630552

Interface classes shall have a defaulted virtual destructor.

#### Model

ECSS-E-ST-40-07\_1630553

Model types shall be mapped to ISO/ANSI C++ classes as follows:

Syntax as per “Model” template in Table 6‑1;

If Base element is defined, the class inherits from the Base class;

If Interface elements are defined, the class inherits from the Interface classes;

If at least one EntryPoint is defined, the class inherits from the Smp::IEntryPointPublisher class;

If at least one EventSink element is defined, the class inherits from the Smp::IEventConsumer class;

If at least one EventSource element is defined, the class inherits from the Smp::IEventProvider class;

If at least one Container element is defined, the class inherits from the Smp::IComposite class;

If at least one Reference element is defined, the class inherits from the Smp::IAggregate class.

ECSS-E-ST-40-07\_1630554

Model classes shall have a virtual destructor.

ECSS-E-ST-40-07\_1630555

Field and Association elements belonging to the Model type shall be mapped within the exact same C++ class the Model type is mapped to.

1. See clause 6.2.4.3 for details on the mapping of Field elements and clause 6.2.4.4 for details on the mapping of Association elements.

ECSS-E-ST-40-07\_1630556

EntryPoint, EventSink, EventSource, Container and Reference elements belonging to the Model type shall be mapped within the exact same C++ class the Model type is mapped to.

1. See clause 6.2.4.8 for details on the mapping of EntryPoint elements, clause 6.2.4.9 for details on the mapping of EventSink elements, clause 6.2.4.10 for details on the mapping of EventSource elements, clause 6.2.4.11 for details on the mapping of Container elements and clause 6.2.4.12 for details on the mapping of Reference elements.

ECSS-E-ST-40-07\_1630557

The Fallible attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect:

If set to “true”, then the C++ class implements the IFallibleModel interface;

If not set, then it has no effect;

If set to “false”, then it has no effect.

ECSS-E-ST-40-07\_1630558

The BaseClass attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Model C++ mapping:

If set, then the class includes an inheritance link to a base class that the attribute points to;

If not set, then it has no effect.

#### Service

ECSS-E-ST-40-07\_1630559

Service types shall be mapped to ISO/ANSI C++ classes as follows:

Syntax as per “Service” template in Table 6‑1;

If Base element is defined, the class inherits from the Base class;

If Interface elements are defined, the class inherits from the Interface classes;

If at least one EntryPoint is defined, the class inherits from the Smp::IEntryPointPublisher class;

If at least one EventSink element is defined, the class inherits from the Smp::IEventConsumer class;

If at least one EventSource element is defined, the class inherits from the Smp::IEventProvider class;

ECSS-E-ST-40-07\_1630560

Service classes shall have a virtual destructor.

ECSS-E-ST-40-07\_1630561

Field and Association elements belonging to the Service type shall be mapped within the exact same C++ class the Service type is mapped to.

1. See clause 6.2.4.3 for details on the mapping of Field elements and clause 6.2.4.4 for details on the mapping of Association elements.

ECSS-E-ST-40-07\_1630562

EntryPoint, EventSink and EventSource elements belonging to the Service type shall be mapped within the exact same C++ class the Service type is mapped to.

1. See clause 6.2.4.8 for details on the mapping of EntryPoint elements, clause 6.2.4.9 for details on the mapping of EventSink elements and clause 6.2.4.10 for details on the mapping of EventSource elements.

ECSS-E-ST-40-07\_1630563

The BaseClass attribute as per ecss.smp.l1.smpcat in [SMP\_FILES] shall have the following effect for the Model C++ mapping:

If set, then the class includes an inheritance link to a base class that the attribute points to;

If not set, then it has no effect.

## Package to library

### Mapping templates

1. Syntax and expression rules used in the specification of C++ mapping templates:
   1. Information from the package to be mapped in the C++ code is specified by means of placeholders encased within dollar ‘$’ symbols. For example, $Package.Name$ for the value of the field ‘Name’ of some ‘Package’ referred in the context the template is applicable.
2. Table 6‑8 contains the C++ declaration templates for packages and is referred to from requirements of clause 6.3.

ECSS-E-ST-40-07\_1630614

Table 6‑8: C++ declaration templates for packages

| Template | C++ mapping |
| --- | --- |
| Static Initialise | extern “C” bool Initialise\_$Package.Name$(  Smp::ISimulator\* simulator,  Smp::Publication::ITypeRegistry\* typeRegistry); |
| Static Finalise | extern “C” bool Finalise\_$Package.Name$(Smp::ISimulator\* simulator); |
| Static GetSmpVersion | extern “C” Smp::UInt64 GetSmpVersion\_$Package.Name$(); |
| Dynamic Initialise | extern ʺCʺ bool Initialise(  Smp::ISimulator\* simulator,  Smp::Publication::ITypeRegistry\* typeRegistry); |
| Dynamic Finalise | extern ʺCʺ bool Finalise(Smp::ISimulator\* simulator); |
| Dynamic GetSmpVersion | extern “C” Smp::UInt64 GetSmpVersion(); |
| DLL Initialise | extern ʺCʺ DLL\_EXPORT bool Initialise(  Smp::ISimulator\* simulator,  Smp::Publication::ITypeRegistry\* typeRegistry); |
| DLL Finalise | extern ʺCʺ DLL\_EXPORT bool Finalise(Smp::ISimulator\* simulator); |
| DLL GetSmpVersion | extern ʺCʺ DLL\_EXPORT Smp::UInt64 GetSmpVersion(); |
| DLL\_EXPORT | #ifdef WIN32  #define DLL\_EXPORT declspec(dllexport) #else  #define DLL\_EXPORT #endif |

### Common to Unix and Windows

ECSS-E-ST-40-07\_1630564

The SMDL Package Provider shall implement the Package as a Static or Dynamic Library file.

1. The Library file can be materialized differently on different Operating Systems.

ECSS-E-ST-40-07\_1630565

The Library shall contain an Initialise function as per Initialise template in Table 6‑8.

ECSS-E-ST-40-07\_1630566

The Library shall contain a Finalise method as per Finalise template in Table 6‑8.

ECSS-E-ST-40-07\_1630567

The Finalise function shall release memory allocated during Initialise method, unless ownership has been handed over.

ECSS-E-ST-40-07\_1630568

The Initialise function shall register all user-defined Types in the library with the Type Registry using the provided Type Registry interface.

1. This is done by calling the global register function (for Enumeration, Integer, Float, Array, String) or method (Structure, Class, Exception) of the type.

ECSS-E-ST-40-07\_1630569

The Initialise function shall register the class Factory of all implemented models in the library using the ISimulator RegisterFactory method.

1. The ownership of the class factory is handed over to the object implementing ISimulator.

ECSS-E-ST-40-07\_1630570

The Initialise function shall add an instance of all Services in the library using the ISimulator AddService method.

1. The ownership of the service is handed over to the object implementing ISimulator.

ECSS-E-ST-40-07\_1630571

The Initialise function may add instances of Model in the library using the ISimulator AddModel method.

1. The ownership of the model is handed over to the object implementing ISimulator.

ECSS-E-ST-40-07\_1630572

The Initialise function may register instances of Entry Point in the library using the ISimulator AddInitEntryPoint method.

1. The ownership of the entry point remains in the caller of AddInitEntryPoint.

ECSS-E-ST-40-07\_1630573

The Library shall contain a GetSmpVersion method as per GetSmpVersion template in Table 6‑8.

ECSS-E-ST-40-07\_1630574

The GetSmpVersion function shall return ECSS\_SMP\_VERSION as per Version.h in [SMP\_FILES].

### Unix (Shared object)

ECSS-E-ST-40-07\_1630575

The SMDL Package shall be implementation mapped on UNIX based Operation Systems using on the following two methods:

As a Static Library file with extension “.a”;

As a Dynamic Shared Object file with extension “.so”.

ECSS-E-ST-40-07\_1630576

The Static Library shall contain an Initialise method as per the “Static Initialise” template in Table 6‑8.

ECSS-E-ST-40-07\_1630577

The Dynamic Shared Object shall contain an Initialise method as per the “Dynamic Initialise” template in Table 6‑8.

ECSS-E-ST-40-07\_1630578

The Static Library shall contain a Finalise method as per the Static Finalise template in Table 6‑8.

ECSS-E-ST-40-07\_1630579

The Dynamic Shared Object shall contain a Finalise method as per the “Dynamic Finalise” template in Table 6‑8.

ECSS-E-ST-40-07\_1630580

The Initialise function shall call the Initialise$Package.Name$ ( ) function.

ECSS-E-ST-40-07\_1630581

The Finalise function shall call the Finalise$Package.Name$ ( ) function.

ECSS-E-ST-40-07\_1630582

The Initialise$Package.Name$ function shall call the initialization functions of the Packages which are referenced as Dependencies of the Package.

* 1. 1 Dependency indicates that a type referenced from an implementation in the package needs a type implemented in the referenced package.
  2. 2 There are no rules on the order in which packages are initialised, as the type registration process via Universally Unique Identifiers (UUIDs) does not introduce dependencies on the order.

ECSS-E-ST-40-07\_1630583

The Initialise and Finalise functions shall be implemented so that multiple calls are possible.

* 1. 1 The Initialise and Finalise functions may get called several times during initialization when a library is referenced from more than one package.
  2. 2 Ensuring that types are only registered once and memory is only allocated once allows multiple calls to Initialise.

ECSS-E-ST-40-07\_1630584

Packages shall map to either static or dynamic libraries.

* 1. 1 Two dynamic library implementations are currently mapped
     + Unix Shared Object (SO)
     + Windows Dynamic Link Library (DLL)
  2. 2 The requirements for the static library are common to all the dynamic library implementations, therefore they are not repeated in the corresponding clauses. The clauses on the dynamic library implementations cover only the specific delta specifications applicable to the case at hand.

ECSS-E-ST-40-07\_1630585

The Static Library shall contain a GetSmpVersion method as per the “Static GetSmpVersion” template in Table 6‑8.

ECSS-E-ST-40-07\_1630586

The Dynamic Shared Object shall contain a GetSmpVersion method as per the “Dynamic GetSmpVersion” template in Table 6‑8.

ECSS-E-ST-40-07\_1630587

The GetSmpVersion function shall call the GetSmpVersion $Package.Name$() function.

### Addendum for Windows Dynamic Link Library (DLL)

ECSS-E-ST-40-07\_1630588

A package shall be mapped to a single DLL file.

ECSS-E-ST-40-07\_1630589

A single DLL file shall implement a single package.

ECSS-E-ST-40-07\_1630590

All functions exported by a DLL file shall be exported with platform-specific decorations based on the calling convention.

1. This is typically achieved by using the ‘C’ linkage (extern “C”) along with the \_\_declspec(dllexport) storage-class attributes.

ECSS-E-ST-40-07\_1630591

A DLL file shall export the function Initialise() with the following “DLL Initialise” template in Table 6‑8 where DLL\_EXPORT is as per “DLL\_EXPORT” template in Table 6‑8.

ECSS-E-ST-40-07\_1630592

A DLL file shall export the function Finalise() with the following DLL Finalise template in Table 6‑8 where DLL\_EXPORT is as per DLL\_EXPORT template in Table 6‑8.

ECSS-E-ST-40-07\_1630593

A DLL file shall export the function GetSmpVersion() following the DLL GetSmpVersion template in Table 6‑8 where DLL\_EXPORT is as per DLL\_EXPORT template in Table 6‑8.

### SMP Bundle

ECSS-E-ST-40-07\_1630594

A SMP bundle shall be composed by one or more SMDL packages.

ECSS-E-ST-40-07\_1630595

A SMP bundle shall be composed by one or more package dynamic libraries, directly related to the SMDL packages.

ECSS-E-ST-40-07\_1630596

A SMP bundle may be composed by one or more package static libraries, directly related to the SMDL packages.

ECSS-E-ST-40-07\_1630597

A SMP bundle shall be composed by all the SMP catalogues related to the SMDL packages.

ECSS-E-ST-40-07\_1630598

A SMP Bundle shall include a SMP manifest file in conformance with the Manifest file DRD of Annex D.

1. (normative)  
   Catalogue file - DRD
   1. Catalogue DRD
      1. Requirement identification and source document

This DRD is called from ECSS-E-ST-40-07 requirement 5.4.1.1a.

* + 1. Purpose and objective

The purpose of the Catalogue file is to hold the model meta data.

* 1. Expected response 
     1. Scope and content

ECSS-E-ST-40-07\_1630599

The suffix for catalogue files shall be “smpcat”.

ECSS-E-ST-40-07\_1630600

The document shall be compliant with the Catalogue XML XSD in xml/Smdl/Catalogue.xsd in [SMP\_FILES] and the files referred from it:

xml/Core/Types.xsd in [SMP\_FILES]

xml/Core/Elements.xsd in [SMP\_FILES]

* + 1. Special remarks

None.

1. (normative)  
   Package file - DRD
   1. Package DRD
      1. Requirement identification and source document

This DRD is called from ECSS-E-ST-40-07 requirement 5.4.2.1a.

* + 1. Purpose and objective

The purpose of the Package file is to contain all metamodel elements that are needed in order to define how implementations of types defined in catalogues are packaged.

* 1. Expected response
     1. Scope and content

ECSS-E-ST-40-07\_1630601

The suffix for package files shall be “smppkg”.

ECSS-E-ST-40-07\_1630602

The document shall be compliant with the Package XML XSD in xml/Smdl/Package.xsd in [SMP\_FILES] and the files referred from it:

xml/Smdl/Types.xsd in [SMP\_FILES]

xml/Smdl/Elements.xsd in [SMP\_FILES]

* + 1. Special remarks

None.

1. (normative)  
   Configuration file - DRD
   1. Configuration DRD
      1. Requirement identification and source document

This DRD is called from ECSS-E-ST-40-07 requirement 5.4.3.1a

* + 1. Purpose and objective

The purpose of the Configuration file is to hold configuration data for a simulation.

* 1. Expected response 
     1. Scope and content

ECSS-E-ST-40-07\_1630603

The suffix for configuration files shall be “smpcfg”.

ECSS-E-ST-40-07\_1630604

The document shall be compliant with the Configuration XML XSD in xml/Smdl/Configuration.xsd in [SMP\_FILES] and the files referred from it:

xml/Smdl/Types.xsd in [SMP\_FILES]

xml/Smdl/Elements.xsd in [SMP\_FILES]

* + 1. Special remarks

None.

1. (normative)  
   Manifest file - DRD
   1. Manifest DRD
      1. Requirement identification and source document

This DRD is called from ECSS-E-ST-40-07 requirement 6.3.5e.

* + 1. Purpose and objective

The purpose of the Manifest file is to hold meta data for a bundle.

* 1. Expected response 
     1. Scope and content

ECSS-E-ST-40-07\_1630605

The SMP Manifest files name shall be “SMP.MF”.

ECSS-E-ST-40-07\_1630606

The SMP Manifest file shall be an ASCII file which contains key-value pairs in the following format: “Key: Value”

ECSS-E-ST-40-07\_1630607

In the SMP Manifest file the Key and Value shall be separated by a colon.

ECSS-E-ST-40-07\_1630608

In the SMP Manifest file the, the Key shall only contain alpha-numerical characters, underscore (“\_”) or dash (“-“).

ECSS-E-ST-40-07\_1630609

In the SMP Manifest file the, the Value shall start at the first non-whitespace character after the colon (“:”), and is terminated by the end of line.

ECSS-E-ST-40-07\_1630610

The SMP Manifest file shall contain the Mandatory Keys listed in Table D-1 as indicated in the Mandatory column.

ECSS-E-ST-40-07\_1630611

The SMP Manifest file shall conform to the OSGi Core Release 6 Bundle Manifest file format.

1. Internet link to the OSGI Core manifest: https://osgi.org/download/r6/osgi.core-6.0.0.pdf

ECSS-E-ST-40-07\_1630612

: SMP Manifest Key

| Key | Meaning | Mandatory |
| --- | --- | --- |
| Bundle-Copyright | Copyright statement for the bundle. | Yes |
| Bundle-ContactAddress | Full address of a person or company that can be contacted. | No |
| Bundle-DocURL | URL where documentation for the bundle can be retrieved from. | No |
| Bundle-Description | Textual description of the bundle and its content. | Yes |
| Bundle-ManifestVersion | A bundle manifest may express the version of the OSGi manifest header syntax in the Bundle-ManifestVersion header. If specified, the bundle manifest version must be ’2’. | Yes |
| Bundle-Name | The Bundle-Name header defines a readable name for this bundle. This should be a short, human-readable name that can contain spaces. | Yes |
| Bundle-SymbolicName | The Bundle-SymbolicName manifest header is a mandatory header. The bundle symbolic name and bundle version allow a bundle to be uniquely identified in the Framework. That is, a bundle with a given symbolic name and version is treated as equal to another bundle with the same (case sensitive) symbolic name and exact version.  The installation of a bundle with a Bundle-SymbolicName and Bundle-Version identical to an existing bundle fail. | Yes |
| Bundle-Vendor | The Bundle-Vendor header contains a human-readable description of the bundle vendor. | Yes |
| Bundle-Version | Bundle-Version is an optional header; the default value is 0.0.0.  A version consists of major, minor and micro version components. If the minor or micro version components are not specified, they have a default value of 0.  Versions are comparable. Their comparison is done numerically and sequentially on the major, minor, and micro components. A version is considered equal to another version if the major, minor, and micro components are equal. | Yes |
| Require-Bundle | The Require-Bundle header specifies the required exports from another bundle. This is a comma-separated list of required bundles, where each bundle is at least specified by its symbolic name, optionally followed by a specific version:  <Bundle-SymbolicName>[; Bundle-Version="<Bundle-Version>"] | No |
| Compiler-Name | Name of the compiler that has been used to compile the source code. | No |
| Compiler-Version | Version of the compiler that has been used to compile the source code. | No |
| OS-Name | Name of the Operating System. | No |
| OS-Version | Version of the Operating System. | No |

* + 1. Special remarks

None.

Bibliography

|  |  |
| --- | --- |
| ECSS-S-ST-00 | ECSS system – Description, implementation and general requirements |
| ISO 9000 series | Quality management systems standards International Organization for Standardization (ISO) http://www.iso.org |
| ISO/IEC 9899:2011 | ISO/IEC 9899:2011 Information technology -- Programming languages -- C |
| ISO/IEC 14882:2011 | ISO/IEC 14882:2011 Information technology -- Programming languages -- C++ |
| Open Group UUID | Open Group <http://www.opengroup.org> |
| OSGi Manifest | Open Services Gateway initiative http://www.osgi.org |
| SMP v1.2 | Simulation Model Portability Specification version 1.2 |
| XML | Extensible Markup Language World Wide Web Consortium (W3C) http://www.w3.org/XM |